Connected: An Internet Encyclopedia
RFC 1510 - 8.2.1. IP transport

Top: Connected: An Internet Encyclopedia
Up: Requests For Comments
Up: RFC 1510
Up: 8. Constants and other defined values
Up: 8.2. KDC messages
Prev: 8.2. KDC messages
Next: 8.2.2. OSI transport

### 8.2.1. IP transport

When contacting a Kerberos server (KDC) for a KRB_KDC_REQ request using IP transport, the client shall send a UDP datagram containing only an encoding of the request to port 88 (decimal) at the KDC's IP address; the KDC will respond with a reply datagram containing only an encoding of the reply message (either a KRB_ERROR or a KRB_KDC_REP) to the sending port at the sender's IP address.

Next: 8.2.2. OSI transport

Connected: An Internet Encyclopedia
RFC 1510 - 8.2.1. IP transport