Connected: An Internet Encyclopedia
RFC 1661 - 6.6. Address-and-Control-Field-Compression (ACFC)

Top: Connected: An Internet Encyclopedia
Up: Requests For Comments
Up: RFC 1661
Up: 6. LCP Configuration Options
Prev: 6.5. Protocol-Field-Compression (PFC)
Next: Security Considerations

### 6.6. Address-and-Control-Field-Compression (ACFC)

Description

  This Configuration Option provides a method to negotiate the compression of the Data Link Layer Address and Control fields. By default, all implementations MUST transmit frames with Address and Control fields appropriate to the link framing.

  Since these fields usually have constant values for point-to-point links, they are easily compressed. This Configuration Option is sent to inform the peer that the implementation can receive compressed Address and Control fields.

  If a compressed frame is received when Address-and-Control-Field- Compression has not been negotiated, the implementation MAY silently discard the frame.

  The Address and Control fields MUST NOT be compressed when sending any LCP packet. This rule guarantees unambiguous recognition of LCP packets.

  When the Address and Control fields are compressed, the Data Link Layer FCS field is calculated on the compressed frame, not the original uncompressed frame.

A summary of the Address-and-Control-Field-Compression configuration option format is shown below. The fields are transmitted from left to right.

        0                   1
        0 1 2 3 4 5 6 7 8 9 0 1 2 3 4 5
       +-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+
       |     Type      |    Length     |
       +-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+

Type

  8

Length

  2

Next: Security Considerations

Connected: An Internet Encyclopedia
RFC 1661 - 6.6. Address-and-Control-Field-Compression (ACFC)