Connected: An Internet Encyclopedia
RFC 1812 - 7.5.3 Advanced Route Filtering

Top: Connected: An Internet Encyclopedia
Up: Requests For Comments
Up: RFC 1812
Up: 7. APPLICATION LAYER - ROUTING PROTOCOLS
Up: 7.5 FILTERING OF ROUTING INFORMATION
Prev: 7.5.2 Basic Route Filtering
Next: 7.6 INTER-ROUTING-PROTOCOL INFORMATION EXCHANGE

### 7.5.3 Advanced Route Filtering

As the topology of a network grows more complex, the need for more complex route filtering arises. Therefore, a router SHOULD provide the ability to specify independently for each routing protocol:

- Which logical interfaces or routers routing information (routes) will be accepted from and which routes will be believed from each other router or logical interface,

- Which routes will be sent via which logical interface(s), and

- Which routers routing information will be sent to, if this is supported by the routing protocol in use.

In many situations it is desirable to assign a reliability ordering to routing information received from another router instead of the simple believe or don't believe choice listed in the first bullet above. A router MAY provide the ability to specify:

- A reliability or preference to be assigned to each route received. A route with higher reliability will be chosen over one with lower reliability regardless of the routing metric associated with each route.

If a router supports assignment of preferences, the router MUST NOT propagate any routes it does not prefer as first party information. If the routing protocol being used to propagate the routes does not support distinguishing between first and third party information, the router MUST NOT propagate any routes it does not prefer.

DISCUSSION

  For example, assume a router receives a route to network C from router R and a route to the same network from router S. If router R is considered more reliable than router S traffic destined for network C will be forwarded to router R regardless of the route received from router S.

Routing information for routes which the router does not use (router S in the above example) MUST NOT be passed to any other router.

Next: 7.6 INTER-ROUTING-PROTOCOL INFORMATION EXCHANGE

Connected: An Internet Encyclopedia
RFC 1812 - 7.5.3 Advanced Route Filtering