Connected: An Internet Encyclopedia
RFC 1510 - 3.3.2. Receipt of KRB_TGS_REQ message

Top: Connected: An Internet Encyclopedia
Up: Requests For Comments
Up: RFC 1510
Up: 3. Message Exchanges
Up: 3.3. The Ticket-Granting Service (TGS) Exchange
Prev: 3.3.1. Generation of KRB_TGS_REQ message
Next: 3.3.3. Generation of KRB_TGS_REP message

### 3.3.2. Receipt of KRB_TGS_REQ message

The KRB_TGS_REQ message is processed in a manner similar to the KRB_AS_REQ message, but there are many additional checks to be performed. First, the Kerberos server must determine which server the accompanying ticket is for and it must select the appropriate key to decrypt it. For a normal KRB_TGS_REQ message, it will be for the ticket granting service, and the TGS's key will be used. If the TGT was issued by another realm, then the appropriate inter-realm key must be used. If the accompanying ticket is not a ticket granting ticket for the current realm, but is for an application server in the current realm, the RENEW, VALIDATE, or PROXY options are specified in the request, and the server for which a ticket is requested is the server named in the accompanying ticket, then the KDC will decrypt the ticket in the authentication header using the key of the server for which it was issued. If no ticket can be found in the padata field, the KDC_ERR_PADATA_TYPE_NOSUPP error is returned.

Once the accompanying ticket has been decrypted, the user-supplied checksum in the Authenticator must be verified against the contents of the request, and the message rejected if the checksums do not match (with an error code of KRB_AP_ERR_MODIFIED) or if the checksum is not keyed or not collision-proof (with an error code of KRB_AP_ERR_INAPP_CKSUM). If the checksum type is not supported, the KDC_ERR_SUMTYPE_NOSUPP error is returned. If the authorization-data are present, they are decrypted using the sub-session key from the Authenticator.

If any of the decryptions indicate failed integrity checks, the KRB_AP_ERR_BAD_INTEGRITY error is returned.

Next: 3.3.3. Generation of KRB_TGS_REP message

Connected: An Internet Encyclopedia
RFC 1510 - 3.3.2. Receipt of KRB_TGS_REQ message