Connected: An Internet Encyclopedia
RFC 1945 - 6.1.1 Status Code and Reason Phrase

Top: Connected: An Internet Encyclopedia
Up: Requests For Comments
Up: RFC 1945
Up: 6. Response
Up: 6.1 Status-Line
Prev: 6.1 Status-Line
Next: 6.2 Response Header Fields

### 6.1.1 Status Code and Reason Phrase

The Status-Code element is a 3-digit integer result code of the attempt to understand and satisfy the request. The Reason-Phrase is intended to give a short textual description of the Status-Code. The Status-Code is intended for use by automata and the Reason-Phrase is intended for the human user. The client is not required to examine or display the Reason-Phrase.

The first digit of the Status-Code defines the class of response. The last two digits do not have any categorization role. There are 5 values for the first digit:

- 1xx: Informational - Not used, but reserved for future use

- 2xx: Success - The action was successfully received, understood, and accepted.

- 3xx: Redirection - Further action must be taken in order to complete the request

- 4xx: Client Error - The request contains bad syntax or cannot be fulfilled

- 5xx: Server Error - The server failed to fulfill an apparently valid request

The individual values of the numeric status codes defined for HTTP/1.0, and an example set of corresponding Reason-Phrase's, are presented below. The reason phrases listed here are only recommended -- they may be replaced by local equivalents without affecting the protocol. These codes are fully defined in Section 9.

           Status-Code    = "200"   ; OK
                          | "201"   ; Created
                          | "202"   ; Accepted
                          | "204"   ; No Content
                          | "301"   ; Moved Permanently
                          | "302"   ; Moved Temporarily
                          | "304"   ; Not Modified
                          | "400"   ; Bad Request
                          | "401"   ; Unauthorized
                          | "403"   ; Forbidden
                          | "404"   ; Not Found
                          | "500"   ; Internal Server Error
                          | "501"   ; Not Implemented
                          | "502"   ; Bad Gateway
                          | "503"   ; Service Unavailable
                          | extension-code

           extension-code = 3DIGIT

           Reason-Phrase  = *<TEXT, excluding CR, LF>

HTTP status codes are extensible, but the above codes are the only ones generally recognized in current practice. HTTP applications are not required to understand the meaning of all registered status codes, though such understanding is obviously desirable. However, applications must understand the class of any status code, as indicated by the first digit, and treat any unrecognized response as being equivalent to the x00 status code of that class, with the exception that an unrecognized response must not be cached. For example, if an unrecognized status code of 431 is received by the client, it can safely assume that there was something wrong with its request and treat the response as if it had received a 400 status code. In such cases, user agents should present to the user the entity returned with the response, since that entity is likely to include human-readable information which will explain the unusual status.

Next: 6.2 Response Header Fields

Connected: An Internet Encyclopedia
RFC 1945 - 6.1.1 Status Code and Reason Phrase