Connected: An Internet Encyclopedia
RFC 1583 - 10.4. Whether to become adjacent

Top: Connected: An Internet Encyclopedia
Up: Requests For Comments
Up: RFC 1583
Up: 10. The Neighbor Data Structure
Prev: 10.3. The Neighbor state machine
Next: 10.5. Receiving Hello Packets

### 10.4. Whether to become adjacent

Adjacencies are established with some subset of the router's neighbors. Routers connected by point-to-point networks and virtual links always become adjacent. On multi-access networks, all routers become adjacent to both the Designated Router and the Backup Designated Router.

The adjacency-forming decision occurs in two places in the neighbor state machine. First, when bidirectional communication is initially established with the neighbor, and secondly, when the identity of the attached network's (Backup) Designated Router changes. If the decision is made to not attempt an adjacency, the state of the neighbor communication stops at 2- Way.

An adjacency should be established with a bidirectional neighbor when at least one of the following conditions holds:

- The underlying network type is point-to-point

- The underlying network type is virtual link

- The router itself is the Designated Router

- The router itself is the Backup Designated Router

- The neighboring router is the Designated Router

- The neighboring router is the Backup Designated Router

Next: 10.5. Receiving Hello Packets

Connected: An Internet Encyclopedia
RFC 1583 - 10.4. Whether to become adjacent