Connected: An Internet Encyclopedia
RFC 922 - 2. Terminology

Top: Connected: An Internet Encyclopedia
Up: Requests For Comments
Up: RFC 922
Prev: 1. Introduction
Next: 3. Why Broadcast?

### 2. Terminology

Because broadcasting depends on the specific data link layer in use on a local network, we must discuss it with reference to both physical networks and logical networks.

The terms we will use in referring to physical networks are, from the point of view of the host sending or forwarding a broadcast:

       Local Hardware Network

          The physical link to which the host is attached.

       Remote Hardware Network

          A physical network which is separated from the host by at least
          one gateway.

       Collection of Hardware Networks

          A set of hardware networks (transitively) connected by gateways.

The IP world includes several kinds of logical network. To avoid ambiguity, we will use the following terms:

       Internet

          The DARPA Internet collection of IP networks.

       IP Network

          One or a collection of several hardware networks that have one
          specific IP network number.

       Subnet

          A single member of the collection of hardware networks that
          compose an IP network.  Host addresses on a given subnet share an
          IP network number with hosts on all other subnets of that IP
          network, but the local-address part is divided into subnet-number

          and host-number fields to indicate which subnet a host is on.  We
          do not assume a particular division of the local-address part;
          this could vary from network to network.

The introduction of a subnet level in the addressing hierarchy is at variance with the IP specification [12], but as the use of addressable subnets proliferates it is obvious that a broadcasting scheme should support subnetting. For more on subnets, see [8].

In this paper, the term "host address" refers to the host-on-subnet address field of a subnetted IP network, or the host-part field otherwise.

An IP network may consist of a single hardware network or a collection of subnets; from the point of view of a host on another IP network, it should not matter.

Next: 3. Why Broadcast?

Connected: An Internet Encyclopedia
RFC 922 - 2. Terminology