Connected: An Internet Encyclopedia
RFC 1123 - 6.2.2.2 Loading Phase

Top: Connected: An Internet Encyclopedia
Up: Requests For Comments
Up: RFC 1123
Up: 6. SUPPORT SERVICES
Up: 6.2 HOST INITIALIZATION
Up: 6.2.2 REQUIREMENTS
Prev: 6.2.2.1 Dynamic Configuration
Next: 6.3 REMOTE MANAGEMENT

### 6.2.2.2 Loading Phase

A suggested approach for the loading phase is to use TFTP [BOOT:1] between the IP addresses established by BOOTP.

TFTP to a broadcast address SHOULD NOT be used, for reasons explained in Section 4.2.3.4.

Next: 6.3 REMOTE MANAGEMENT

Connected: An Internet Encyclopedia
RFC 1123 - 6.2.2.2 Loading Phase