Connected: An Internet Encyclopedia
RFC 1812 - 9.1.1 Introduction

Top: Connected: An Internet Encyclopedia
Up: Requests For Comments
Up: RFC 1812
Up: 9. APPLICATION LAYER - MISCELLANEOUS PROTOCOLS
Up: 9.1 BOOTP
Prev: 9.1 BOOTP
Next: 9.1.2 BOOTP Relay Agents

### 9.1.1 Introduction

The Bootstrap Protocol (BOOTP) is a UDP/IP-based protocol that allows a booting host to configure itself dynamically and without user supervision. BOOTP provides a means to notify a host of its assigned IP address, the IP address of a boot server host, and the name of a file to be loaded into memory and executed ([APPL:1]). Other configuration information such as the local prefix length or subnet mask, the local time offset, the addresses of default routers, and the addresses of various Internet servers can also be communicated to a host using BOOTP ([APPL:2]).

Next: 9.1.2 BOOTP Relay Agents

Connected: An Internet Encyclopedia
RFC 1812 - 9.1.1 Introduction