Connected: An Internet Encyclopedia
RFC 1157 - 3.2.6.3.3. ipAddrTable Object Type Names

Top: Connected: An Internet Encyclopedia
Up: Requests For Comments
Up: RFC 1157
Up: 3. The SNMP Architecture
Up: 3.2. Elements of the Architecture
Up: 3.2.6. Form and Meaning of References to Managed Objects
Up: 3.2.6.3. Identification of Object Instances
Prev: 3.2.6.3.2. atTable Object Type Names
Next: 3.2.6.3.4. ipRoutingTable Object Type Names

### 3.2.6.3.3. ipAddrTable Object Type Names

The name of an IP-addressable network element, x, is the OBJECT IDENTIFIER of the form a.b.c.d such that a.b.c.d is the value (in the familiar "dot" notation) of that instance of the ipAdEntAddr object type associated with x.

For each object type, t, for which the defined name, n, has a prefix of ipAddrEntry, an instance, i, of t is named by an OBJECT IDENTIFIER of the form n.y, where y is the name of the IP-addressable network element about which i represents information.

For example, suppose one wanted to find the network mask of an entry in the IP interface table associated with an IP address of 89.1.1.42. Accordingly, ipAdEntNetMask.89.1.1.42 would identify the desired instance.

Next: 3.2.6.3.4. ipRoutingTable Object Type Names

Connected: An Internet Encyclopedia
RFC 1157 - 3.2.6.3.3. ipAddrTable Object Type Names