Connected: An Internet Encyclopedia
RFC 1772 - 9.4 Combined Properties

Top: Connected: An Internet Encyclopedia
Up: Requests For Comments
Up: RFC 1772
Up: 9. Operations over Switched Virtual Circuits
Prev: 9.3 TCP Properties
Next: 10. Conclusion

### 9.4 Combined Properties

Some implementations may not be able to guarantee that the BGP process and the circuit manager will operate as a single entity; i.e. they can have a separate existence when the other has been stopped or has crashed.

If this is the case, a periodic two-way poll between the BGP process and the circuit manager should be implemented. If the BGP process discovers the circuit manager has gone away it should close all relevant TCP connections. If the circuit manager discovers the BGP process has gone away it should close all its connections associated with the BGP process and reject any further incoming connections.

Next: 10. Conclusion

Connected: An Internet Encyclopedia
RFC 1772 - 9.4 Combined Properties