Connected: An Internet Encyclopedia
RFC 1771 - 9.2.3.2 Frequency of Route Origination

Top: Connected: An Internet Encyclopedia
Up: Requests For Comments
Up: RFC 1771
Up: 9. UPDATE Message Handling
Up: 9.2 Update-Send Process
Up: 9.2.3 Controlling Routing Traffic Overhead
Prev: 9.2.3.1 Frequency of Route Advertisement
Next: 9.2.3.3 Jitter

### 9.2.3.2 Frequency of Route Origination

The parameter MinASOriginationInterval determines the minimum amount of time that must elapse between successive advertisements of UPDATE messages that report changes within the advertising BGP speaker's own autonomous systems.

Next: 9.2.3.3 Jitter

Connected: An Internet Encyclopedia
RFC 1771 - 9.2.3.2 Frequency of Route Origination