Connected: An Internet Encyclopedia
RFC 1157 - 4.1.6.5. The authenticationFailure Trap

Top: Connected: An Internet Encyclopedia
Up: Requests For Comments
Up: RFC 1157
Up: 4. Protocol Specification
Up: 4.1. Elements of Procedure
Up: 4.1.6. The Trap-PDU
Prev: 4.1.6.4. The linkUp Trap
Next: 4.1.6.6. The egpNeighborLoss Trap

### 4.1.6.5. The authenticationFailure Trap

An authenticationFailure(4) trap signifies that the sending protocol entity is the addressee of a protocol message that is not properly authenticated. While implementations of the SNMP must be capable of generating this trap, they must also be capable of suppressing the emission of such traps via an implementation-specific mechanism.

Next: 4.1.6.6. The egpNeighborLoss Trap

Connected: An Internet Encyclopedia
RFC 1157 - 4.1.6.5. The authenticationFailure Trap