Connected: An Internet Encyclopedia
RFC 1421 - 4.6.3 Encapsulated Header Fields with Variable Occurrences

Top: Connected: An Internet Encyclopedia
Up: Requests For Comments
Up: RFC 1421
Up: 4. Processing of Messages
Up: 4.6 Summary of Encapsulated Header Fields
Prev: 4.6.2.3 MIC-Info Field
Next: 4.6.3.1 Issuer-Certificate Field

### 4.6.3 Encapsulated Header Fields with Variable Occurrences

This group of encapsulated header fields contains fields which will normally occur variable numbers of times within a message, with numbers of occurrences ranging from zero to non-zero values which are independent of the number of recipients.

4.6.3.1 Issuer-Certificate Field

Next: 4.6.3.1 Issuer-Certificate Field

Connected: An Internet Encyclopedia
RFC 1421 - 4.6.3 Encapsulated Header Fields with Variable Occurrences