Connected: An Internet Encyclopedia
RFC 1451 - 3.3.2. Units of Conformance

Top: Connected: An Internet Encyclopedia
Up: Requests For Comments
Up: RFC 1451
Up: 3. Definitions
Up: 3.3. Conformance Information
Prev: 3.3.1. Compliance Statements
Next: 4. Acknowledgements

### 3.3.2. Units of Conformance

       -- units of conformance

       snmpAlarmGroup OBJECT-GROUP
           OBJECTS { snmpAlarmNextIndex,
                     snmpAlarmVariable, snmpAlarmInterval,
                     snmpAlarmSampleType, snmpAlarmValue,
                     snmpAlarmStartupAlarm, snmpAlarmRisingThreshold,
                     snmpAlarmFallingThreshold,
                     snmpAlarmRisingEventIndex,
                     snmpAlarmFallingEventIndex,
                     snmpAlarmUnavailableEventIndex,
                     snmpAlarmStatus }
           STATUS  current
           DESCRIPTION
                   "A collection of objects allowing the description
                   and configuration of threshold alarms from a
                   SNMPv2 entity acting in a dual role."
           ::= { snmpM2MGroups 1 }

       snmpEventGroup OBJECT-GROUP
           OBJECTS { snmpEventNextIndex,
                     snmpEventID, snmpEventDescription,
                     snmpEventEvents, snmpEventLastTimeSent,
                     snmpEventStatus, snmpEventNotifyMinInterval,
                     snmpEventNotifyMaxRetransmissions,
                     snmpEventNotifyIntervalRequested,
                     snmpEventNotifyRetransmissionsRequested,
                     snmpEventNotifyLifetime, snmpEventNotifyStatus }
           STATUS  current
           DESCRIPTION
                   "A collection of objects allowing the description
                   and configuration of events from a SNMPv2 entity
                   acting in a dual role."
           ::= { snmpM2MGroups 2 }

       END

Next: 4. Acknowledgements

Connected: An Internet Encyclopedia
RFC 1451 - 3.3.2. Units of Conformance