Connected: An Internet Encyclopedia
RFC 1813 - 6.1.3 Transport Address

Top: Connected: An Internet Encyclopedia
Up: Requests For Comments
Up: RFC 1813
Up: 6. Appendix II: Lock manager protocol
Up: 6.1 RPC Information
Prev: 6.1.2 Constants
Next: 6.1.4 Basic Data Types

### 6.1.3 Transport Address

The NLM service is normally supported over the TCP and UDP protocols. The rpcbind daemon should be queried for the correct transport address.

Next: 6.1.4 Basic Data Types

Connected: An Internet Encyclopedia
RFC 1813 - 6.1.3 Transport Address