Connected: An Internet Encyclopedia
RFC 1904 - 3.6. Usage Example

Top: Connected: An Internet Encyclopedia
Up: Requests For Comments
Up: RFC 1904
Up: 3. Mapping of the OBJECT-GROUP macro
Prev: 3.5. Mapping of the OBJECT-GROUP value
Next: 4. Mapping of the NOTIFICATION-GROUP macro

### 3.6. Usage Example

The SNMP Group [3] is described:

    snmpGroup OBJECT-GROUP
        OBJECTS { snmpInPkts,
                  snmpInBadVersions,
                  snmpInASNParseErrs,
                  snmpBadOperations,
                  snmpSilentDrops,
                  snmpProxyDrops,
                  snmpEnableAuthenTraps }
        STATUS  current
        DESCRIPTION
                "A collection of objects providing basic instrumentation and
                control of an SNMPv2 entity."
        ::= { snmpMIBGroups 8 }

According to this invocation, the conformance group named

         { snmpMIBGroups 8 }

contains 7 objects.

Next: 4. Mapping of the NOTIFICATION-GROUP macro

Connected: An Internet Encyclopedia
RFC 1904 - 3.6. Usage Example