Connected: An Internet Encyclopedia
RFC 1812 - 4.2.2.3 Unused IP Header Bits: RFC 791 Section 3.1

Top: Connected: An Internet Encyclopedia
Up: Requests For Comments
Up: RFC 1812
Up: 4. INTERNET LAYER - PROTOCOLS
Up: 4.2 INTERNET PROTOCOL - IP
Up: 4.2.2 PROTOCOL WALK-THROUGH
Prev: 4.2.2.2 Addresses in Options: RFC 791 Section 3.1
Next: 4.2.2.4 Type of Service: RFC 791 Section 3.1

### 4.2.2.3 Unused IP Header Bits: RFC 791 Section 3.1

The IP header contains two reserved bits: one in the Type of Service byte and the other in the Flags field. A router MUST NOT set either of these bits to one in datagrams originated by the router. A router MUST NOT drop (refuse to receive or forward) a packet merely because one or more of these reserved bits has a non-zero value; i.e., the router MUST NOT check the values of thes bits.

DISCUSSION

  Future revisions to the IP protocol may make use of these unused bits. These rules are intended to ensure that these revisions can be deployed without having to simultaneously upgrade all routers in the Internet.

Next: 4.2.2.4 Type of Service: RFC 791 Section 3.1

Connected: An Internet Encyclopedia
RFC 1812 - 4.2.2.3 Unused IP Header Bits: RFC 791 Section 3.1