  Special OS/2 Commandline options
------------------------------------

-stretch <number>  Stretch PM Window by a factor of <number>
-border <number>   Display border (2=big, 1=small, 
                   else=no border<default>)
-joydev1 <number>  Set CBM-Joystick #1 to 0=none, 1=Joystick 1, 
                   2=Joystick 2
-joydev2 <number>  Set CBM-Joystick #2 to 0=none, 1=Joystick 1, 
                   2=Joystick 2
-joy1cal           Start Auto Calibration for Joystick#1 at 
                   startup
-joy2cal           Start Auto Calibration for Joystick#1 at 
                   startup
-mouse             Support mouse
+mouse             Don't support mouse
-hidemouseptr      Hide OS/2 mouse pointer in Vice-Window
+hidemouseptr      Don't hide mouse pointer
-menu              Show menu bar <DEFAULT>
+menu              Hide menu bar


  Keys
--------

Scrllck:    Warp mode on/off
Esc:        Run/Stop
Pg up, F12: Restore
Alt-0:      Attach tape image to Datasette
Alt-8:      Attach disk image to Drive 8
Alt-9:      Attach disk image to Drive 9
Alt-A:      Open about-dialog
Alt-C:      Open datasette-control-dialog
Alt-D:      Open drive-dialog
Alt-E:      Open emulator-dialog
Alt-F:      Flip Drive #8 to next image of fliplist
Alt-H:      Open hardware-dialog
Alt-J:      Open joystick-dialog
Alt-M:      Open monitor
Alt-N:      Save Snapshot (setup name in the emulator dialog)
Alt-Q:      Do hard-reset (switch machine off and on)
Alt-R:      Do soft-reset (press reset)
Alt-S:      Open sound-dialog
Alt-T:      Switch true drive emulation on/off
Alt-V, F11: Switch VDC-Key on/off (x128 only)
Alt-W:      Write actual configuration to file
Alt-PrtScr: Write screenshot to file (setup file-type and 
            -name in the emulator dialog)
            

  Additional info
-------------------

 - The video cache for CRTC doesn't work yet.


  Reported bugs/problems
--------------------------
 
 - some people reported problems with caps-lock after exiting 
   vice
 - somebody had problems with cs4235 based soundcard 
   (using sound-dialog hangs OS/2)
 - somebody had problems with the attach-dialog and a 
   Matrox g400
 - x128 hangs when closing on some systems. This seems to be a
   problem of the graphic card driver. The use of SciTech
   Display Doctor instead of the drivers solves the problem. It 
   is available from the IBM Device Driver Pack


  To Do
---------

