Recognita Plus 2.0 for OS/2 2.X README file (1994 feb. 8.)
   
INSTALLATION

start A:\RECSETUP.EXE (or B:\RECSETUP.EXE) and select install! command
to install the program

SCANNER INSTALLATION!

HP ScanJet & ScanJet Plus
	DEVICE=c:\recogn\scanjet.sys

HP ScanJet II/c & II/p with the old HP's SCSI Card
	DEVICE=c:\recogn\sjiios2.sys

HP ScanJet II/c,II/p,II/cx with any ASPI SCSI Card which is supperted by OS/2
	DEVICE=c:\recogn\sjiix2.sys

Umax UG630, UC630, UC300, UG80	(ISA now only)
	DEVICE=c:\recogn\umaxdrv.sys /XXX /T:TTT
		   XXX = 300 or 330 (port addr.)
		   TTT = UG80 or UC630 or UG630 or UC300 or UG80 (scanner typ.)


Epson GT-4000, GT-6000, GT-6500, GT-8000 (ISA now only)
	DEVICE=c:\recogn\epsondrv.sys /XXX /T:TTT
		   XXX = 278 or 3f8 (port addr.)
		   TTT = GT-4000 or GT-6000 or GT-6500 or GT-8000 (scanner typ.)


Pentax SB-L301, SB-A4301 (ISA now only)
	DEVICE=c:\recogn\pentxdrv.sys /XXX /T:TTT
		   XXX = 300 (port addr.)
		   TTT = SB-L301 or SB-A4301 (scanner typ.)

AVision AV100
	DEVICE=c:\recogn\av2.sys /N
		N = 1-16 (port addr.) See the scanner documentation
