OS/2 DEVICE DRIVER FOR WD90C24/31 GRAPHICS CONTROLLER
(Build D.036)

This package contains the following:

o   An OS/2* graphics controller driver supporting
    the 90C24/31 chip set from the Western Digital**
    Corporation.
o   This README file, which is formatted for viewing
    on your screen.  You can:
    -   Use the Table of Contents to
        help you locate specific topics.
    -   Use the Find option in the Edit menu of the
        OS/2 System Editor to help you locate
        specific information.
    -   Print the file.


IMPORTANT

PLEASE READ THE FOLLOWING TERMS AND CONDITIONS.  YOUR
USE OF THE OS/2 DEVICE DRIVER FOR WD90C24/31 GRAPHICS
CONTROLLER INDICATES YOUR ACCEPTANCE OF THE FOLLOWING
TERMS AND CONDITIONS:

o   YOU MUST BE A LICENSEE OF OS/2.
o   YOU MAY MAKE COPIES OF THE OS/2 DEVICE DRIVER FOR
    WD90C24/31 GRAPHICS CONTROLLER EQUAL TO THE
    NUMBER OF LICENSED COPIES OF OS/2 YOU POSSESS.
o   ALL OTHER TERMS AND CONDITIONS OF YOUR OS/2
    LICENSE AGREEMENT APPLY TO THIS OS/2 DEVICE
    DRIVER FOR WD90C24/31 GRAPHICS CONTROLLER;
    HOWEVER, THIS DOES NOT EXTEND ANY WARRANTY
    OUTLINED IN SUCH AGREEMENT.


CONTENTS
________

         1.0  Supported Features
           1.1  Supported Resolutions
           1.2  Supported Adapters
         2.0  Compatibility
         3.0  Preliminary Steps
         4.0  Installation from Diskette
         5.0  Installation in a CID Environment
         6.0  Functional Restrictions
           6.1  Functional Restrictions for Laptop Computers
         7.0  Setting Your Display to VGA Mode
         8.0  APAR Fixes Included in This Driver
         9.0  Trademarks


1.0  SUPPORTED FEATURES
_______________________

The WD90C24/31 device driver provides seamless
support for accelerated display graphics and advanced
color resolutions when used with the minimum required
video memory.  It conforms to the OS/2 32-bit flat
memory model and is designed to function as a 32-bit
Presentation Manager* graphics display driver under
the OS/2 32-bit graphics engine.  This driver has
been enabled for use with the IBM* Distributed Console
Access Facility* (DCAF) product.


1.1  SUPPORTED RESOLUTIONS

This video device driver supports these resolutions
and color depths:

                   Number of    Video Memory
   Resolutions      Colors        Required

    640x480          256           1MB
    800x600          256           1MB
   1024x768          256           1MB*

    640x480        65,536          1MB**
    800x600        65,536          1MB***

    * Only on laptops with external monitor connected.
   ** Only on laptops that support 64K colors.
  *** Only some video adapters with the WD90C31 chip support
      this resolution.


1.2  SUPPORTED ADAPTERS

IBM has tested display adapters and systems containing the
WD90C24/31 chip set with the specified amount of memory.
IBM is continuing to test; therefore, support for additional
cards might be added over time.

For a comprehensive listing of all major manufacturing products
that have been tested by IBM and are OS/2 compatible, refer to the
"OS/2 Hardware Compatibility List" book.  This book is available
electronically on the following Bulletin Board Systems:

  IBM National Support Center BBS (data connection: 919-517-0001)
  CompuServe (IBM OS/2 Support Forum \Library\IBMFiles\PCMTABLE.ZIP)
  Prodigy
  LAN Server & OS/2 BBS -Sydney Australia
  IBM Austria BBS - Vienna, Austria
  IBM BBS - Vancouver, BC, Canada
  IBM PS BBS - Hong Kong
  IBM OS/2 BBS & IBM AP OS/2 BBS - Singapore
  IBM BBS - Belgium
  IBM BBS - England
  IBM BBS - Spain
  OS2BBS  - Denmark
  Hitline BBS- Switzerland
  DAP & PSP BBS - Italy
  IBM BBS - Jakarta
  IBM BBS - Thailand

NOTE: The compatibility hardware test information supplied is provided for
information purposes.  IBM makes no warranty, express or implied,
with respect to the operation of OS/2 on the personal computers listed.


2.0  COMPATIBILITY
__________________

This graphics accelerator driver is compatible with
OS/2 2.1, 2.11, OS/2 for Windows, and OS/2 Warp 3.


3.0  PRELIMINARY STEPS
______________________

The following steps prepare your computer for the
WD90C24/31 graphics controller device driver:

1.  You must have OS/2 DOS Support installed in order
    to install this driver.
2.  If you previously installed SVGA support, return
    to VGA resolution using the procedures in
    "Setting Your Display to VGA Mode" later in this
    README before you install this driver.
3.  Be sure to copy the VESA** program supplied with
    your system or video adapter and update your
    AUTOEXEC.BAT file to get support for high
    resolution and high color modes.
4.  If you have a video feature disk, verify that it
    has run successfully.
    For Thinkpads, install the "Thinkpad Features" icon
    and utility by using the "install2.exe" program located
    on your video features diskette.  Configure your Thinkpad
    with the utility to support the resolutions and refresh
    settings you desire.  Refer to the README file on the
    video features diskette for more information.


4.0  INSTALLATION FROM DISKETTE
_______________________________

To install the WD90C24/31 device driver from
diskette, do the following:

1.  Insert the WD90C24/31 diskette into drive A (or
    any other diskette drive).
    Note:  This diskette should have a volume label
    of "WD2431 1".  To verify, use "Label A:".
2.  Open an OS/2 full-screen or OS/2 window session.
3.  At the OS/2 command prompt, type the following
    command to copy all necessary files to the OS/2
    drive:

      A:SETUP A: C:

    (where A: is the diskette drive, and C: is the
    drive where OS/2 is installed.)

    Then press Enter.
4.  When prompted to do so, remove the diskette from
    drive A, perform a shutdown, and then restart
    your computer.
5.  Open the OS/2 System folder.
6.  Open the System Setup folder.
7.  Open the Display Driver Install object.
    When the Display Driver Install window appears,
    select Primary Display Driver and then select OK.
8.  When the Display Driver Select window appears,
    select "Western Digital 90C24 (IBM BBS)" or
    "Western Digital 90C31 (IBM BBS)"
    to install the BBS video driver.
9.  When the Monitor Configuration/Selection Utility
    window appears, the "Install Using Defaults for
    Monitor Type" choice is preselected.  You can
    accept this choice or select "Install Using
    Display Adapter Utility Program" to choose a
    different refresh rate.  Then select OK.

    If you select the "Install Using Display Adapter
    Utility Program" choice, you must have the DOS
    monitor utility that came with your display
    adapter.  Contact the display adapter
    manufacturer's technical support for information
    on how to use the monitor utility under OS/2.

    NOTE:  At this point, DSPINSTL determines the
           hardware configuration by creating the
           \OS2\SVGADATA.PMI file.  If the
           \OS2\SVGADATA.PMI file has not been
           created, the adapter will not be
           supported.  This process can take
           several seconds and will black-out the screen.

10. When the Source Directory pop-up window appears,
    insert the WD90C24/31 diskette into drive A.
    Then select Install.

11. When the installation is complete, do the
    following:
    a.  Open the OS/2 System folder.
    b.  Open the System Setup folder.
    c.  Open the System object.
    d.  When the Settings notebook appears, select
        the Screen tab.
    e.  Select a resolution.  Then close the
        notebook.
    f.  Perform a shutdown and restart your computer.

Note that during the installation of this driver,
DISPLAY.LOG and DSPINSTL.LOG files are created in the
OS2\INSTALL directory.  These files identify the OS/2
system files that were updated and indicate whether
the installation was successful.  The contents of
these files might be useful if you need to report an
installation problem to IBM.


5.0 INSTALLATION IN A CID ENVIRONMENT
_____________________________________

NOTES:

1.  The server must contain a directory named WD_DRVS
    on the same drive where the OS/2 diskettes
    reside.  The WD_DRVS directory must contain all
    of the files from the WD90C24/31 device driver
    diskette.
2.  OS/2 must have been successfully installed on the
    client using the CID (Configuration Installation
    Distribution) method.

To install the WD90C24/31 device driver using CID,
use the following information to modify your LCU
command file.

NOTE:  The following information is meant as a guide.
       Your LCU command file might be different.

  /*****************************************************/
  /*           LCU PRODUCT DATA SECTION                */
  /*****************************************************/

                        .
                        .
                        .

  x.wdvideo = 15
  x.15.name='WD Video'
  x.15.statevar = 'CAS_' || x.15.name
  x.15.instprog = 'x:\img\wd_drvs\SETUP.CMD',
                  ' x:\img\wd_drvs ' || bootdrive || ' CID'
  x.15.rspdir   = ''
  x.15.default  = ''

  x.wddspinstl = 16
  x.16.name='WD CID Dspinstl'
  x.16.statevar = 'CAS_' || x.16.name

  /*****************************************************/
  /* FOR WESTERN DIGITAL 31 CHANGE wdc24bb TO          */
  /* wdc31bb WHERE IT OCCURS                           */
  /*****************************************************/

  x.16.instprog = bootdrive || '\os2\install\DSPINSTL.EXE',
                  ' /pd:' || bootdrive || '\os2\install\wdc24bb.dsc',
                  ' /s:x:\img\wd_drvs',
                  ' /t:' || bootdrive,
                  ' /res:640x480x256',
                  ' /u'
  x.16.rspdir   = ''
  x.16.default  = ''

  /*---------------------------------------------------*/
  /*         NUMBER OF PROGRAMS SET UP IN THE          */
  /*               PRODUCT DATA SECTION                */
  /*---------------------------------------------------*/

  NUM_INSTALL_PROGS = 16

  /*****************************************************/
  /*                  INSTALLATION SECTION             */
  /*****************************************************/
                        .
                        .
                        .

      when OVERALL_STATE = 2 then do
        if RunInstall(x.wdvideo) == BAD_RC then exit
        Call RebootAndGotoState(3)
      end
      when OVERALL_STATE = 3 then do
        if RunInstall(x.wddspinstl) == BAD_RC then exit
        Call CheckBoot
      end
                        .
                        .
                        .
  /******************************************************/
  /*                ROUTINE SECTION                     */
  /*  The following information should already exist in */
  /*  the LCU command file.                             */
  /******************************************************/
                       .
                       .
                       .
  RebootAndGotoState:
    parse arg new_state, other

    rc2 = SetState(new_state, 'RebootAndGotoState', 1)    /* Set the state */
                                                          /*  to go to in  */
                                                          /* OVERALL_STATE */

    Call SaveStates                          /* Save the environment vars */

    Call Reboot                              /* Reboot the machine */

    return

                        .
                        .
                        .


  /*****************************************************/
              END OF LCU INFORMATION TO BE ADDED
  /*****************************************************/

Following is an explanation of the line that is
executed in the LCU command file:

  C:\OS2\INSTALL\DSPINSTL /PK:SVGA /SK:NONE /S:X:\
  /T:C: /MC:4 /res:640x480x256

  C:\OS2\INSTALL\DSPINSTL /pd:c:\os2\install\wdc24bb.dsc
  /S:X:\img\wdc_drvs /T:C: /res:640x480x256 /u

     /pd:c:\os2\install\wdc24bb.dsc
      is the dsc laid down during setup phase.

     /S:X:\img\wdc_drvs
      where X:\img\wdc_drvs is the redirected source path.

     /T:C:
      where C: is the drive where OS/2 is installed.

     /res:640x480x256
      is a resolution/color depth from the list of "Supported
      Resolutions" that appears earlier in this README.

     /u
      means Unattended installation.

NOTES:

1.  Be sure you have the stated video memory
    required, as listed in "Supported Resolutions"
    earlier in this README.  A safe choice is
    640x480x256.  Any of the listed resolutions can
    be selected, but your display might be damaged if
    you select a resolution that your display does
    not support.
2.  After the WD90C24 or WD90C31 device driver has been
    successfully installed on the client machine
    using the CID method and the client machine is
    restarted, the resolution will be as specified by
    command line argument.
3.  After the CID install, refer the end user to
    4.0 INSTALLATION FROM DISKETTE step 11.


6.0  FUNCTIONAL RESTRICTIONS
____________________________

o   The WD90C24/31 driver does not support 16-million
    color mode.
o   To avoid a general protection fault while loading
    Ventura Publisher** for Windows**, be sure it is
    in one of the 256 color resolutions.
o   WordPerfect** Versions 5.1 and 5.2 for Windows
    produce a general protection fault when the
    "Print Preview" option is selected while using
    800x600x64K color mode.
o   Users of the software motion video feature of
    MMPM/2* should expect satisfactory results in
    256-color modes.  However, in 64K-color modes,
    OS/2 2.1 users of the feature will experience unusual
    results.  An OS/2 pervasive-fix package is available
    as Fix Package XR06200 for APAR PJ110151.  OS/2 versions
    2.11 and above have this fix.  The software motion video
    feature is not supported in 16-million color mode.
o   Distributed Console Access Facility* (DCAF) is
    supported in 256-color modes only.
o   CorelDRAW** 2.0 will not run in a WIN-OS/2*
    window session.  It must be run in a WIN-OS/2
    full-screen session.
o   Micrografx** Charisma 2.1 will not run in a
    WIN-OS/2 window session.  It must be run in a
    WIN-OS/2 full-screen session.


6.1  FUNCTIONAL RESTRICTIONS FOR LAPTOP COMPUTERS

o   To change refresh rates on the ThinkPad, edit the
    file called IBMVESA\FRATE.DAT.  See
    IBMVESA\TPADVESA.DOC for instructions on how to
    edit this file.
o   On laptop computers with Super-Twisted Nematode
    (STN) display, even though 1MB video memory is
    shipped with the system, only 0.5MB is
    addressable by the software.  The other 0.5MB is
    used internally by the controller.  This will,
    therefore, restrict the number of supported
    resolutions.  Most laptops with STN panels have
    model numbers ending with "S."
o   Many laptops have a built-in internal display
    capable of only a 640x480 resolution when used
    during transportation or at remote sites.
    However, when connected to an external display at
    the office, these systems are capable of 800x600
    and 1024x768 resolutions.
    To avoid the need to select the lower resolution
    prior to leaving the office, the OS/2 device
    driver for the WDC24 automatically detects when
    the internal display is ON and sets the lower
    resolution (even though a higher resolution is
    shown as selected on the Screen page of the
    System Settings notebook).  However, because the
    Windows display drivers cannot automatically
    detect that the internal display is ON, you must
    open the System object, select the Screen page,
    change to a lower resolution, and then shut down
    and restart your system if you want to use a
    WIN-OS/2 window or full-screen session.  (If you
    do not need to use a WIN-OS/2 session, you do not
    need to make the change to the resolution in the
    Settings notebook.  When the laptop is
    reconnected to an external display, the
    originally chosen resolution will be used again.)

    When using your laptop away from the office, the
    System Settings notebook will most likely show
    resolutions which are not possible to use on the
    internal display.  On some laptops, all
    resolutions appear in the System Settings
    notebook, regardless of which displays were on
    when the OS/2 display driver was installed.  On
    most laptops, the higher resolutions appear in
    the System Settings notebook only if the OS/2
    display driver was installed while the internal
    display was OFF.
o   An external display attached to your system can
    use resolutions above 640x480 while an internal
    display cannot.  Whenever you switch to an
    internal display, you should change the
    resolution to 640x480x256 while the external
    display is attached.  To change the resolution,
    do the following:
    1.  Open OS/2 System.
    2.  Open System Setup.
    3.  Open System.
    4.  On the Screen page of the notebook, select
        640x480x256.
    5.  Close the notebook.
    6.  Shut down and restart your computer.

    NOTE:  If you do not follow the above steps, the
           Desktop will automatically switch to the
           640x480x256 resolution because the
           internal display cannot handle the higher
           resolutions.  However, Windows
           applications running in a WIN-OS/2 window
           or full-screen session will have problems
           because the WIN-OS/2 session settings
           cannot automatically update from a higher
           resolution to the 640x480x256 resolution.
           The OS/2 Desktop will be functional enough
           to correct this situation by using the
           above steps.  These steps can be done
           using either the internal or external
           display.

o   MODE 132 will not work on the internal display.
o   MODE 40 on an external display will utilize only
    half of the screen.
o   If your system comes up with a black screen while
    the external display is attached, press the
    display toggle keys to correct the problem.  If
    you have an external keyboard attached to your
    system, refer to the documentation that came with
    your computer for information about the internal
    or external display function key.
o   If you are using an external display, you might
    occasionally encounter a band (usually black)
    across the screen when you start the system.  To
    correct this problem, do the following:
    1.  Perform a shutdown of your system.
    2.  Turn your computer off and then on again.
o   On the Thinkpad 755 CSE, there is a noticeable
    "moving-ripple" effect, especially in the grey areas
    of inactive title bars.  This can be circumvented by
    using different color schemes.  In some cases, running
    Lockup once clears up the problem.


7.0  SETTING YOUR DISPLAY TO VGA MODE
_____________________________________

Use the following procedures to return to VGA mode.

o   If you are installing this driver on OS/2 Warp,
    and you do not have a usable OS/2 Desktop, use
    the following procedures to return to VGA mode.
    However, if you have a usable Desktop, it is
    recommended that you use Selective Install to set
    your display to VGA mode.

    1.  Turn on your computer.  If your computer is
        already on, press Ctrl+Alt+Del to restart it.
    2.  When a small white box appears in the upper
        left-hand corner of your screen, press Alt+F1.
    3.  When the Recovery Choices screen appears, press V.
    4.  Run Selective Install to change the Windows drivers.

    Your display adapter is restored and can work in
    VGA mode.  If you want to install a new display
    adapter or video device driver, refer to Chapter
    16, "Video Procedures," in the User's Guide to
    OS/2 Warp.

o   If you are installing this driver on OS/2 2.1,
    2.11, or OS/2 for Windows, and you do not have a
    usable OS/2 Desktop, use the following procedures
    to return to VGA mode.  However, if you have a
    usable Desktop, it is recommended that you use
    the Display Driver Install object to set your
    display to VGA mode.

    -   If you installed OS/2 from diskettes, do the
        following:

        1.  Start OS/2 using the OS/2 Installation
            Diskette.  When prompted, insert Diskette
            1 and then press Enter.  When the install
            option screen appears, press F3 (or Esc) to
            exit to a command prompt.
        2.  Be sure RSPDSPI.EXE is in the
            \OS2\INSTALL directory.  If it is, go to
            step 3.  If it is not, insert Diskette 8
            into drive A and unpack RSPDSPI.EXE with
            the following command:

              C:\OS2\UNPACK A:\INSTAID C: /N:RSPDSPI.EXE

            (where A: is the drive containing
            Diskette 8, and C: is the drive where
            OS/2 is installed.)
        3.  Type C: and then press Enter.
        4.  Type CD C:\OS2\INSTALL and then press
            Enter.
        5.  Type the following:

              RSPDSPI /PK:VGA /SK:NONE /S:A:\ /T:C:

            (In /T:C:, C: is the drive where OS/2 is
            installed.  In /S:A:, A: is the diskette
            drive you use to install OS/2.)

            Then press Enter.

    -   If you installed OS/2 from CD-ROM or a LAN,
        do the following:

        1.  Start OS/2 using the OS/2 Installation
            Diskette.  When prompted, insert Diskette
            1 and then press Enter.  When the install
            option screen appears, press F3 (or Esc) to
            exit to a command prompt.
        2.  Be sure RSPDSPI.EXE is in the
            \OS2\INSTALL directory.  If it is, go to
            step 3.  If it is not, unpack RSPDSPI.EXE
            with the following command:

              C:\OS2\UNPACK E:\DISK_8\INSTAID C: /N:RSPDSPI.EXE

            (where C: is the drive where OS/2 is
            installed, and E: is the CD-ROM or LAN
            drive.)
        3.  Type C: and then press Enter.
        4.  Type CD C:\OS2\INSTALL and then press
            Enter.
        5.  Type the following:

              RSPDSPI /PK:VGA /SK:NONE /S:E:\OS2SE21\ /T:C:

            (In /T:C:, C: is the drive where OS/2 is
            installed.  In /S:E:, E: is the CD-ROM or
            LAN drive.)

            Then press Enter.


8.0  APAR FIXES INCLUDED IN THIS DRIVER
_______________________________________

Some fixed APARs may not be listed. If you received this
driver through the IBM OS/2 support channel and your requested
APAR is not listed, please install the driver, as your
requested APAR is included.

APAR=PJ17068
750CS/755CS BOOTS TO A BLACK SCREEN ON THE LCD AFTER EXTERNAL
MONITOR IN DISCONNECTED. HAVING CRT HIGHPERFORMANCE ENABLED.

APAR=PJ17994
750CS/755CS BOOT TO A BLACK SCREEN ON THE LCD AFTER EXTERNAL
MONITOR IN DISCONNECTED UNDER WARP FULLPACK.

APAR=PJ16637
IBM THINKPAD IN VGA MODE ALLOWS TESTCASE TO DRAW OUTSIDE THE
AREA GIVEN.

APAR=PJ17803
SEAMLESS WINOS2 SESSION ON IBM THINKPAD 755C SPLITS INTO PIECES
RUNNING UNDER OS2 WARP 3.0 FULLPAK IN SVGA. VGA WORKS FINE.

APAR=PJ18129
SELECTING FILE PULLDOWN MENU FROM WINOS2 FULLSREEN SESSION IN
1024*768*256 ON CRT, LEAVES BEHIND COLOR TRACES CAUSING CORRUPTION.

APAR=PJ18487
SEAMLESS WINDOWS APPLICATIONS ON LCD WHILE WD3108SL IS STILL SET
TO 1024*768 CAUSES THE MOUSE POINTER TO TURN INTO A 1-INCH BLACK
BLOCK.

***********
Build D.036
***********

APAR= PJ16415
TRAP 000D MICROSOFT COMPILER 6.0,SYS3175
AN ACCESS VIOLATION AT 17FE0F9A BVHSVGA.

APAR= PJ17608
BM_SRCTRANSPARENT OPTION OF GPISETBACKMIX DOES NOT FUNCTION
DISPLAYS PINK TITLE BAR.

APAR= PJ18290
TELENEX V9.1 UNDER WARP FOR WINDOWS HANGS THE SYSTEM WHEN USING
WESTERN DIGITAL DRIVERS IN SVGA MODE

APAR= PJ18312
TELENEX V9.1 UNDER WARP FULLPACK HANGS THE SYSTEM WHEN USING
WESTERN DIGITAL DRIVERS IN SVGA MODE

APAR= PJ18376
VIDEO CORRUPTION ON THINKPADS 755CD/755CE RUNNING CM/2 IN 65K
COLORS (640*480*65K). CORRUPTION DOES NOT ACCUR IN 16/256 COLORS

APAR= PJ18377
VIDEO CORRUPTION ON THINKPADS 755CD/755CE RUNNING CM/2 IN 65K CO
LORS (640X480X65K) UNDER WARP FULLPACK

APAR= PJ18666
PROBLEM EDITING IMAGE UNDER ULTIMEDIA BUILDER/2 V1.0.1 FOR OS2
ON IBM THINKPAD 750/755CD USING WD90C24 DRIVERS.

APAR= PJ18707
THINKPAD 755CE USING WD90C24 LATEST DRIVERS BOOTS UP TO A BLANK
SCREEN IN 640X480X256 ONLY, UNDER WARP FULLPACK

APAR= PJ18709
THINKPAD 755CE WD90C24 LATEST DRIVERS BOOTS UP TO A BLANK
SCREEN IN 640*480*256 ONLY, UNDER WARP HALF-PAK

APAR= PJ18961
THINKPAD 755C WITH WD90C24 BUILD .026 PRODUCES BLUE HAZE ON LCD
IN SVGA AFTER UNPLUGGING THE EXTERNAL MONITOR WITH WARP FULLPACK

APAR= PJ18963
THINKPAD 755C WITH WD90C24 BUILD .026 PRODUCES BLUE HAZE ON LCD
N SVGA AFTER UNPLUGGING THE EXTERNAL MONITOR WITH WARP HALF PACK

APAR= PJ19011
THINKPAD 755CSE, NO HIGH RESOLUTION AVAILABLE ON THE EXTERNAL
MONITOR AFTER INSTALLING THE NEW WD90C24 BUILD D.026 DRIVERS.

APAR= PJ19163
WD90C24 DRIVERS BUILD 027 UNDER 1024X768X256 RESOLUTION ON
THINKPAD 755CX UNDER WARP FULL PACK GIVES MOUSE CORRUPTION

APAR= PJ19164
WD90C24 DRIVERS BUILD 027 IN 1024X768X256 RESOLUTION ON
THINKPAD 755CX UNDER WARP FULL PACK GIVES MOUSE CORRUPTION

APAR= PJ20406
WD90C24 UNDER 800X600X256 DISPLAYS WINOS2 FULL SCREEN IN VGA
MODE UNDER WARP FULLPACK


9.0  TRADEMARKS
_______________

The following terms, denoted by an asterisk (*) in
this file, are trademarks or registered trademarks of
IBM Corporation in the United States and/or other
countries:

    DCAF
    IBM
    MMPM/2
    OS/2
    Presentation Manager
    ThinkPad
    WIN-OS/2

The following terms, denoted by a double asterisk
(**) in this file, are trademarks or registered
trademarks of other companies as follows:

TRADEMARK                OWNER

CorelDRAW                Corel Corporation

Dell                     Dell Computer Corporation

Micrografx               Micrografx Incorporated

Ventura Publisher        Ventura Software, Inc.

VESA                     Video Electronics Standards
                         Association

Western Digital          Western Digital Corporation

Windows                  Microsoft Corporation

WordPerfect              WordPerfect Corporation


IBM DISCLAIMS ALL WARRANTIES, WHETHER EXPRESS OR
IMPLIED, INCLUDING WITHOUT LIMITATION, THE IMPLIED
WARRANTIES OF FITNESS FOR A PARTICULAR PURPOSE AND
MERCHANTABILITY WITH RESPECT TO THE INFORMATION IN
THIS DOCUMENT.  BY FURNISHING THIS DOCUMENT, IBM
GRANTS NO LICENSES TO ANY RELATED PATENTS OR
COPYRIGHTS.

THIS DRIVER IS COPYRIGHTED BY INTERNATIONAL BUSINESS
MACHINES CORPORATION.  ALL APPROPRIATE RESTRICTIONS
APPLY.

                              (End of Document)
