**
**
**  VIA Rhine Family Fast Ethernet Adapter
**
**  Linux Driver
**
**  v4.25  Jun. 2003
**
**
                 
         
Introduction:
=============

    The instructions listed below are for linux driver installation. You must
    compile the source code to generate rhinefet.o and use insmod command to
    insert rhinefet.o as module.


Contents of the Subdirectory:
=============================

    linux.txt               This file.    
    rhinefet.c              The linux core driver source code file
    Makefile                Makefile for generating driver object file
    rhine_vmns.c            The vmns driver support source file
    rhine_proc.c            The source to create proc entries
    rhine_wol.c             The WOL supporting source file   
    rhine.h                 The extended driver header file
    rhine_vmns.h            The vmns driver support header file
    rhine_proc.h            The header file for proc entries
    rhine_wol.h             The WOL supporting header file
    rhine_cfg.h             The vmns driver support header file
    vmns_drv.h              The vmns driver support header file

Kernel Supported
================
    This driver support linux kernel version 2.2.x and 2.4.x now.

Installation
============
    Please enter the following commands at the UNIX prompt. Remember, UNIX is
    case sensitive.

    1) Create a temporary directory:
        mkdir /temp

    2) Change to the temporary directory:
        cd /temp

    2) Copy driver (rhinefet.tgz) from DOS disk, (mcopy below is one tool in
       mtools, if you didn't install mtools, you can type 
       'mount -t msdos /dev/fd0 /mnt' and use 'cp /mnt/rhinefet.tgz /temp'
       command to copy the driver to the temporary directory):
        mcopy a:rhinefet.tgz .

    3) untar the archive file:

        tar xzvf rhinefet.tgz
        cd rhinefet
                         
    4) Compile the driver source files and it will generate rhinefet.o, and
       copy it to correct driver installation path (The installation directory
       is different in different kernel versions. In 2.4.x kernel, the path is 
       /lib/modules/KERNEL_VERSION/kernel/drivers/net/, and in 2.2.x kernel,
       the path is /lib/modules/KERNEL_VERSION/net/, the KERNEL_VERSION (see
       above) means the kernel version of your Linux distribution. If you don't
       know your kernel version , please run 'uname -r' command in command 
       line. The kernel version will look like '2.2.16', '2.4.2-2smp' etc.) :
        make install

    5) Check configuration file (/etc/modules.conf or /etc/conf.modules,it 
       depend on your Linux distribution) for loading kernel modules. Make sure
       there is the following content in the configuration file, where # is 
       interface number (eg: alias eth0 rhinefet):
        alias eth# rhinefet

    6) Reboot now:
        shutdown -r now

    7) Install your driver module (If the driver module is in the wrong place,
       an error message will appear, and say that can't find the driver 
       module):
        insmod rhinefet

    8) Use ifconfig command to assign the IP address, where # is network 
       interface number:
        ifconfig eth# <IP>

    9) Check the interface works:
        ping <remote_host_IP>


Uninstallation
==============
    Please enter the following commands to uninstall your driver:
        make uninstall

Note 
====
    1) Make sure the link file /usr/src/linux (or /usr/src/linux-2.4) is linked
       to correctly kernel sources directory (eg: if you run 'uname -r', it
       appears "2.4.2-2", then the link file must be linked to 
       /usr/src/linux-2.4.2 directory, or you will fail in compiling),
       and make sure there are kernel header files in /usr/src/linux/include
       directory (or /usr/src/linux-2.4/include), we need kernel header files
       in compling.

    2) If you can't install driver in SUSE Linux using insmod or modprobe
       commands, and error messages appear (see below), please run 'uname -r'
       in command line. And make sure the result of 'uname -r' (eg: 2.4.2-4GB)
       is the same with the definition of UTS_RELEASE in 
       /usr/src/linux/include/linux/version.h. If not, please modify the 
       definition of UTS_RELEASE in /usr/src/linux/include/linux/version.h.

         rhinefet.o: kernel-module version mismatch
	         rhinefet.o was compiled for kernel version 2.4.2
	         while this kernel is version 2.4.2-4GB.

    3) Make sure that your kernel is built with network, fast_ethernet
       and module support. Otherwise, you have to rebuild your kernel (see
       below).
        1. Go to /usr/src/linux (or /usr/src/linux-2.4) directory:
            cd /usr/src/linux
        2: Run 'make menuconfig' or 'make config' in text mode, or 'make 
           xconfig' in graphic mode.
        3: Mark the options list above.
        4: Exit and rebuild your kernel:
            make dep;make clean;make bzImage
           The file 'bzImage' will be at /usr/src/linux/arch/i386/boot/bzImage
        5: Modify /etc/lilo.conf.(this file specifies where kernel image is)
        6: Run 'lilo'
        7: Reboot, and select the correct kernel image to boot your system.

    4) You can use the utility (like netconfig, linuxconf) in your Linux 
       distribution to set your network parameters(like ip,gateway). These
       parameters will be used at boot time. The following is the demonstration
       to show how to use linuxconf (it's a utitlity in RedHat Linux 6.x) set
       the network paramters.
       1. Run linuxconf:
           linuxconf
       2. Enter setting in the Config/Networking/Client tasks/Basic host information/
          and fill out the following information. Where 'xxx' is the IP address
          what you have.
                    IP address:    xxx.xxx.xxx.xxx
                    Netmask:       255.255.255.xxx
                    Net device:    eth0
                    Kernel module: rhinefet
        
    5) If you can't install driver at boot time.
       If you can install your driver using insmod command, but you can't
       install it at boot time, please check whether the driver is in the
       correct directory (eg: /lib/modules/2.2.XXX/net/), and check the
       /lib/modules/2.2.XXX/modules.dep file, it must include the following
       line:
            /lib/modules/2.2.XXX/net/rhinefet.o:

       You can insert this line using depmod command or insert it manually.
       Also, you must consult your Linux distribution installation guide
       and learn how to set the IP address of your network interface and 
       up it at boot time.

    6) If you can't compile this driver, and parse error messages appear,
       please make sure your source code text format is right. You must convert
       your source code text format from MS-DOS to UNIX, as show below (see
       Solution 1 and 2).
       Make sure the files in floppy disk are not rhinefet.tgz file. They must
       be the source code text files (5 files), rhinefet.tgz is not a text file
       , so it can't be converted.

        Solution1:
            If you use mcopy command to copy your driver from floppy disk to
            linux, you can type:
                mcopy -t a:\* .
            then it will convert the format for you. 

        Solution2:
            If you use mount command to mount floppy disk to linux, you can
            type:
                mount -t vfat -o conv=t /dev/fd0 /mnt/floppy
            then, when you copy files from /mnt/floppy, these files format will
            be right.

Module Parameter:
=================
The following parameters can be set when we install the driver module. You can add this parameters when
you execute 'insmod' or 'modprobe' command to install the driver (as below).
    insmod rhinefet.o parameter=value1,value2,value3,...
For example, if you have 3 NIC cards, and you want to set the speed_duplex paramter value of them .
You can type the following command to set it.
    insmod rhinefet.o speed_duplex=1,2,3
Then, the parameter value of first card will be 1 (100Mbps half duplex mode), the second card will
be 2 (100Mbps full duplex mode), and the third card will be 3 (10Mbps half duplex mode).
Remember, our driver only support 8 cards parameter setting. 

1) speed_duplex
   speed_duplex[] is used for setting the speed and duplex mode of NIC.
   Value:
       0: indicate autonegotiation for both speed and duplex mode (Default).
       1: indicate 100Mbps half duplex mode
       2: indicate 100Mbps full duplex mode
       3: indicate 10Mbps half duplex mode
       4: indicate 10Mbps full duplex mode

2) enable_tagging
   enable_tagging[] is used for enabling VLAN ID setting and enabling
   priority transmit.
   Value:
       0: disable VID setting and priority transmit (Default).
       1: enable VID setting and priority transmit.

3) VID_setting
   VID_setting[] is used for setting the VLAN ID of NIC.
   Value:
       0: default VID.
       1-4094: other VIDs.

4) csum_offload
   csum_offload[] is used for setting the checksum offload ability of NIC.
   Value:
       0: disable csum_offload (Default).
       1: enable checksum offload. (We only support RX checksum offload now)

5) txcsum_offload (For management adapter only) 
   csum_offload[] is used for setting the checksum offload ability of NIC.
   Value:
       0: disable (default)
       1: enable


6) flow_control
   flow_control[] is used for setting the flow control ability of NIC.
   Value:
       1: hardware deafult (Default). Use Hardware default value in ANAR.
       2: disable PAUSE in ANAR.
       3: enable PAUSE in ANAR.


7) IP_byte_align
   IP_byte_align[] is used for IP header DWORD byte aligned (For IPVS environment).
   (In some enviroment, the IP header should be DWORD byte aligned,or the packet
   will be droped when we receive it. (eg: IPVS))
   Value:
       0: indicate the IP header won't be DWORD byte aligned (Default).
       1: indicate the IP header will be DWORD byte aligned.


8) tx_thresh
   tx_thresh[] is used for controlling the transmit fifo threshold.
   Value:
       0: indicate the txfifo threshold is 128 bytes (Default).
       1: indicate the txfifo threshold is 256 bytes.
       2: indicate the txfifo threshold is 512 bytes.
       3: indicate the txfifo threshold is 1024 bytes.
       4: indicate that we use store and forward

9) rx_thresh
   rx_thresh[] is used for controlling the receive fifo threshold.
   Value:
       0: indicate the rxfifo threshold is 64 bytes (Default).
       1: indicate the rxfifo threshold is 32 bytes.
       2: indicate the rxfifo threshold is 128 bytes.
       3: indicate the rxfifo threshold is 256 bytes.
       4: indicate the rxfifo threshold is 512 bytes.
       5: indicate the rxfifo threshold is 768 bytes.
       6: indicate the rxfifo threshold is 1024 bytes.   
       7: indicate that we use store and forward
       
10) DMA_length
   DMA_length[] is used for controlling the DMA length.
   Value:
       0: 8 DWORDs
       1: 16 DWORDs (Deafult)
       2: 32 DWORDs
       3: 64 DWORDs
       4: 128 DWORDs
       5: 256 DWORDs
       6: SF(flush till emply)
       7: SF(flush till emply)

11) ValPktLen
    ValPktLen[] is used for controlling driver to receive or drop
    the frame with invalid layer 2 length.
    Value:
        0: Receive frame with invalid layer 2 length.
        1: Drop frame with invalid layer 2 length.

12) wol_opts
    wol_opts[] is used for controlling wake on lan behavior of NIC.
    0: Wake up if recevied a magic packet. (Default)
    1: Wake up if link status is on/off.
    2: Wake up if recevied an arp packet.
    4: Wake up if recevied any unicast packet.
    Those value can be sumed up to support more than one option.
