### System Requirements

> In addition to the items shipped with the client adapter, you need the following items in order to install and use the adapter:

> - A computer running the Windows 2000 or XP operating system and equipped with a 32-bit Cardbus slot or an empty PCI expansion slot
> - Service Pack 1 for Windows XP (recommended)
> - 20 MB of free hard disk space (minimum)
> - 128 MB of RAM or later (recommended)
> - The appropriate tools for removing your computer's cover and expansion slot dust cover and for mounting the antenna base
> - Certificate Authority (CA) and user certificates for EAP-TLS authentication or CA certificate for PEAP authentication
> - If your wireless network uses EAP-TLS or PEAP authentication, Certificate Authority (CA) and user certificates for EAP-TLS authentication or CA certificate for PEAP authentication
> - If your wireless network uses PEAP (EAP-GTC) authentication with a One-Time Password (OTP) user database, you need a hardware token device and your hardware or software token password.

> The following information from your system administrator:

> - The logical name for your workstation (also known as client name)
> - The protocols necessary to bind to the client adapter, such as TCP/IP
> - The case-sensitive service set identifier (SSID) for your RF network
> - If your network setup does not include a DHCP server, the IP address, subnet mask, and default gateway address of your computer
> - The wired equivalent privacy (WEP) keys of the access points with which your client adapter will communicate, if your wireless network uses static WEP for security
> - The username and password for your network account