----------------------------------------------------------------------------
                   Canon Camera TWAIN Driver
                         ReadMe File

                          Version 6.0
----------------------------------------------------------------------------
                  Copyright (c) 2003 Canon Inc.
____________________________________________________________________________

Congratulations on your purchase of a Canon camera! 
This ReadMe file presents the latest information about the Canon Camera 
TWAIN driver. Be sure to read it before using the TWAIN driver.


About the TWAIN specification

The TWAIN specification is regularly updated, and software developers modify
their software to reflect these changes. However, problems may occur because
some applications do not fully comply with the current TWAIN specification. 
Canon works closely with many software companies to identify and resolve 
these problems so that you can run our software without difficulty. 


You can find the latest information on the Canon Camera TWAIN driver 
at the following URL:

  http://web.canon.jp/Imaging/readme/index-e.html 
____________________________________________________________________________


--------
Contents
--------
1. Problems that may occur when using some display cards 
2. RAW images and video images
3. Applications and system configurations
4. Communication between the Canon Camera TWAIN driver and a Canon camera
5. About Windows 98SE
6. Connecting to an EOS digital camera



1. Problems that may occur when using some display cards 
================================================
Some display cards may cause operations to be unstable when the TWAIN driver
is started from Photoshop 5.0 LE. 
If this happens, run the dispinit.exe fix program and then start Photoshop 
to use the TWAIN driver. 
We recommend that you register dispinit.exe as a Windows startup program 
since it must be run after each system startup. 

   The dispinit.exe program is located in the same folder as the installer 
(setup.exe). 
   On the CD, it is stored in the 
[SOFTWARE / TWAIN / camera model name / language] folder. 


2. RAW images and video images
==================================
RAW images and video images are not displayed in the Thumbnails list using 
this TWAIN driver. 
Be sure to check the contents of your memory card before formatting it. 


3. Applications and system configurations
===========================================
Canon has tested this driver with as many TWAIN-compatible applications and 
system configurations as possible. The following compatibility problems have
been found. 

[Transferring images to Photoshop 5.0 LE]
    The maximum number of images that can be transferred to Photoshop 5.0 LE
at one time is 30. 


4. Communication between the Canon Camera TWAIN driver and a Canon camera
=============================================================
(1) When connected to a camera with the TWAIN driver running, the driver 
regularly communicates with the camera. Do not use the camera controls, 
remove the memory card or battery, or unplug the communications cable while 
the driver and the camera are in communication. 
These actions may cause misoperation on some PCs. 
Exit the TWAIN driver before performing these actions. 

(2) Do not put your computer in Standby mode while a Canon camera is 
connected to the USB or IEEE1394 port. 
If you accidentally put your computer in Standby mode while a Canon camera 
is connected to the USB or IEEE1394 port, leave the camera connected to the 
computer and bring the computer out of Standby mode. 
Unplugging the cable from the computer while in Standby mode may cause some 
computers to fail to come out of Standby mode correctly. See the user manual
for your computer for more information about Standby mode. 


5. About Windows 98SE
=============================
(1) For more stable operations, we recommend that users connecting a camera 
with an IEEE1394 interface to a computer running Windows 98SE download and 
install the following update program from the Microsoft web site. 

    "Windows 98 Second Edition 1394 Storage Supplement"

(2) If you connect a camera to a computer running Windows 98SE, set 
the Auto Power Off setting to [Off]. 


6. Connecting to an EOS digital camera
==================================
You cannot communicate with a camera when the camerafs LCD monitor is on. 
If the LCD monitor is on, turn it off by pressing the shutter button 
halfway, and then connect the camera. 

<End of File>
