;
; nv_agp.inf
;
;
; NVIDIA Windows 2000 AGP INF file
; Copyright 1999-2002 NVIDIA Corporation.  All Rights Reserved.
;

[Version]
CatalogFile=nv_agp.cat
Signature="$WINDOWS NT$"
Class=System
ClassGuid={4D36E97D-E325-11CE-BFC1-08002BE10318}
Provider=%NVIDIA%
LayoutFile=layout.inf
DriverVer = 09/06/2002, 2.7.8

[DestinationDirs]
DefaultDestDir = 12        ; DIRID_DRIVERS

[SourceDisksNames]
222=%DiskDescription%,,,

[SourceDisksFiles]
nv_agp.sys=222

[Manufacturer]
%NVIDIA_MFG%=NVIDIA_AGP

[AGP_Filter_Reg]
HKR,,"UpperFilters", 0x00010000,"nv_agp"

[pci_ServiceInstallSection]
DisplayName    = %pci_svcdesc%
ServiceType    = %SERVICE_KERNEL_DRIVER%
StartType      = %SERVICE_BOOT_START%
ErrorControl   = %SERVICE_ERROR_NORMAL%
ServiceBinary  = %12%\pci.sys
LoadOrderGroup = "Boot Bus Extender"


[NVIDIA_AGP]
%PCI\VEN_10DE&DEV_01B7.DeviceDesc%=NVIDIAAGP_Install,PCI\VEN_10DE&DEV_01B7
%PCI\VEN_10DE&DEV_01E8.DeviceDesc%=NVIDIAAGP_Install,PCI\VEN_10DE&DEV_01E8

;
; NVIDIA AGP chipset
;
[NVIDIAAGP_Install]
CopyFiles=@nv_agp.SYS

[NVIDIAAGP_Install.HW]
AddReg = AGP_Filter_Reg

[NVIDIAAGP_Install.Services]
AddService = nv_agp,0,NVIDIAAGP_ServiceInstallSection
AddService = pci, %SPSVCINST_ASSOCSERVICE%, pci_ServiceInstallSection

[NVIDIAAGP_ServiceInstallSection]
DisplayName    = %agpnvidia_svcdesc%
ServiceType    = %SERVICE_KERNEL_DRIVER%
StartType      = %SERVICE_DEMAND_START%
ErrorControl   = %SERVICE_ERROR_NORMAL%
ServiceBinary  = %12%\nv_agp.sys
LoadOrderGroup = PnP Filter

[ControlFlags]
ExcludeFromSelect=*

[Strings]
NVIDIA="NVIDIA Corporation"
NVIDIA_MFG="NVIDIA"
PCI\VEN_10DE&DEV_01B7.DeviceDesc = "NVIDIA nForce AGP Host to PCI Bridge"
PCI\VEN_10DE&DEV_01E8.DeviceDesc = "NVIDIA nForce2 AGP Host to PCI Bridge"
DiskDescription  = "NVIDIA nForce Driver Disk"

;service descriptions
pci_svcdesc = "PCI Bus Driver"
agpnvidia_svcdesc = "NVIDIA nForce AGP Bus Filter"

;Handy macro substitutions (non-localizable)
SPSVCINST_ASSOCSERVICE = 0x00000002
SERVICE_KERNEL_DRIVER  = 1
SERVICE_BOOT_START     = 0
SERVICE_DEMAND_START   = 3
SERVICE_ERROR_NORMAL   = 1
