Intel® Server Board SE7500WV2
The products you are looking for are no longer manufactured by Intel. Additionally, Intel no longer provides interactive support for these products via telephone or e-mail, nor will Intel provide any future content updates or software updates to support new operating systems or improve compatibility with third party devices and software products. THESE PRODUCT SUPPORT DOCUMENTS ARE PROVIDED FOR HISTORICAL REFERENCE ONLY AND ARE SUBJECT TO THE TERMS SET FORTH IN THE "TERMS OF USE" INFORMATION. Information on currently available Intel products is available at www.intel.com and/or developer.intel.com

Identify your product
  Product Discontinuance Announcement
    Intel® will no longer provide interactive support for these products via telephone or e-mail.

Software and drivers

Technical specifications
  Technical Product Specifications
    Product overview, including descriptions and diagrams of the integrated features
    SE7500WV2_TPS.PDF
  Specification update
    An update to the specifications contained in the Technical Product Specification
    Specification Update [PDF]

Installation and Use
  Adapter Teaming
    Intel® Server Management and Adapter Teaming are not compatible with each other. A third network adapter is necessary if you require both management and a teamed network interface.
  AGP Support on Server Products
    Only the Intel® Server Boards T440BX, S845WD1-E, S875WP1-E, and SE7505VB2 have an AGP slot to allow an AGP video card to be plugged in.
  Authentication of "None" allowed by management utilities
    Download the BMC LAN Fix Utility and the CLI AutoConfig Utility 1.05.
  Clearing Processor Errors During POST
    BIOS > Main > Processor Settings > Processor Retest
  Configuring a RAID Array using the on-board Promise* ATA RAID Controller
    When the Promise* FastTrack100™ BIOS screen appears, press CTRL+F to go to the setup screen.
  DPC console reports "connection lost" with Cisco* Catalyst 4006
    Enable PortFast on the switch.
  Error: "Warning - FastTrak does not detect proper interrupts"
    Do not press the "Pause" key while the Promise* option ROM is loading.
  Error: CMOS Checksum Bad
    Clear the CMOS. See the TPS for instructions.
  How to set up LAN Alerts
    On the managed server:
    Boot to the System Setup Utility (SSU) from either the Service Partition or the System Resource CD > Platform Event Manager > Configure LAN > Enable LAN Alerts
    On the client side:
    Install Intel® Server Management > Start > Programs > Intel Server Management > LAN Alerts Viewer > Configure
  OS install cannot detect hard drives
    A single drive jumpered as slave will allow RAID array creation, but the OS install will fail. Configure single drives as master instead.
  Platform Confidence Test Manual
    Generic_BYO_PCT_Manual_3.0.pdf
  Product Guide
    Product Guide in English [WV2_PG.PDF]
    Product Guide in Simplified Chinese [WV2_PG_SCHINESE.PDF]
    Product Guide in Spanish [WV2_PG_SPANISH.PDF]
  Quick Start User Guide
    Quick Start User Guide [PDF]
    Step #7-B of the Intel® Server Chassis SR2300 Quick Start User Guide incorrectly states that four system fans are required for dual processor configurations. Three system fans are sufficient.
  Setting Up a Password for Intel® Server Management
    System Setup Utility > Platform Event Manager > Configure LAN > Password
  Spares/Parts List & Configuration Guide
    Spares/Parts List & Configuration Guide
  SRCMRU with firmware 2.32 not working
    The SRCMR controller requires firmware 2.33.01-R01B.
  System Event Log #83
    The BMC logs one or two system boot events in the SEL when the BIOS finishes POST. These messages are normal.
  Troubleshooting Guide
    TS_GUIDE.PDF
  Unable to access the RAID Option ROM during POST
    The Matrix Storage Manager Option ROM will display only when RAID is enabled in the BIOS, at least two drives are connected to the system, and Quiet Boot is disabled in the BIOS.
  Unknown devices in Device Manager
    Download the INF Update Utility and the Windows* 2000 NIC Driver and the ESG-SHV Backplane Driver for Microsoft Windows*.
  Viewing the System Event Log (SEL)
    System Setup Utility > System Setup Screen > SEL Manager > View SEL Manager > File > Save As > Save as *.sel or *.txt.
  Windows* 2000 Advanced Server recognizes only 4 GB of memory
    The /PAE option must be enabled in the ARC path in the boot.ini file in order for Windows* 2000 to recognize memory above 4.0GB (e.g. multi(0)disk(0)rdisk(0)partition(2)\WINNT="Windows 2000 Advanced Server" /PAE /basevideo /sos).

Compatibility
  Tested Chassis
    Intel SR1300 (KCW)
    Intel SR2300 (KSW or KSW480)
    AIC RMC1Q2-51-SWV2
    AIC RMC2Q2-SWV2
    CiDesign RS2601
    CCSI RC-0103X-WV2
    Chenbro RM115
    Chenbro RM118
    Chenbro RM214
  Tested Hardware and Operating Systems
    Microsoft* Windows* 2000 Advanced Server, Service Pack 2
    Novell Netware* 6.0
    Red Hat Linux* 7.3
    SuSE* Linux 8.0
    TESTEDHW_OS.PDF
  Tested Memory
    Tested Memory List Report [PDF]
  Tested Power Supplies
    Delta* DPS-B480BBA 480W
    Enhance* ENS00246 460W
    NMB* SD237U480NSW 480W
    Zippy* P2G-6460P 460W
  Tested Processors
    80532KC041512U
    80532KC049512
    80532KC056512
    80532KC064512
    80532KC072512
    BX80532KC1800D
    BX80532KC1800DU
    BX80532KC2000D
    BX80532KC2000DU
    BX80532KC2200D
    BX80532KC2200D
    BX80532KC2200DU
    BX80532KC2400D
    BX80532KC2400D
    BX80532KC2400DU
    BX80532KC2600D
    BX80532KC2600DU
    BX80532KC2800D
    BX80532KC2800DU

Technical advisories
  TA615: VBAT, POST 8300 errors or RTC time loss instances
    TA_615.PDF
  TA628: BIOS Flash Chip Not Fully Write Protected
    TA_628.PDF
  TA654: Hang at POST Code 12, 13, and 15 Or During Operating System Boot
    TA_654.PDF
  TA693: Updates Needed After Intel® Server Management Uninstall
    TA69301.PDF