Intel® Server Board SE7501WV2
The products you are looking for are no longer manufactured by Intel. Additionally, Intel no longer provides interactive support for these products via telephone or e-mail, nor will Intel provide any future content updates or software updates to support new operating systems or improve compatibility with third party devices and software products. THESE PRODUCT SUPPORT DOCUMENTS ARE PROVIDED FOR HISTORICAL REFERENCE ONLY AND ARE SUBJECT TO THE TERMS SET FORTH IN THE "TERMS OF USE" INFORMATION. Information on currently available Intel products is available at www.intel.com and/or developer.intel.com

Identify your product
  Product Discontinuance Announcement
    Intel will no longer provide interactive support for these products via telephone or e-mail.

Software and drivers

Technical specifications
  Technical Product Specifications

    Product overview, including descriptions and diagrams of the integrated features (PDF)

    | Technical Product Specification (PDF)

    Note: PDF Files require Adobe Acrobat* Reader*

Installation and use
  4-3-4-4 beep code during POST
    Fully populate memory Bank 1 (slots 1A and 1B) before populating other memory banks.
  Adaptec* Host RAID supported RAID Levels
    The onboard Adaptec* 7901/7902 SCSI controller supports RAID 0 and RAID 1.
  Adaptec* Host RAID User's Guide (PDF)

    | Adaptec* Host RAID User's Guide (PDF)

    Note: PDF Files require Adobe Acrobat* Reader*

  AGP Support on Server Products
    Only the Intel® Server Boards T440BX, S845WD1-E, S875WP1-E, and SE7505VB2 have an AGP slot to allow an AGP video card to be plugged in.
  Authentication of "None" allowed by management utilities
    Download the BMC LAN Fix Utility and the CLI AutoConfig Utility 1.05.
  Clearing Memory Errors During POST
    BIOS > Advanced > Memory Settings > Memory Retest
  Clearing Processor Errors During POST
    BIOS > Main > Processor Settings > Processor Retest
  Error: CMOS Checksum Bad
    Clear the CMOS. See the TPS for instructions.
  Error: No Valid Controller Found with a Zero Channel RAID Controller
    Disable the Adaptec* Host RAID option:
    1. During POST, while the Adaptec* Option ROM is initializing, press the [CTRL+A] key combination.
    2. From the device menu that appears, select a channel and press Enter.
    3. From the Main Options menu, select Disable HostRAID and press Enter. (If the controller has two channels, make sure that steps 1 through 3 are performed for the second channel)
    4. Save and exit.
  Fault Resilient Booting (FRB) Functionality

    The BMC (Baseboard Management Controller) implements FRB levels 1, 2, and 3. If the default bootstrap processor (BSP) fails to complete the boot process, FRB attempts to boot using an alternate processor.

    FRB level 1 is intended to recover from a BIST failure detected during POST. This FRB recovery is fully handled by BIOS code.

    FRB level 2 is intended to recover from a watchdog timeout during POST. The watchdog timer for FRB level 2 is implemented in the BMC.

    FRB level 3 is intended to recover from a watchdog timeout on hard reset or power-up. This provides hardware functionality for this level of FRB.

    FRB-1 In a multiprocessor system, the BIOS registers the application processors in the multi-processor (MP) table and the ACPI APIC tables. When started by the BSP, if an application processor (AP) fails to complete initialization within a certain time, it is assumed to be nonfunctional. If the BIOS detects that an application processor has failed BIST or is nonfunctional, it requests the BMC disable that processor. The BMC then generates a system reset while disabling the processor; the BIOS will not see the failed processor in the next boot cycle. The failing AP is not listed in the MP table, nor in the ACPI APIC tables, and is invisible to the OS. If the BIOS detects that the BSP has failed BIST, it sends a request to the BMC to disable the present processor. If there is no alternate processor available, the BMC beeps the speaker and halts the system. If the BMC can find another processor, BSP ownership is transferred to that processor via a system reset.

    FRB-2 The second watchdog timer (FRB-2) in the BMC is set for approximately 6 minutes by BIOS and is designed to guarantee that the system completes BIOS POST. The FRB-2 timer is enabled before the FRB-3 timer is disabled to prevent any "unprotected" window of time. Near the end of POST, before the option ROMs are initialized, the BIOS will disable the FRB-2 timer in the BMC. If the system contains more than 1 GB of memory and the user chooses to test every DWORD of memory, the watchdog timer is disabled before the extended memory test starts, because the memory test can take more than 6 minutes under this configuration. If the system hangs during POST, the BIOS will not disable the timer in the BMC, which generates an asynchronous system reset (ASR).

    FRB-3 The first timer (FRB-3) starts counting down whenever the system comes out of hard reset, which is usually about 5 seconds. If the BSP successfully resets and starts executing, the BIOS will disable the FRB-3 timer in the BMC by de-asserting the FRB_TIMER_HLT signal (GPIO) and the system continues on with the POST. If the timer expires because of the BSP's failure to fetch or execute BIOS code, the BMC resets the system and disables the failed processor. The system continues to change the BSP until the BIOS POST gets past disabling the FRB-3 timer in the BMC. The BMC sounds beep codes on the speaker if it fails to find a good processor. The process of cycling through all the processors is repeated upon system reset or power cycle.

  How to set up LAN Alerts

    On the managed server:
    Boot to the System Setup Utility (SSU) from either the Service Partition or the System Resource CD > Platform Event Manager > Configure LAN > Enable LAN Alerts

    On the client side:
    Install Intel® Server Management > Start > Programs > Intel Server Management > LAN Alerts Viewer > Configure

  Korean EMC Certification
    E-G011-03-0304(A)
  One Boot/Flash Update Utility Appears To Hang
    The utility may take up to 45 seconds updating a system with a Hot Swap Controller (HSC).
  Platform Confidence Test - Installation and operating instructions (PDF)

    | Intel® Server Board Platform Confidence Test (PDF)

    Note: PDF Files require Adobe Acrobat* Reader*

  Product Guide (PDF)

    | Product Guide for the Intel® Server Board SE7501WV2 (PDF)

    Note: PDF Files require Adobe Acrobat* Reader*

  Quick Start Guide (PDF)

    | Quick Start Guide (PDF)

    Note: PDF Files require Adobe Acrobat* Reader*

  Setting Up a Password for Intel® Server Management
    System Setup Utility > Platform Event Manager > Configure LAN > Password
  Spares/Parts List & Configuration Guide (PDF)

    | Spares/Parts List and Configuration Guide (PDF)

    Note: PDF Files require Adobe Acrobat* Reader*

  System Event Log #83
    The BMC logs one or two system boot events in the SEL when the BIOS finishes POST. These messages are normal.
  Unable to access the RAID Option ROM during POST
    The hotkey option to enter the Option ROM is disabled by default. Disable Intel® Quiet or Silent Boot options in the BIOS.
  Viewing the System Event Log (SEL)
    System Setup Utility > System Setup Screen > SEL Manager > View SEL Manager > File > Save As > Save as *.sel or *.txt.
  Windows* 2000 Advanced Server recognizes only 4 GB of memory
    The /PAE option must be enabled in the ARC path in the boot.ini file in order for Windows 2000* to recognize memory above 4.0GB (e.g. multi(0)disk(0)rdisk(0)partition(2)\WINNT="Windows 2000 Advanced Server" /PAE /basevideo /sos)

Compatibility
  Tested Chassis
    Intel® Server Chassis SR1300 (KCW)
  Tested Hardware and Operating Systems (PDF)

    | Tested Hardware and Operating System List (PDF)

    Note: PDF Files require Adobe Acrobat* Reader*

  Tested Memory (PDF)

    | Tested Memory List Report (PDF)

    Note: PDF Files require Adobe Acrobat* Reader*

  Tested Processors
    BX80532KE3200FSL7AE
    BX80532KE3200FUSL7BW
    BX80532KE3200E
    BX80532KE3200EU
    BX80532KE3200E
    BX80532KE3200EU
    BX80532KE3066E
    BX80532KE3066EU
    BX80532KE3066D
    80532KE083512
    BX80532KE3066DU
    BX80532KC3000D
    80532KC080512
    BX80532KE2080ESL7D5
    BX80532KE2080EUSL7DG
    BX80532KE2800DU
    BX80532KE2800D
    BX80532KC2800D
    80532KC072512
    BX80532KC2800DU
    BX80532KE2667DU
    BX80532KE2667D
    BX80532KE2667DU
    BX80532KE2667D
    BX80532KC2600D
    80532KC064512
    BX80532KC2600DU
    BX80532KE2400ESL7D4
    BX80532KE2400EUSL7DF
    BX80532KE2400DU
    BX80532KE2400D
    BX80532KC2400D
    80532KC056512
    BX80532KC2400DU
    BX80532KC2200D
    80532KC049512
    BX80532KC2200DU
    BX80532KE2000D
    BX80532KE2000DU
    BX80532KC2000D
    BX80532KC2000DU
    80532KC041512U
    BX80532KC1800D
    BX80532KC1800DU

Technical advisories
  AA679: Invalid firmware setting is present after using Intel® Server Setup Utilities (PDF)

    | Action Alert 679-1 (PDF)

    Note: PDF Files require Adobe Acrobat* Reader*

  TA627: BIOS Flash Chip Not Fully Write Protected (PDF)

    | TA_627 (PDF)

    Note: PDF Files require Adobe Acrobat* Reader*

  TA639: DDR 266 DIMM Slew Rate Observation Sighting (PDF)

    | TA_639 (PDF)

    Note: PDF Files require Adobe Acrobat* Reader*

  TA654: Hang at POST Code 12, 13, and 15 Or During Operating System Boot (PDF)

    | TA_654 (PDF)

    Note: PDF Files require Adobe Acrobat* Reader*

  TA656: 2 Gigabyte DIMM Support on the Intel® Server Board SE7501WV2 (PDF)

    | TA_656 (PDF)

    Note: PDF Files require Adobe Acrobat* Reader*

  TA667: Unexpected Reset Actions from Intel® Server Management (PDF)

    | TA_667 (PDF)

    Note: PDF Files require Adobe Acrobat* Reader*

  TA672: Power Cycling Issue (PDF)

    | TA_672 (PDF)

    Note: PDF Files require Adobe Acrobat* Reader*

  TA692: DC Power Supply for the Intel® Server Chassis SR2300 (PDF)

    | TA692-1 (PDF)

    Note: PDF Files require Adobe Acrobat* Reader*

  TA693: Updates Needed After Intel® Server Management Uninstall (PDF)

    | TA69301.PDF (PDF)

    Note: PDF Files require Adobe Acrobat* Reader*