RELEASE NOTES FOR SR870BH2 BMC RELEASE  0.30 - HPC - Feature Complete release
December 8 2004

- This release contains a fix for a Madison 6M processor errata which sometimes causes the 
  processor to come up in IO loop-back mode. This fix checks the SNC early for signs that 
  the processor is in this state, and if so, does an early, pre-emptive reset. 
- This BMC is required for supporting Madison9M processors, and that 
  this BMC is also backward compatible with previous versions of processors.i.e   
  BMC is compatible with BIOS using SNC address 18h or 00h (Madison9M).
- SDR15 should be used with this BMC version.

- This T2BMC29 is the Feature Complete HPC Release.

- Use 'FWUpdate' utility to flash BMC30 operational code into the BMC flash if current BMC 
  version is 15.  
- This version of BMC has been released with a working old BootCode version 15.
- All the user settings from current BMC will be restored when moved to new BMC28.
- Down revising the BMC may result in all settings being returned to factory defaults.
- Updating to this version from BMC 0.08 or lower requires Boot Block update.
  Use jumper J3A3 on the MB and switch FROM default 1-2 (Boot protected) TO 
  2-3 (Boot programmable) 
      
CHANGES SINCE PREVIOUS VERSION (VER 0.29)

- Tracker 39877 AC Lost SEL Events are reversed   


DEPENDENCIES 

* Same as in BMC29

KNOWN ISSUES 

* BMC v0.15 or earlier has the byte alignment problem in the private store area.

* Updating from BMC v0.15 or ealier may cause this BMC version to reload some previous default settings.  

Reference to NETFn Numbers
CHASSIS_REQUEST					0x00
BRIDGE_REQUEST					0x02
SNSR_EVENT_REQUEST				0x04
APP_REQUEST					0x06
FIRMWARE_REQUEST				0x08
STORAGE_REQUEST					0x0a
TRANSPORT_REQUEST				0x0c
INTEL_GENERAL_APP_REQUEST		0x30
INTEL_PLATFORM_SPECIFIC_REQUEST	0x32
INTEL_SOL_TMODE_REQUEST			0x34

LIST OF SUPPORTED APPLICATION COMMANDS (0x06)

Same as previous release.

LIST OF SUPPORTED SENSOR/EVENT COMMANDS	(0x04)

Same as previous release.

LIST OF SUPPORTED FIRMWARE TRANSFER COMMANDS (0x01)

Same as previous release.

LIST OF SUPPORTED CHASSIS COMMANDS

Same as previous release.

LIST OF SUPPORTED INTEL SPECIFIC COMMANDS (0x30)

0xA0 - 	RQ_CmdStagedPrepareForUpdate
0xA1 -	RQ_CmdStagedUpdateOpenArea
0xA2 - 	RQ_CmdStagedUpdateWriteArea
0xA3 -	RQ_CmdStagedUpdateCloseArea
0xA4 -	RQ_CmdStagedUpdateRegisterUpdate
0xA6 -	RQ_CmdStagedUpdateGetStatus
0xA7 -	RQ_CmdStagedUpdateGetCapabilities
0xA8 -	RQ_CmdStagedUpdateReadArea

Same as previous release.

LIST OF SUPPORTED BRIDGE COMMANDS

Same as previous release.

SUPPORTED SENSORS

Sensor#      	Sensor Name

Same as previous release. 

HEX IMAGE INFORMATION

OPCD CHECKSUM:  0xFB2F Start Address 0x00030000 ->  End Address  0x0007A33e	
BOOT CHECKSUM:	0x359A	Start Address 0x00000000 ->  End Address  0x00001CBE
PIA CHECKSUM:	0x1570	Start Address 0x00008000 ->  End Address  0x00008BCB

HEX CODE FILE:  T2BMC30.HEX   12/08/04  756,516 bytes

INFOBLOCK INFORMATION RETURNED BY: FWUPDATE T2BMC30.HEX /INFOBLOCK

OP CHECKSUM:			0x5208	(DIB ONLY)
BOOT CHECKSUM:			0xA28B	(DIB ONLY)
PIA HEADER CHECKSUM:		0x564A	(DIB ONLY)

REVISION INFORMATION RETURNED BY: FWUPDATE /FWVERSION

Op Code:		v00.30
Boot Code:		v00.15
PIA version: 	1
PIA instance: 	30

FILE VERSION TAGS
ACPIEC_VER			 	= 	v0.26	
ALERT_VER			 	= 	v0.54.5
BOOT_VER			 	= 	v0.19	
CHANNEL_VER			 	= 	v0.47.2  	
COMMON_VER			 	= 	v0.14.1  	
CPU_VER				 	= 	v0.51.4.1 	
DEBUG_VER			 	= 	v0.09	
DRIVERS_VER			 	= 	v0.14	
EMP_VER				 	= 	v0.62.6	
EXTERNAL_VER		 	= 	v0.64.2	
ICMB_VER			 	= 	v0.29.2	
IPMB_VER			 	= 	v0.25	
IPMI_VER			 	= 	v0.61.4.1
KCS_VER				 	= 	v0.39.1	
LAN_VER				 	= 	v0.52.2	
MEMALLOC_VER		 	= 	v0.42.2
MEMERR_VER			 	= 	v0.62.5	
MISC_VER			 	= 	v0.64.2.2
NVSTORE_VER			 	= 	v0.56.7
OS_VER				 	= 	v0.08	
PIA_VER				 	= 	v0.17	
PLATFORM_VER		 	= 	v0.30
POWER_VER			 	= 	v0.64.1	
SAHALEE_VER			 	= 	v0.39.1	
SCANNING_VER		 	= 	v0.51.2.1	
SENSORIPMI_VER		 	= 	v0.55.4
SENSORS_VER			 	= 	v0.35	
SESSION_VER			 	= 	v0.49.4	
USERINTF_VER		 	= 	v0.25	
UTILITIES_VER		 	= 	v0.41.2
TMODE_VER			 	= 	v0.10.1	
OPCODESTAGEDUPDATE_VER	= 	v0.12


TOOLS USED IN BUILD
getbmc.bat	version 1.5
gmake		Version 3.79.1
get 		v6.6.10
PVCS		version 6.6
ARM tools	version 2.51
WinZip		v7.0
Windiff

----------------------------------------------------------------------------

RELEASE NOTES FOR SR870BH2 BMC RELEASE  0.29 - HPC - Feature Complete release
December 7 2004

- This release contains a fix for a Madison 6M processor errata which sometimes causes the 
  processor to come up in IO loop-back mode. This fix checks the SNC early for signs that 
  the processor is in this state, and if so, does an early, pre-emptive reset. 
- This BMC is required for supporting Madison9M processors, and that 
  this BMC is also backward compatible with previous versions of processors.i.e   
  BMC is compatible with BIOS using SNC address 18h or 00h (Madison9M).
- SDR15 should be used with this BMC version.

- This T2BMC29 is the Feature Complete HPC Release.

- Use 'FWUpdate' utility to flash BMC29 operational code into the BMC flash if current BMC 
  version is 15.  
- This version of BMC has been released with a working old BootCode version 15.
- All the user settings from current BMC will be restored when moved to new BMC28.
- Down revising the BMC may result in all settings being returned to factory defaults.
- Updating to this version from BMC 0.08 or lower requires Boot Block update.
  Use jumper J3A3 on the MB and switch FROM default 1-2 (Boot protected) TO 
  2-3 (Boot programmable) 
      
CHANGES SINCE PREVIOUS VERSION (VER 0.28)

- Tracker 39747 POWER_SUPPLY sensors reproting a wrong "presence"  


DEPENDENCIES 

* Same as in BMC28

KNOWN ISSUES 

* BMC v0.15 or earlier has the byte alignment problem in the private store area.

* Updating from BMC v0.15 or ealier may cause this BMC version to reload some previous default settings.  

Reference to NETFn Numbers
CHASSIS_REQUEST					0x00
BRIDGE_REQUEST					0x02
SNSR_EVENT_REQUEST				0x04
APP_REQUEST					0x06
FIRMWARE_REQUEST				0x08
STORAGE_REQUEST					0x0a
TRANSPORT_REQUEST				0x0c
INTEL_GENERAL_APP_REQUEST		0x30
INTEL_PLATFORM_SPECIFIC_REQUEST	0x32
INTEL_SOL_TMODE_REQUEST			0x34

LIST OF SUPPORTED APPLICATION COMMANDS (0x06)

Same as previous release.

LIST OF SUPPORTED SENSOR/EVENT COMMANDS	(0x04)

Same as previous release.

LIST OF SUPPORTED FIRMWARE TRANSFER COMMANDS (0x01)

Same as previous release.

LIST OF SUPPORTED CHASSIS COMMANDS

Same as previous release.

LIST OF SUPPORTED INTEL SPECIFIC COMMANDS (0x30)

0xA0 - 	RQ_CmdStagedPrepareForUpdate
0xA1 -	RQ_CmdStagedUpdateOpenArea
0xA2 - 	RQ_CmdStagedUpdateWriteArea
0xA3 -	RQ_CmdStagedUpdateCloseArea
0xA4 -	RQ_CmdStagedUpdateRegisterUpdate
0xA6 -	RQ_CmdStagedUpdateGetStatus
0xA7 -	RQ_CmdStagedUpdateGetCapabilities
0xA8 -	RQ_CmdStagedUpdateReadArea

Same as previous release.

LIST OF SUPPORTED BRIDGE COMMANDS

Same as previous release.

SUPPORTED SENSORS

Sensor#      	Sensor Name

Same as previous release. 

HEX IMAGE INFORMATION

OPCD CHECKSUM:  0x8605 Start Address 0x00030000 ->  End Address  0x0007A336	
BOOT CHECKSUM:	0x359A	Start Address 0x00000000 ->  End Address  0x00001CBE
PIA CHECKSUM:	0x1570	Start Address 0x00008000 ->  End Address  0x00008BCB

HEX CODE FILE:  T2BMC29.HEX   12/07/04  756,500 bytes

INFOBLOCK INFORMATION RETURNED BY: FWUPDATE T2BMC29.HEX /INFOBLOCK

OP CHECKSUM:			0x4916	(DIB ONLY)
BOOT CHECKSUM:			0x9E8A	(DIB ONLY)
PIA HEADER CHECKSUM:		0x5D4A	(DIB ONLY)

REVISION INFORMATION RETURNED BY: FWUPDATE /FWVERSION

Op Code:		v00.29
Boot Code:		v00.15
PIA version: 	1
PIA instance: 	29

FILE VERSION TAGS
ACPIEC_VER			 	= 	v0.26	
ALERT_VER			 	= 	v0.54.5
BOOT_VER			 	= 	v0.19	
CHANNEL_VER			 	= 	v0.47.2  	
COMMON_VER			 	= 	v0.14.1  	
CPU_VER				 	= 	v0.51.4.1 	
DEBUG_VER			 	= 	v0.09	
DRIVERS_VER			 	= 	v0.14	
EMP_VER				 	= 	v0.62.6	
EXTERNAL_VER		 	= 	v0.64.2	
ICMB_VER			 	= 	v0.29.2	
IPMB_VER			 	= 	v0.25	
IPMI_VER			 	= 	v0.61.4.1
KCS_VER				 	= 	v0.39.1	
LAN_VER				 	= 	v0.52.2	
MEMALLOC_VER		 	= 	v0.42.2
MEMERR_VER			 	= 	v0.62.5	
MISC_VER			 	= 	v0.64.2.2
NVSTORE_VER			 	= 	v0.56.7
OS_VER				 	= 	v0.08	
PIA_VER				 	= 	v0.17	
PLATFORM_VER		 	= 	v0.29
POWER_VER			 	= 	v0.64.1	
SAHALEE_VER			 	= 	v0.39.1	
SCANNING_VER		 	= 	v0.51.2.1	
SENSORIPMI_VER		 	= 	v0.55.4
SENSORS_VER			 	= 	v0.35	
SESSION_VER			 	= 	v0.49.4	
USERINTF_VER		 	= 	v0.25	
UTILITIES_VER		 	= 	v0.41.2
TMODE_VER			 	= 	v0.10.1	
OPCODESTAGEDUPDATE_VER	= 	v0.12


TOOLS USED IN BUILD
getbmc.bat	version 1.5
gmake		Version 3.79.1
get 		v6.6.10
PVCS		version 6.6
ARM tools	version 2.51
WinZip		v7.0
Windiff

----------------------------------------------------------------------------
RELEASE NOTES FOR SR870BH2 BMC RELEASE  0.28 - HPC - Feature Complete release
December 2 2004

- This release contains a fix for a Madison 6M processor errata which sometimes causes the 
  processor to come up in IO loop-back mode. This fix checks the SNC early for signs that 
  the processor is in this state, and if so, does an early, pre-emptive reset. 
- This BMC is required for supporting Madison9M processors, and that 
  this BMC is also backward compatible with previous versions of processors.i.e   
  BMC is compatible with BIOS using SNC address 18h or 00h (Madison9M).
- SDR15 should be used with this BMC version.

- This T2BMC28 is the Feature Complete HPC Release.

- Use 'FWUpdate' utility to flash BMC28 operational code into the BMC flash if current BMC 
  version is 15.  
- This version of BMC has been released with a working old BootCode version 15.
- All the user settings from current BMC will be restored when moved to new BMC28.
- Down revising the BMC may result in all settings being returned to factory defaults.
- Updating to this version from BMC 0.08 or lower requires Boot Block update.
  Use jumper J3A3 on the MB and switch FROM default 1-2 (Boot protected) TO 
  2-3 (Boot programmable) 
      
CHANGES SINCE PREVIOUS VERSION (VER 0.27)
- This release contains a fix for a Madison 6M processor errata which sometimes causes the 
  processor to come up in IO loop-back mode. This fix checks the SNC early for signs that 
  the processor is in this state, and if so, does an early, pre-emptive reset. 


DEPENDENCIES 

* Same as in BMC27

KNOWN ISSUES 

* BMC v0.15 or earlier has the byte alignment problem in the private store area.

* Updating from BMC v0.15 or ealier may cause this BMC version to reload some previous default settings.  

Reference to NETFn Numbers
CHASSIS_REQUEST					0x00
BRIDGE_REQUEST					0x02
SNSR_EVENT_REQUEST				0x04
APP_REQUEST					0x06
FIRMWARE_REQUEST				0x08
STORAGE_REQUEST					0x0a
TRANSPORT_REQUEST				0x0c
INTEL_GENERAL_APP_REQUEST		0x30
INTEL_PLATFORM_SPECIFIC_REQUEST	0x32
INTEL_SOL_TMODE_REQUEST			0x34

LIST OF SUPPORTED APPLICATION COMMANDS (0x06)

Same as previous release.

LIST OF SUPPORTED SENSOR/EVENT COMMANDS	(0x04)

Same as previous release.

LIST OF SUPPORTED FIRMWARE TRANSFER COMMANDS (0x01)

Same as previous release.

LIST OF SUPPORTED CHASSIS COMMANDS

Same as previous release.

LIST OF SUPPORTED INTEL SPECIFIC COMMANDS (0x30)

0xA0 - 	RQ_CmdStagedPrepareForUpdate
0xA1 -	RQ_CmdStagedUpdateOpenArea
0xA2 - 	RQ_CmdStagedUpdateWriteArea
0xA3 -	RQ_CmdStagedUpdateCloseArea
0xA4 -	RQ_CmdStagedUpdateRegisterUpdate
0xA6 -	RQ_CmdStagedUpdateGetStatus
0xA7 -	RQ_CmdStagedUpdateGetCapabilities
0xA8 -	RQ_CmdStagedUpdateReadArea

Same as previous release.

LIST OF SUPPORTED BRIDGE COMMANDS

Same as previous release.

SUPPORTED SENSORS

Sensor#      	Sensor Name

Same as previous release. 

HEX IMAGE INFORMATION

OPCD CHECKSUM:  0x1F55 Start Address 0x00030000 ->  End Address  0x0007A2DE	
BOOT CHECKSUM:	0x359A	Start Address 0x00000000 ->  End Address  0x00001CBE
PIA CHECKSUM:	0x1570	Start Address 0x00008000 ->  End Address  0x00008BCB

HEX CODE FILE:  T2BMC28.HEX   12/02/04  756,285 bytes

INFOBLOCK INFORMATION RETURNED BY: FWUPDATE T2BMC28.HEX /INFOBLOCK

OP CHECKSUM:			0x4870	(DIB ONLY)
BOOT CHECKSUM:			0x9C90	(DIB ONLY)
PIA HEADER CHECKSUM:		0x5E4A	(DIB ONLY)

REVISION INFORMATION RETURNED BY: FWUPDATE /FWVERSION

Op Code:		v00.28
Boot Code:		v00.15
PIA version: 	1
PIA instance: 	28

FILE VERSION TAGS
ACPIEC_VER			 	= 	v0.26	
ALERT_VER			 	= 	v0.54.5
BOOT_VER			 	= 	v0.19	
CHANNEL_VER			 	= 	v0.47.2  	
COMMON_VER			 	= 	v0.14.1  	
CPU_VER				 	= 	v0.51.4.1 	
DEBUG_VER			 	= 	v0.09	
DRIVERS_VER			 	= 	v0.14	
EMP_VER				 	= 	v0.62.6	
EXTERNAL_VER		 	= 	v0.64.2	
ICMB_VER			 	= 	v0.29.2	
IPMB_VER			 	= 	v0.25	
IPMI_VER			 	= 	v0.61.4.1
KCS_VER				 	= 	v0.39.1	
LAN_VER				 	= 	v0.52.2	
MEMALLOC_VER		 	= 	v0.42.2
MEMERR_VER			 	= 	v0.62.5	
MISC_VER			 	= 	v0.64.2.2
NVSTORE_VER			 	= 	v0.56.7
OS_VER				 	= 	v0.08	
PIA_VER				 	= 	v0.17	
PLATFORM_VER		 	= 	v0.28
POWER_VER			 	= 	v0.64.1	
SAHALEE_VER			 	= 	v0.39.1	
SCANNING_VER		 	= 	v0.51.2.1	
SENSORIPMI_VER		 	= 	v0.55.4
SENSORS_VER			 	= 	v0.35	
SESSION_VER			 	= 	v0.49.4	
USERINTF_VER		 	= 	v0.25	
UTILITIES_VER		 	= 	v0.41.2
TMODE_VER			 	= 	v0.10.1	
OPCODESTAGEDUPDATE_VER	= 	v0.12


TOOLS USED IN BUILD
getbmc.bat	version 1.5
gmake		Version 3.79.1
get 		v6.6.10
PVCS		version 6.6
ARM tools	version 2.51
WinZip		v7.0
Windiff

----------------------------------------------------------------------------

RELEASE NOTES FOR SR870BH2 BMC RELEASE  0.27 - HPC - Feature Complete release
September 15, 2004

- This BMC is required for supporting Madison9M processors, and that 
  this BMC is also backward compatible with previous versions of processors.i.e   
  BMC is compatible with BIOS using SNC address 18h or 00h (Madison9M).
- SDR15 should be used with this BMC version.

- This T2BMC27 is the Feature Complete HPC Release.

- Use 'FWUpdate' utility to flash BMC27 operational code into the BMC flash if current BMC 
  version is 15.  
- This version of BMC has been released with a working old BootCode version 15.
- All the user settings from current BMC will be restored when moved to new BMC27.
- Down revising the BMC may result in all settings being returned to factory defaults.
- Updating to this version from BMC 0.08 or lower requires Boot Block update.
  Use jumper J3A3 on the MB and switch FROM default 1-2 (Boot protected) TO 
  2-3 (Boot programmable) 
      
CHANGES SINCE PREVIOUS VERSION (VER 0.24)
* IPMI 1.5 core bug fixes in this release.  
none

* Platform Specific bug fixes in this release.  
Tracker 37894: Cannot recover "failed BIST" processors with Mad6M PR6.2 or Mad9M PR2.0 
Tracker 37674: Inconsistent FP status LED behavior relating to power state 
Tracker 38017: Incorrect behavior of System status LED during PSU and AC events  



DEPENDENCIES 

* Same as in BMC26

KNOWN ISSUES 

* BMC v0.15 or earlier has the byte alignment problem in the private store area.

* Updating from BMC v0.15 or ealier may cause this BMC version to reload some previous default settings.  

Reference to NETFn Numbers
CHASSIS_REQUEST					0x00
BRIDGE_REQUEST					0x02
SNSR_EVENT_REQUEST				0x04
APP_REQUEST					0x06
FIRMWARE_REQUEST				0x08
STORAGE_REQUEST					0x0a
TRANSPORT_REQUEST				0x0c
INTEL_GENERAL_APP_REQUEST		0x30
INTEL_PLATFORM_SPECIFIC_REQUEST	0x32
INTEL_SOL_TMODE_REQUEST			0x34

LIST OF SUPPORTED APPLICATION COMMANDS (0x06)

Same as previous release.

LIST OF SUPPORTED SENSOR/EVENT COMMANDS	(0x04)

Same as previous release.

LIST OF SUPPORTED FIRMWARE TRANSFER COMMANDS (0x01)

Same as previous release.

LIST OF SUPPORTED CHASSIS COMMANDS

Same as previous release.

LIST OF SUPPORTED INTEL SPECIFIC COMMANDS (0x30)

0xA0 - 	RQ_CmdStagedPrepareForUpdate
0xA1 -	RQ_CmdStagedUpdateOpenArea
0xA2 - 	RQ_CmdStagedUpdateWriteArea
0xA3 -	RQ_CmdStagedUpdateCloseArea
0xA4 -	RQ_CmdStagedUpdateRegisterUpdate
0xA6 -	RQ_CmdStagedUpdateGetStatus
0xA7 -	RQ_CmdStagedUpdateGetCapabilities
0xA8 -	RQ_CmdStagedUpdateReadArea

Same as previous release.

LIST OF SUPPORTED BRIDGE COMMANDS

Same as previous release.

SUPPORTED SENSORS

Sensor#      	Sensor Name

Same as previous release. 

HEX IMAGE INFORMATION

OPCD CHECKSUM:  0xD716	Start Address 0x00030000 ->  End Address  0x0007A2CE	
BOOT CHECKSUM:	0x359A	Start Address 0x00000000 ->  End Address  0x00001CBE
PIA CHECKSUM:	0x1570	Start Address 0x00008000 ->  End Address  0x00008BCB

HEX CODE FILE:  T2BMC27.HEX   09/15/04  756,253 bytes

INFOBLOCK INFORMATION RETURNED BY: FWUPDATE T2BMC27.HEX /INFOBLOCK

OP CHECKSUM:			0x4D5E	(DIB ONLY)
BOOT CHECKSUM:			0x9B6B	(DIB ONLY)
PIA HEADER CHECKSUM:	0x5F4A	(DIB ONLY)

REVISION INFORMATION RETURNED BY: FWUPDATE /FWVERSION

Op Code:		v00.27
Boot Code:		v00.15
PIA version: 	1
PIA instance: 	27

FILE VERSION TAGS
ACPIEC_VER			 	= 	v0.26	
ALERT_VER			 	= 	v0.54.5
BOOT_VER			 	= 	v0.19	
CHANNEL_VER			 	= 	v0.47.2  	
COMMON_VER			 	= 	v0.14.1  	
CPU_VER				 	= 	v0.51.4.1 	
DEBUG_VER			 	= 	v0.09	
DRIVERS_VER			 	= 	v0.14	
EMP_VER				 	= 	v0.62.6	
EXTERNAL_VER		 	= 	v0.64.2	
ICMB_VER			 	= 	v0.29.2	
IPMB_VER			 	= 	v0.25	
IPMI_VER			 	= 	v0.61.4.1
KCS_VER				 	= 	v0.39.1	
LAN_VER				 	= 	v0.52.2	
MEMALLOC_VER		 	= 	v0.42.2
MEMERR_VER			 	= 	v0.62.5	
MISC_VER			 	= 	v0.64.2.2
NVSTORE_VER			 	= 	v0.56.7
OS_VER				 	= 	v0.08	
PIA_VER				 	= 	v0.17	
PLATFORM_VER		 	= 	v0.27
POWER_VER			 	= 	v0.64.1	
SAHALEE_VER			 	= 	v0.39.1	
SCANNING_VER		 	= 	v0.51.2.1	
SENSORIPMI_VER		 	= 	v0.55.4
SENSORS_VER			 	= 	v0.35	
SESSION_VER			 	= 	v0.49.4	
USERINTF_VER		 	= 	v0.25	
UTILITIES_VER		 	= 	v0.41.2
TMODE_VER			 	= 	v0.10.1	
OPCODESTAGEDUPDATE_VER	= 	v0.12


TOOLS USED IN BUILD
getbmc.bat	version 1.5
gmake		Version 3.79.1
get 		v6.6.10
PVCS		version 6.6
ARM tools	version 2.51
WinZip		v7.0
Windiff

----------------------------------------------------------------------------

RELEASE NOTES FOR SR870BH2 BMC RELEASE  0.26 - HPC - Feature Complete release
June 09, 2004

- This T2BMC26 is the Feature Complete HPC Release.

- Use 'FWUpdate' utility to flash BMC26 operational code into the BMC flash if current BMC 
  version is 15.  
- This version of BMC has been released with a working old BootCode version 15.
- All the user settings from current BMC will be restored when moved to new BMC26.
- Down revising the BMC may result in all settings being returned to factory defaults.
- Updating to this version from BMC 0.08 or lower requires Boot Block update.
  Use jumper J3A3 on the MB and switch FROM default 1-2 (Boot protected) TO 
  2-3 (Boot programmable) 
- SDR13 or later should be used with this BMC version.
      
CHANGES SINCE PREVIOUS VERSION (VER 0.24)
* IPMI 1.5 core bug fixes in this release.  
none

* Platform Specific bug fixes in this release.  
Tracker 35379: Register Update allows various 'reserved bits' to be sent 
Tracker 37161: Goblin SEL locks up at 7% when trying to read it through the SMU 



DEPENDENCIES 

* Same as in BMC25

KNOWN ISSUES 

* BMC v0.15 or earlier has the byte alignment problem in the private store area.

* Updating from BMC v0.15 or ealier may cause this BMC version to reload some previous default settings.  

Reference to NETFn Numbers
CHASSIS_REQUEST					0x00
BRIDGE_REQUEST					0x02
SNSR_EVENT_REQUEST				0x04
APP_REQUEST					0x06
FIRMWARE_REQUEST				0x08
STORAGE_REQUEST					0x0a
TRANSPORT_REQUEST				0x0c
INTEL_GENERAL_APP_REQUEST		0x30
INTEL_PLATFORM_SPECIFIC_REQUEST	0x32
INTEL_SOL_TMODE_REQUEST			0x34

LIST OF SUPPORTED APPLICATION COMMANDS (0x06)

Same as previous release.

LIST OF SUPPORTED SENSOR/EVENT COMMANDS	(0x04)

Same as previous release.

LIST OF SUPPORTED FIRMWARE TRANSFER COMMANDS (0x01)

Same as previous release.

LIST OF SUPPORTED CHASSIS COMMANDS

Same as previous release.

LIST OF SUPPORTED INTEL SPECIFIC COMMANDS (0x30)

0xA0 - 	RQ_CmdStagedPrepareForUpdate
0xA1 -	RQ_CmdStagedUpdateOpenArea
0xA2 - 	RQ_CmdStagedUpdateWriteArea
0xA3 -	RQ_CmdStagedUpdateCloseArea
0xA4 -	RQ_CmdStagedUpdateRegisterUpdate
0xA6 -	RQ_CmdStagedUpdateGetStatus
0xA7 -	RQ_CmdStagedUpdateGetCapabilities
0xA8 -	RQ_CmdStagedUpdateReadArea

Same as previous release.

LIST OF SUPPORTED BRIDGE COMMANDS

Same as previous release.

SUPPORTED SENSORS

Sensor#      	Sensor Name

Same as previous release. 

HEX IMAGE INFORMATION

OPCD CHECKSUM:  0xB8AB	Start Address 0x00030000 ->  End Address  0x0007A1DA	
BOOT CHECKSUM:	0x359A	Start Address 0x00000000 ->  End Address  0x00001CBE
PIA CHECKSUM:	0x28D8	Start Address 0x00008000 ->  End Address  0x00008BBF

HEX CODE FILE:  T2BMC26.HEX   06/09/04  755,584 bytes

INFOBLOCK INFORMATION RETURNED BY: FWUPDATE T2BMC26.HEX /INFOBLOCK

OP CHECKSUM:			0x3467	(DIB ONLY)
BOOT CHECKSUM:			0x8E7D	(DIB ONLY)
PIA HEADER CHECKSUM:		0x4D2A	(DIB ONLY)

REVISION INFORMATION RETURNED BY: FWUPDATE /FWVERSION

Op Code:		v00.26
Boot Code:		v00.15
PIA version: 	1
PIA instance: 	26

FILE VERSION TAGS
ACPIEC_VER			 	= 	v0.26	
ALERT_VER			 	= 	v0.54.5
BOOT_VER			 	= 	v0.19	
CHANNEL_VER			 	= 	v0.47.2  	
COMMON_VER			 	= 	v0.14.1  	
CPU_VER				 	= 	v0.51.4 	
DEBUG_VER			 	= 	v0.09	
DRIVERS_VER			 	= 	v0.14	
EMP_VER				 	= 	v0.62.6	
EXTERNAL_VER		 		= 	v0.64.2	
ICMB_VER			 	= 	v0.29.2	
IPMB_VER			 	= 	v0.25	
IPMI_VER			 	= 	v0.61.4.1
KCS_VER				 	= 	v0.39.1	
LAN_VER				 	= 	v0.52.2	
MEMALLOC_VER		 		= 	v0.42.2
MEMERR_VER			 	= 	v0.62.5	
MISC_VER			 	= 	v0.64.2.2
NVSTORE_VER			 	= 	v0.56.7
OS_VER				 	= 	v0.08	
PIA_VER				 	= 	v0.17	
PLATFORM_VER		 		= 	v0.26
POWER_VER			 	= 	v0.64.1	
SAHALEE_VER			 	= 	v0.39.1	
SCANNING_VER		 		= 	v0.51.2	
SENSORIPMI_VER		 		= 	v0.55.4
SENSORS_VER			 	= 	v0.35	
SESSION_VER			 	= 	v0.49.4	
USERINTF_VER		 		= 	v0.25	
UTILITIES_VER		 		= 	v0.41.2
TMODE_VER			 	= 	v0.10.1	
OPCODESTAGEDUPDATE_VER			= 	v0.12


TOOLS USED IN BUILD
getbmc.bat	version 1.5
gmake		Version 3.79.1
get 		v6.6.10
PVCS		version 6.6
ARM tools	version 2.51
WinZip		v7.0
Windiff

----------------------------------------------------------------------------

RELEASE NOTES FOR SR870BH2 BMC RELEASE  0.25 - HPC - Feature Complete release
February 20, 2004

- This T2BMC25 is the Feature Complete HPC Release.

- Use 'FWUpdate' utility to flash BMC25 operational code into the BMC flash if current BMC 
  version is 15.  
- This version of BMC has been released with a working old BootCode version 15.
- All the user settings from current BMC will be restored when moved to new BMC25.
- Down revising the BMC may result in all settings being returned to factory defaults.
- Updating to this version from BMC 0.08 or lower requires Boot Block update.
  Use jumper J3A3 on the MB and switch FROM default 1-2 (Boot protected) TO 
  2-3 (Boot programmable) 
- SDR13 or later should be used with this BMC version.
      
CHANGES SINCE PREVIOUS VERSION (VER 0.24)
* IPMI 1.5 core bug fixes in this release.  
none

* Platform Specific bug fixes in this release.  
36133 Byte alignment problem in the private store data (Sev2)


DEPENDENCIES 

* Same as in BMC24

KNOWN ISSUES 

* BMC v0.15 or earlier has the byte alignment problem in the private store area.

* Updating from BMC v0.15 or ealier may cause this BMC version to reload some previous default settings.  

Reference to NETFn Numbers
CHASSIS_REQUEST					0x00
BRIDGE_REQUEST					0x02
SNSR_EVENT_REQUEST				0x04
APP_REQUEST					0x06
FIRMWARE_REQUEST				0x08
STORAGE_REQUEST					0x0a
TRANSPORT_REQUEST				0x0c
INTEL_GENERAL_APP_REQUEST		0x30
INTEL_PLATFORM_SPECIFIC_REQUEST	0x32
INTEL_SOL_TMODE_REQUEST			0x34

LIST OF SUPPORTED APPLICATION COMMANDS (0x06)

Same as previous release.

LIST OF SUPPORTED SENSOR/EVENT COMMANDS	(0x04)

Same as previous release.

LIST OF SUPPORTED FIRMWARE TRANSFER COMMANDS (0x01)

Same as previous release.

LIST OF SUPPORTED CHASSIS COMMANDS

Same as previous release.

LIST OF SUPPORTED INTEL SPECIFIC COMMANDS (0x30)

0xA0 - 	RQ_CmdStagedPrepareForUpdate
0xA1 -	RQ_CmdStagedUpdateOpenArea
0xA2 - 	RQ_CmdStagedUpdateWriteArea
0xA3 -	RQ_CmdStagedUpdateCloseArea
0xA4 -	RQ_CmdStagedUpdateRegisterUpdate
0xA6 -	RQ_CmdStagedUpdateGetStatus
0xA7 -	RQ_CmdStagedUpdateGetCapabilities
0xA8 -	RQ_CmdStagedUpdateReadArea

Same as previous release.

LIST OF SUPPORTED BRIDGE COMMANDS

Same as previous release.

SUPPORTED SENSORS

Sensor#      	Sensor Name

Same as previous release. 

HEX IMAGE INFORMATION

OPCD CHECKSUM:  0xBFC9	Start Address 0x00030000 ->  End Address  0x0007A162	
BOOT CHECKSUM:	0x359A	Start Address 0x00000000 ->  End Address  0x00001CBE
PIA CHECKSUM:	0x28D8	Start Address 0x00008000 ->  End Address  0x00008BBF

HEX CODE FILE:  T2BMC25.HEX   02/20/04  755,305 bytes

INFOBLOCK INFORMATION RETURNED BY: FWUPDATE T2BMC25.HEX /INFOBLOCK

OP CHECKSUM:			0x54ED	(DIB ONLY)
BOOT CHECKSUM:			0xA08C	(DIB ONLY)
PIA HEADER CHECKSUM:		0x4E2A	(DIB ONLY)

REVISION INFORMATION RETURNED BY: FWUPDATE /FWVERSION

Op Code:		v00.25
Boot Code:		v00.15
PIA version: 	1
PIA instance: 	25

FILE VERSION TAGS
ACPIEC_VER			 	= 	v0.26	
ALERT_VER			 	= 	v0.54.5
BOOT_VER			 	= 	v0.19	
CHANNEL_VER			 	= 	v0.47.2  	
COMMON_VER			 	= 	v0.14.1  	
CPU_VER				 	= 	v0.51.4 	
DEBUG_VER			 	= 	v0.09	
DRIVERS_VER			 	= 	v0.14	
EMP_VER				 	= 	v0.62.6	
EXTERNAL_VER		 	= 	v0.64.2	
ICMB_VER			 	= 	v0.29.2	
IPMB_VER			 	= 	v0.25	
IPMI_VER			 	= 	v0.61.4
KCS_VER				 	= 	v0.39.1	
LAN_VER				 	= 	v0.52.2	
MEMALLOC_VER		 	= 	v0.42.2
MEMERR_VER			 	= 	v0.62.5	
MISC_VER			 	= 	v0.64.2.2
NVSTORE_VER			 	= 	v0.56.6
OS_VER				 	= 	v0.08	
PIA_VER				 	= 	v0.17	
PLATFORM_VER		 	= 	v0.25
POWER_VER			 	= 	v0.64.1	
SAHALEE_VER			 	= 	v0.39.1	
SCANNING_VER		 	= 	v0.51.2	
SENSORIPMI_VER		 	= 	v0.55.4
SENSORS_VER			 	= 	v0.35	
SESSION_VER			 	= 	v0.49.4	
USERINTF_VER		 	= 	v0.25	
UTILITIES_VER		 	= 	v0.41.2
TMODE_VER			 	= 	v0.10.1	
OPCODESTAGEDUPDATE_VER	= 	v0.11

TOOLS USED IN BUILD
getbmc.bat	version 1.5
gmake		Version 3.79.1
get 		v6.6.10
PVCS		version 6.6
ARM tools	version 2.51
WinZip		v7.0
Windiff

----------------------------------------------------------------------------


RELEASE NOTES FOR SR870BH2 BMC RELEASE  0.24 - HPC - Feature Complete release
February 10, 2004

- This T2BMC24 is the Feature Complete HPC Release.

- Use 'FWUpdate' utility to flash BMC23 operational code into the BMC flash if current BMC 
  version is 15.  If upgrading from BMC22 to BMC23 you may use OFU utility.
- Subsequent updates of Operational Firmware, PIA, and SDR can be staged and updated using BMC23.
- This version of BMC has been released with a working old BootCode version 15.
- All the user settings from current BMC will be restored when moved to new BMC23.
- Down revising the BMC may result in all settings being returned to factory defaults.
- Updating to this version from BMC 0.08 or lower requires Boot Block update.
  Use jumper J3A3 on the MB and switch FROM default 1-2 (Boot protected) TO 
  2-3 (Boot programmable) 
- SDR13 should be used with this BMC version.
      
CHANGES SINCE PREVIOUS VERSION (VER 0.23)
* IPMI 1.5 core bug fixes in this release.  
none

* Platform Specific bug fixes in this release.  
35565 Increase mandatory off-time to 20 seconds  (BMC Change Request)) (Sev2)
35740 SDR load fail with FRUSDR utility (Sev1)


DEPENDENCIES 

* Same as in BMC23

KNOWN ISSUES 

* Updating from BMC v0.13 or ealier will result in the loss of some PEF filter settings 
  in private store.


- There is a byte alignment problem in the user configuration data area, which will result in the loss
of some user configuration settings after updating to this BMC version.


Reference to NETFn Numbers
CHASSIS_REQUEST					0x00
BRIDGE_REQUEST					0x02
SNSR_EVENT_REQUEST				0x04
APP_REQUEST					0x06
FIRMWARE_REQUEST				0x08
STORAGE_REQUEST					0x0a
TRANSPORT_REQUEST				0x0c
INTEL_GENERAL_APP_REQUEST		0x30
INTEL_PLATFORM_SPECIFIC_REQUEST	0x32
INTEL_SOL_TMODE_REQUEST			0x34

LIST OF SUPPORTED APPLICATION COMMANDS (0x06)

Same as previous release.

LIST OF SUPPORTED SENSOR/EVENT COMMANDS	(0x04)

Same as previous release.

LIST OF SUPPORTED FIRMWARE TRANSFER COMMANDS (0x01)

Same as previous release.

LIST OF SUPPORTED CHASSIS COMMANDS

Same as previous release.

LIST OF SUPPORTED INTEL SPECIFIC COMMANDS (0x30)

0xA0 - 	RQ_CmdStagedPrepareForUpdate
0xA1 -	RQ_CmdStagedUpdateOpenArea
0xA2 - 	RQ_CmdStagedUpdateWriteArea
0xA3 -	RQ_CmdStagedUpdateCloseArea
0xA4 -	RQ_CmdStagedUpdateRegisterUpdate
0xA6 -	RQ_CmdStagedUpdateGetStatus
0xA7 -	RQ_CmdStagedUpdateGetCapabilities
0xA8 -	RQ_CmdStagedUpdateReadArea

Same as previous release.

LIST OF SUPPORTED BRIDGE COMMANDS

Same as previous release.

SUPPORTED SENSORS

Sensor#      	Sensor Name

Same as previous release. 

HEX IMAGE INFORMATION

OPCD CHECKSUM:  0xE5D6	Start Address 0x00030000 ->  End Address  0x0007A14E	
BOOT CHECKSUM:	0x359A	Start Address 0x00000000 ->  End Address  0x00001CBE
PIA CHECKSUM:	0x28D8 	Start Address 0x00008000 ->  End Address  0x00008BBF

HEX CODE FILE:  T2BMC24.HEX   02/02/04  755,252 bytes

INFOBLOCK INFORMATION RETURNED BY: FWUPDATE T2BMC23.HEX /INFOBLOCK

OP CHECKSUM:			0x4A01	(DIB ONLY)
BOOT CHECKSUM:			0xA08A	(DIB ONLY)
PIA HEADER CHECKSUM:		0x4F2A	(DIB ONLY)

REVISION INFORMATION RETURNED BY: FWUPDATE /FWVERSION

Op Code:		v00.24
Boot Code:		v00.15
PIA version: 	1
PIA instance: 	24

FILE VERSION TAGS
ACPIEC_VER			 	= 	v0.26	
ALERT_VER			 	= 	v0.54.5
BOOT_VER			 	= 	v0.19	
CHANNEL_VER			 	= 	v0.47.2  	
COMMON_VER			 	= 	v0.14.1  	
CPU_VER				 	= 	v0.51.4 	
DEBUG_VER			 	= 	v0.09	
DRIVERS_VER			 	= 	v0.14	
EMP_VER				 	= 	v0.62.6	
EXTERNAL_VER		 	= 	v0.64.2	
ICMB_VER			 	= 	v0.29.2	
IPMB_VER			 	= 	v0.25	
IPMI_VER			 	= 	v0.61.4
KCS_VER				 	= 	v0.39.1	
LAN_VER				 	= 	v0.52.2	
MEMALLOC_VER		 	= 	v0.42.2
MEMERR_VER			 	= 	v0.62.5	
MISC_VER			 	= 	v0.64.2.2
NVSTORE_VER			 	= 	v0.56.5
OS_VER				 	= 	v0.08	
PIA_VER				 	= 	v0.17	
PLATFORM_VER		 	= 	v0.24
POWER_VER			 	= 	v0.64.1	
SAHALEE_VER			 	= 	v0.39.1	
SCANNING_VER		 	= 	v0.51.2	
SENSORIPMI_VER		 	= 	v0.55.4
SENSORS_VER			 	= 	v0.35	
SESSION_VER			 	= 	v0.49.4	
USERINTF_VER		 	= 	v0.25	
UTILITIES_VER		 	= 	v0.41.2
TMODE_VER			 	= 	v0.10.1	
OPCODESTAGEDUPDATE_VER	= 	v0.10

TOOLS USED IN BUILD
getbmc.bat	version 1.5
gmake		Version 3.79.1
get 		v6.6.10
PVCS		version 6.6
ARM tools	version 2.51
WinZip		v7.0
Windiff

----------------------------------------------------------------------------


RELEASE NOTES FOR SR870BH2 BMC RELEASE  0.23 - HPC - Feature Complete release.
January 09, 2004

- This T2BMC23 is the Feature Complete HPC Release.

- Use 'FWUpdate' utility to flash BMC23 operational code into the BMC flash if current BMC 
  version is 15.  If upgrading from BMC22 to BMC23 you may use OFU utility.
- Subsequent updates of Operational Firmware, PIA, and SDR can be staged and updated using BMC23.
- This version of BMC has been released with a working old BootCode version 15.
- All the user settings from current BMC will be restored when moved to new BMC23.
- Down revising the BMC may result in all settings being returned to factory defaults.
- Updating to this version from BMC 0.08 or lower requires Boot Block update.
  Use jumper J3A3 on the MB and switch FROM default 1-2 (Boot protected) TO 
  2-3 (Boot programmable) 
- SDR13 should be used with this BMC version.
      
CHANGES SINCE PREVIOUS VERSION (VER 0.22)
* IPMI 1.5 core bug fixes in this release.  
none

* Platform Specific bug fixes in this release.  
"35520"	"Sev2"	"Reset button action during OFU FW update creates problems"

DEPENDENCIES 

* Same as in BMC22

KNOWN ISSUES 

* Updating from BMC v0.13 or ealier will result in the loss of some PEF filter settings 
  in private store.

Reference to NETFn Numbers
CHASSIS_REQUEST					0x00
BRIDGE_REQUEST					0x02
SNSR_EVENT_REQUEST				0x04
APP_REQUEST						0x06
FIRMWARE_REQUEST				0x08
STORAGE_REQUEST					0x0a
TRANSPORT_REQUEST				0x0c
INTEL_GENERAL_APP_REQUEST		0x30
INTEL_PLATFORM_SPECIFIC_REQUEST	0x32
INTEL_SOL_TMODE_REQUEST			0x34

LIST OF SUPPORTED APPLICATION COMMANDS (0x06)

Same as previous release.

LIST OF SUPPORTED SENSOR/EVENT COMMANDS	(0x04)

Same as previous release.

LIST OF SUPPORTED FIRMWARE TRANSFER COMMANDS (0x01)

Same as previous release.

LIST OF SUPPORTED CHASSIS COMMANDS

Same as previous release.

LIST OF SUPPORTED INTEL SPECIFIC COMMANDS (0x30)

0xA0 - 	RQ_CmdStagedPrepareForUpdate
0xA1 -	RQ_CmdStagedUpdateOpenArea
0xA2 - 	RQ_CmdStagedUpdateWriteArea
0xA3 -	RQ_CmdStagedUpdateCloseArea
0xA4 -	RQ_CmdStagedUpdateRegisterUpdate
0xA6 -	RQ_CmdStagedUpdateGetStatus
0xA7 -	RQ_CmdStagedUpdateGetCapabilities
0xA8 -	RQ_CmdStagedUpdateReadArea

Same as previous release.

LIST OF SUPPORTED BRIDGE COMMANDS

Same as previous release.

SUPPORTED SENSORS

Sensor#      	Sensor Name

Same as previous release. 

HEX IMAGE INFORMATION

OPCD CHECKSUM:  0x2E06	Start Address 0x00030000 ->  End Address  0x0007A12A	
BOOT CHECKSUM:	0x359A	Start Address 0x00000000 ->  End Address  0x00001CBE
PIA CHECKSUM:	0x34D8 	Start Address 0x00008000 ->  End Address  0x00008BBF

HEX CODE FILE:  T2BMC23.HEX   01/09/04  755,167 bytes

INFOBLOCK INFORMATION RETURNED BY: FWUPDATE T2BMC23.HEX /INFOBLOCK

OP CHECKSUM:			0x4F19	(DIB ONLY)
BOOT CHECKSUM:			0x9E7E	(DIB ONLY)
PIA HEADER CHECKSUM:	0x4F19	(DIB ONLY)

REVISION INFORMATION RETURNED BY: FWUPDATE /FWVERSION

Op Code:		v00.23
Boot Code:		v00.15
PIA version: 	1
PIA instance: 	23

FILE VERSION TAGS
ACPIEC_VER			 	= 	v0.26	
ALERT_VER			 	= 	v0.54.5
BOOT_VER			 	= 	v0.19	
CHANNEL_VER			 	= 	v0.47.2  	
COMMON_VER			 	= 	v0.14.1  	
CPU_VER				 	= 	v0.51.4 	
DEBUG_VER			 	= 	v0.09	
DRIVERS_VER			 	= 	v0.14	
EMP_VER				 	= 	v0.62.6	
EXTERNAL_VER		 	= 	v0.64.2	
ICMB_VER			 	= 	v0.29.2	
IPMB_VER			 	= 	v0.25	
IPMI_VER			 	= 	v0.61.4
KCS_VER				 	= 	v0.39.1	
LAN_VER				 	= 	v0.52.2	
MEMALLOC_VER		 	= 	v0.42.2
MEMERR_VER			 	= 	v0.62.5	
MISC_VER			 	= 	v0.64.2.2
NVSTORE_VER			 	= 	v0.56.4
OS_VER				 	= 	v0.08	
PIA_VER				 	= 	v0.17	
PLATFORM_VER		 	= 	v0.23
POWER_VER			 	= 	v0.64.1	
SAHALEE_VER			 	= 	v0.39.1	
SCANNING_VER		 	= 	v0.51.2	
SENSORIPMI_VER		 	= 	v0.55.4
SENSORS_VER			 	= 	v0.35	
SESSION_VER			 	= 	v0.49.4	
USERINTF_VER		 	= 	v0.25	
UTILITIES_VER		 	= 	v0.41.1
TMODE_VER			 	= 	v0.10.1	
OPCODESTAGEDUPDATE_VER	= 	v0.09

TOOLS USED IN BUILD
getbmc.bat	version 1.5
gmake		Version 3.79.1
get 		v6.6.10
PVCS		version 6.6
ARM tools	version 2.51
WinZip		v7.0
Windiff

----------------------------------------------------------------------------

RELEASE NOTES FOR SR870BH2 BMC RELEASE  0.22 - HPC RC3 - Feature Complete release.
December 03, 2003

- This T2BMC22 is the Feature Complete HPC (RC3) Release.

- Use 'FWUpdate' utility to flash BMC22 operational code into the BMC flash if current BMC 
  version is 15.  If upgrading from BMC21E to BMC22 you may use OFU utility.
- Subsequent updates of Operational Firmware, PIA, and SDR can be staged and updated using BMC22.
- This version of BMC has been released with a working old BootCode version 15.
- All the user settings from current BMC will be restored when moved to new BMC22.
- Down revising the BMC may result in all settings being returned to factory defaults.
- Updating to this version from BMC 0.08 or lower requires Boot Block update.
  Use jumper J3A3 on the MB and switch FROM default 1-2 (Boot protected) TO 
  2-3 (Boot programmable) 
- SDR13 should be used with this BMC version.
      
CHANGES SINCE PREVIOUS VERSION (VER 0.20)
* IPMI 1.5 core bug fixes in this release.  
none

* Platform Specific bug fixes in this release.  
"35320"	"Sev1"	"Unable to power on system after updating to BMC21"
"34987"	"WriteUpdateNotify command returning CompCode 0x80"	"Sev1"
"35172"	"Front Panel lock command is breaking the online FW Update"	"Sev2"
"35177"	"BMC is not allowing flashing over a previous update of the BMC."	"Sev2"
"35115"	"Syscfg restores disabled proc state"	"Sev2"
"34688"	"Sev2"	"BMC 19 produces ""ERROR: Baseboard Management Controller fails to function"""
"34723"	"Sev3"	"System does not respond to BMC19"

DEPENDENCIES 

* The features added in this release require PLD 1 P/N: A86808-003 (mainboard 401) or later.
* PLD 1 enabling access to second half of the flash needs to be updated with latest version using 
  external Lattice Programmer. 

KNOWN ISSUES 

* Updating from BMC v0.13 or ealier will result in the loss of some PEF filter settings 
  in private store.

Reference to NETFn Numbers
CHASSIS_REQUEST					0x00
BRIDGE_REQUEST					0x02
SNSR_EVENT_REQUEST				0x04
APP_REQUEST						0x06
FIRMWARE_REQUEST				0x08
STORAGE_REQUEST					0x0a
TRANSPORT_REQUEST				0x0c
INTEL_GENERAL_APP_REQUEST		0x30
INTEL_PLATFORM_SPECIFIC_REQUEST	0x32
INTEL_SOL_TMODE_REQUEST			0x34

LIST OF SUPPORTED APPLICATION COMMANDS (0x06)

Same as previous release.

LIST OF SUPPORTED SENSOR/EVENT COMMANDS	(0x04)

Same as previous release.

LIST OF SUPPORTED FIRMWARE TRANSFER COMMANDS (0x01)

Same as previous release.

LIST OF SUPPORTED CHASSIS COMMANDS

Same as previous release.

LIST OF SUPPORTED INTEL SPECIFIC COMMANDS (0x30)

0xA0 - 	RQ_CmdStagedPrepareForUpdate
0xA1 -	RQ_CmdStagedUpdateOpenArea
0xA2 - 	RQ_CmdStagedUpdateWriteArea
0xA3 -	RQ_CmdStagedUpdateCloseArea
0xA4 -	RQ_CmdStagedUpdateRegisterUpdate
0xA6 -	RQ_CmdStagedUpdateGetStatus
0xA7 -	RQ_CmdStagedUpdateGetCapabilities
0xA8 -	RQ_CmdStagedUpdateReadArea

Same as previous release.

LIST OF SUPPORTED BRIDGE COMMANDS

Same as previous release.

SUPPORTED SENSORS

Sensor#      	Sensor Name

Same as previous release. 

HEX IMAGE INFORMATION

OPCD CHECKSUM:  0xE841	Start Address 0x00030000 ->  End Address  0x0007ATBD	
BOOT CHECKSUM:	0x359A	Start Address 0x00000000 ->  End Address  0x00001CBE
PIA CHECKSUM:	0x34D8 	Start Address 0x00008000 ->  End Address  0x00008BBF

HEX CODE FILE:  T2BMC22.HEX   12/03/03  755,074 bytes

INFOBLOCK INFORMATION RETURNED BY: FWUPDATE T2BMC22.HEX /INFOBLOCK

OP CHECKSUM:			0x5D54	(DIB ONLY)
BOOT CHECKSUM:			0xAA90	(DIB ONLY)
PIA HEADER CHECKSUM:	0x452A	(DIB ONLY)

REVISION INFORMATION RETURNED BY: FWUPDATE /FWVERSION

Op Code:		v00.22
Boot Code:		v00.15
PIA version: 	1
PIA instance: 	22

FILE VERSION TAGS
ACPIEC_VER			= 	v0.26	
ALERT_VER			= 	v0.54.5
BOOT_VER			= 	v0.19	
CHANNEL_VER			= 	v0.47.2  	
COMMON_VER			= 	v0.14.1  	
CPU_VER				= 	v0.51.4 	
DEBUG_VER			= 	v0.09	
DRIVERS_VER			= 	v0.14	
EMP_VER				= 	v0.62.6	
EXTERNAL_VER		= 	v0.64.2	
ICMB_VER			= 	v0.29.2	
IPMB_VER			= 	v0.25	
IPMI_VER			= 	v0.61.4
KCS_VER				= 	v0.39.1	
LAN_VER				= 	v0.52.2	
MEMALLOC_VER		= 	v0.42.2
MEMERR_VER			= 	v0.62.5	
MISC_VER			= 	v0.64.2.2
NVSTORE_VER			= 	v0.56.4
OS_VER				= 	v0.08	
PIA_VER				= 	v0.17	
PLATFORM_VER		= 	v0.22
POWER_VER			= 	v0.64.1	
SAHALEE_VER			= 	v0.39.1	
SCANNING_VER		= 	v0.51.2	
SENSORIPMI_VER		= 	v0.55.4
SENSORS_VER			= 	v0.35	
SESSION_VER			= 	v0.49.4	
USERINTF_VER		= 	v0.25	
UTILITIES_VER		= 	v0.41.1
TMODE_VER			= 	v0.10.1	
OPCODESTAGEDUPDATE_VER		= 	v0.07

TOOLS USED IN BUILD
getbmc.bat	version 1.5
gmake		Version 3.79.1
get 		v6.6.10
PVCS		version 6.6
ARM tools	version 2.51
WinZip		v7.0
Windiff

----------------------------------------------------------------------------

RELEASE NOTES FOR SR870BH2 BMC RELEASE  0.21 - HPC RC2 - Feature Complete release.
December 02, 2003


*********************************************************************
***************** This BMC21 has been RECALLED **********************
*********************************************************************
***************** Do not use this BMC21 on any Tiger2 System ********
*********************************************************************

- This T2BMC21 is the Feature Complete HPC (RC2) Release.

- Use 'FWUpdate' utility to flash BMC21 operational code into the BMC flash if current BMC version is 15.
- Subsequent updates of Operational Firmware, PIA, and SDR can be staged and updated using BMC21.
- This version of BMC (21) has been released with a working old BootCode version 15.
- All the user settings from current BMC will be restored when moved to new BMC21.
- Down revising the BMC may result in all settings being returned to factory defaults.
- Updating to this version from BMC 0.08 or lower requires Boot Block update.
  Use jumper J3A3 on the MB and switch FROM default 1-2 (Boot protected) TO 
  2-3 (Boot programmable) 
- SDR13 should be used with this BMC version.
      
CHANGES SINCE PREVIOUS VERSION (VER 0.20)
* IPMI 1.5 core bug fixes in this release.  
none

* Platform Specific bug fixes in this release.  
"34987"	"WriteUpdateNotify command returning CompCode 0x80"	"Sev1"
"35172"	"Front Panel lock command is breaking the online FW Update"	"Sev2"
"35177"	"BMC is not allowing flashing over a previous update of the BMC."	"Sev2"
"35115"	"Syscfg restores disabled proc state"	"Sev2"

DEPENDENCIES 

* The features added in this release require PLD 1 P/N: A86808-003 (mainboard 401) or later.
* PLD 1 enabling access to second half of the flash. needs to be updated with latest version using 
  external Lattice Programmer. 

KNOWN ISSUES 

* Updating from BMC v0.13 or ealier will result in the loss of some PEF filter settings 
  in private store.

Reference to NETFn Numbers
CHASSIS_REQUEST					0x00
BRIDGE_REQUEST					0x02
SNSR_EVENT_REQUEST				0x04
APP_REQUEST						0x06
FIRMWARE_REQUEST				0x08
STORAGE_REQUEST					0x0a
TRANSPORT_REQUEST				0x0c
INTEL_GENERAL_APP_REQUEST		0x30
INTEL_PLATFORM_SPECIFIC_REQUEST	0x32
INTEL_SOL_TMODE_REQUEST			0x34

LIST OF SUPPORTED APPLICATION COMMANDS (0x06)

Same as previous release.

LIST OF SUPPORTED SENSOR/EVENT COMMANDS	(0x04)

Same as previous release.

LIST OF SUPPORTED FIRMWARE TRANSFER COMMANDS (0x01)

Same as previous release.

LIST OF SUPPORTED CHASSIS COMMANDS

Same as previous release.

LIST OF SUPPORTED INTEL SPECIFIC COMMANDS (0x30)

0xA0 - 	RQ_CmdStagedPrepareForUpdate
0xA1 -	RQ_CmdStagedUpdateOpenArea
0xA2 - 	RQ_CmdStagedUpdateWriteArea
0xA3 -	RQ_CmdStagedUpdateCloseArea
0xA4 -	RQ_CmdStagedUpdateRegisterUpdate
0xA6 -	RQ_CmdStagedUpdateGetStatus
0xA7 -	RQ_CmdStagedUpdateGetCapabilities
0xA8 -	RQ_CmdStagedUpdateReadArea

Same as previous release.

LIST OF SUPPORTED BRIDGE COMMANDS

Same as previous release.

SUPPORTED SENSORS

Sensor#      	Sensor Name

Same as previous release. 

HEX IMAGE INFORMATION

OPCD CHECKSUM:  0x7CC2	Start Address 0x00030000 ->  End Address  0x0007A1A6	
BOOT CHECKSUM:	0x359A	Start Address 0x00000000 ->  End Address  0x00001CBE
PIA CHECKSUM:	0x34D8 	Start Address 0x00008000 ->  End Address  0x00008BBF

HEX CODE FILE:  T2BMC21.HEX   12/02/03  755,467 bytes

INFOBLOCK INFORMATION RETURNED BY: FWUPDATE T2BMC21.HEX /INFOBLOCK

OP CHECKSUM:			0x53B2	(DIB ONLY)
BOOT CHECKSUM:			0xAA95	(DIB ONLY)
PIA HEADER CHECKSUM:	0x462A	(DIB ONLY)

REVISION INFORMATION RETURNED BY: FWUPDATE /FWVERSION

Op Code:		v00.21
Boot Code:		v00.15
PIA version: 	1
PIA instance: 	21

FILE VERSION TAGS
ACPIEC_VER			 	= 	v0.26	
ALERT_VER			 	= 	v0.54.5
BOOT_VER			 	= 	v0.19	
CHANNEL_VER			 	= 	v0.47.2  	
COMMON_VER			 	= 	v0.14.1  	
CPU_VER				 	= 	v0.51.4 	
DEBUG_VER			 	= 	v0.09	
DRIVERS_VER			 	= 	v0.14	
EMP_VER				 	= 	v0.62.6	
EXTERNAL_VER		 	= 	v0.64.2	
ICMB_VER			 	= 	v0.29.2	
IPMB_VER			 	= 	v0.25	
IPMI_VER			 	= 	v0.61.4
KCS_VER				 	= 	v0.39.1	
LAN_VER				 	= 	v0.52.2	
MEMALLOC_VER		 	= 	v0.42.2
MEMERR_VER			 	= 	v0.62.5	
MISC_VER			 	= 	v0.64.2.2
NVSTORE_VER			 	= 	v0.56.4
OS_VER				 	= 	v0.08	
PIA_VER				 	= 	v0.17	
PLATFORM_VER		 	= 	v0.21
POWER_VER			 	= 	v0.64.1	
SAHALEE_VER			 	= 	v0.39.1	
SCANNING_VER		 	= 	v0.51.2	
SENSORIPMI_VER		 	= 	v0.55.4
SENSORS_VER			 	= 	v0.35	
SESSION_VER			 	= 	v0.49.4	
USERINTF_VER		 	= 	v0.25	
UTILITIES_VER		 	= 	v0.41.1
TMODE_VER			 	= 	v0.10.1	
OPCODESTAGEDUPDATE_VER	= 	v0.06

TOOLS USED IN BUILD
getbmc.bat	version 1.5
gmake		Version 3.79.1
get 		v6.6.10
PVCS		version 6.6
ARM tools	version 2.51
WinZip		v7.0
Windiff
----------------------------------------------------------------------------

RELEASE NOTES FOR Tiger2 BMC RELEASE  0.20 - HPC RC1 - Feature Complete release.
November 13, 2003

- This T2BMC20 is the Feature Complete HPC (RC1) feature set Release.
Highlights of HPC features; 
  	- Save and Restore completely. (Restore, only restores User settings)
  	- Staging all other three areas (OPFW, PIA, & SDR) 
	- Updating the Staged OPFW, PIA, & SDR image to Execution area upon following system reset
	- Supports Write and Read into UCA area and update it to BMC Private Store upon update request.
	- Private Store and UCA always in sync bi-directionally.

- This version of BMC (20) has been released with a working old BootCode version 15.
- Updating to this version from BMC 0.08 or lower requires Boot Block update.
  Use jumper J3A3 on the MB and switch FROM default 1-2 (Boot protected) TO 
  2-3 (Boot programmable) 
- SDR13 should be used with this BMC version.
      
CHANGES SINCE PREVIOUS VERSION (VER 0.19)
- Complete HPC features set is supported in this release and its at feature complete level.

* IPMI 1.5 core bug fixes in this release.  
none

* Platform Specific bug fixes in this release.  
"NONE"	"Staged Update - The BMC cmd "StagedUpdateReadArea" fails when syscfg tries to read data from UCA multile times."  


DEPENDENCIES 

* The features added in this release require PLD 1 P/N: A86808-003 (mainboard 401) or later.
* PLD 1 enabling access to second half of the flash. needs to be updated with latest version using 
  external Lattice Programmer. 
* PLD 2 needs to be updated with latest version using PLD update utility. 
  This is needed for BMC Snoop function to work, Otherwise old PLD code still works with BMC12 or later.

KNOWN ISSUES 

* The Hurdle Test results may not be available for this release.

* Updateing from BMC v0.13 or ealier will resultin the loss of some PEF filter settings in private store.

Reference to NETFn Numbers
CHASSIS_REQUEST					0x00
BRIDGE_REQUEST					0x02
SNSR_EVENT_REQUEST				0x04
APP_REQUEST						0x06
FIRMWARE_REQUEST				0x08
STORAGE_REQUEST					0x0a
TRANSPORT_REQUEST				0x0c
INTEL_GENERAL_APP_REQUEST		0x30
INTEL_PLATFORM_SPECIFIC_REQUEST	0x32
INTEL_SOL_TMODE_REQUEST			0x34

LIST OF SUPPORTED APPLICATION COMMANDS (0x06)

Same as previous release.

LIST OF SUPPORTED SENSOR/EVENT COMMANDS	(0x04)

Same as previous release.

LIST OF SUPPORTED FIRMWARE TRANSFER COMMANDS (0x01)

Same as previous release.

LIST OF SUPPORTED CHASSIS COMMANDS

Same as previous release.

LIST OF SUPPORTED INTEL SPECIFIC COMMANDS (0x30)

0xA0 - 	RQ_CmdStagedPrepareForUpdate
0xA1 -	RQ_CmdStagedUpdateOpenArea
0xA2 - 	RQ_CmdStagedUpdateWriteArea
0xA3 -	RQ_CmdStagedUpdateCloseArea
0xA4 -	RQ_CmdStagedUpdateRegisterUpdate (revised in this 19 release)
0xA6 -	RQ_CmdStagedUpdateGetStatus
0xA7 -	RQ_CmdStagedUpdateGetCapabilities
0xA8 -	RQ_CmdStagedUpdateReadArea

Same as previous release.

LIST OF SUPPORTED BRIDGE COMMANDS

Same as previous release.

SUPPORTED SENSORS

Sensor#      	Sensor Name

Same as previous release. 

HEX IMAGE INFORMATION

OPCD CHECKSUM:  0xF7F7	Start Address 0x00030000 ->  End Address  0x00079ADE
BOOT CHECKSUM:	0x359A	Start Address 0x00000000 ->  End Address  0x00001CBE
PIA CHECKSUM:	0x34D8 	Start Address 0x00008000 ->  End Address  0x00008BBF

HEX CODE FILE:  T2BMC19.HEX   10/03/03  751,280 bytes

INFOBLOCK INFORMATION RETURNED BY: FWUPDATE T2BMC19.HEX /INFOBLOCK

OP CHECKSUM:			0x5A64	(DIB ONLY)
BOOT CHECKSUM:			0xA173	(DIB ONLY)
PIA HEADER CHECKSUM:	0x4F2C	(DIB ONLY)

REVISION INFORMATION RETURNED BY: FWUPDATE /FWVERSION

Op Code:	v00.19
Boot Code:	v00.15
PIA version: 	1
PIA instance: 	19

FILE VERSION TAGS
ACPIEC_VER						= 	v0.26
ALERT_VER						= 	v0.54.4	
BOOT_VER						= 	v0.19
CHANNEL_VER						= 	v0.47.2
COMMON_VER						= 	v0.14.1
CPU_VER							= 	v0.51.3	
DEBUG_VER						= 	v0.09
DRIVERS_VER						= 	v0.14
EMP_VER							= 	v0.62.4
EXTERNAL_VER					= 	v0.64.1
ICMB_VER						= 	v0.29.1
IPMB_VER						= 	v0.25
IPMI_VER						= 	v0.61.3.3
KCS_VER							= 	v0.39.1
LAN_VER							= 	v0.52.1
MEMALLOC_VER					= 	v0.42.1
MEMERR_VER						= 	v0.62
MISC_VER						= 	v0.64.2.2
NVSTORE_VER						= 	v0.56.1.1
OS_VER							= 	v0.08
PIA_VER							= 	v0.17
PLATFORM_VER					= 	v0.19
POWER_VER						= 	v0.64.1
SAHALEE_VER						= 	v0.39.1	
SCANNING_VER					= 	v0.51
SENSORIPMI_VER					= 	v0.55.3
SENSORS_VER						= 	v0.35
SESSION_VER						= 	v0.49.2
USERINTF_VER					= 	v0.25
UTILITIES_VER					= 	v0.41.1
TMODE_VER						= 	v0.10
OPCODESTAGEDUPDATE_VER			= 	v0.03


TOOLS USED IN BUILD
getbmc.bat	version 1.5
gmake		Version 3.79.1
get 		v6.6.10
PVCS		version 6.6
ARM tools	version 2.51
WinZip		v7.0

----------------------------------------------------------------------------

RELEASE NOTES FOR Tiger2 BMC RELEASE  0.19 - HPC ALPHA3 - Code Complete release.
October 03, 2003

- This BMC19 is the Code Complete HPC (APLHA3) feature set Release.
  This supports 
  	- Save and Restore 
  	- Staging all other three areas (OPFW, PIA, & SDR) 
	- Updating the Staged image to Execution area 
	- Supports Write and Read into UCA area and update it to BMC Priovate Store.
	- Private Store and UCA always in sync bi-directionally.

- This version of BMC (19) has been released with a working old BootCode version 15.
- Updating to this version from BMC 0.08 or lower requires Boot Block update.
  Use jumper J3A3 on the MB and switch FROM default 1-2 (Boot protected) TO 
  2-3 (Boot programmable) 
- SDR13 should be used with this BMC (version 19).
      
CHANGES SINCE PREVIOUS VERSION (VER 0.18)
- Boot Code version rolled back to 15 per programs recommendations.
- Complete HPC features set is supported in the release.  However, this release is code complete
  and will be promoted to Feature complete after its acceptance by Evaluation teams. 
  																 
* IPMI 1.5 core bug fixes in this release.  
none

* Platform Specific bug fixes in this release.  
"34375"	"Staged Update GetStatus command returns too few bytes"
"34406"	"Staged Update - Register Update requests more than 1 byte"
"34610"	"Staged Update -  Online (staging) BMC updates is not working "
"34609 Issue1"	"Staged Update -  Online (staging) cmds for FW & SDR update must be backward compatible."
"34603"	"Staged Update - The BMC cmd "StagedUpdateReadArea" fails when syscfg tries to read data from UCA"  


DEPENDENCIES 

* The features added in this release require PLD 1 P/N: A86808-003 (mainboard 401) or later.
* PLD 1 enabling access to second half of the flash. needs to be updated with latest version using 
  external Lattice Programmer. 
* PLD 2 needs to be updated with latest version using PLD update utility. 
  This is needed for BMC Snoop function to work, Otherwise old PLD code still works with BMC12 or later.

KNOWN ISSUES 

* The Hurdle Test results may not be available for this release.

* Updateing from BMC v0.13 or ealier will resultin the loss of some PEF filter settings in private store.

Reference to NETFn Numbers
CHASSIS_REQUEST					0x00
BRIDGE_REQUEST					0x02
SNSR_EVENT_REQUEST				0x04
APP_REQUEST						0x06
FIRMWARE_REQUEST				0x08
STORAGE_REQUEST					0x0a
TRANSPORT_REQUEST				0x0c
INTEL_GENERAL_APP_REQUEST		0x30
INTEL_PLATFORM_SPECIFIC_REQUEST	0x32
INTEL_SOL_TMODE_REQUEST			0x34

LIST OF SUPPORTED APPLICATION COMMANDS (0x06)

Same as previous release.

LIST OF SUPPORTED SENSOR/EVENT COMMANDS	(0x04)

Same as previous release.

LIST OF SUPPORTED FIRMWARE TRANSFER COMMANDS (0x01)

Same as previous release.

LIST OF SUPPORTED CHASSIS COMMANDS

Same as previous release.

LIST OF SUPPORTED INTEL SPECIFIC COMMANDS (0x30)

0xA0 - 	RQ_CmdStagedPrepareForUpdate
0xA1 -	RQ_CmdStagedUpdateOpenArea
0xA2 - 	RQ_CmdStagedUpdateWriteArea
0xA3 -	RQ_CmdStagedUpdateCloseArea
0xA4 -	RQ_CmdStagedUpdateRegisterUpdate (revised in this 19 release)
0xA6 -	RQ_CmdStagedUpdateGetStatus
0xA7 -	RQ_CmdStagedUpdateGetCapabilities
0xA8 -	RQ_CmdStagedUpdateReadArea

Same as previous release.

LIST OF SUPPORTED BRIDGE COMMANDS

Same as previous release.

SUPPORTED SENSORS

Sensor#      	Sensor Name

Same as previous release. 

HEX IMAGE INFORMATION

OPCD CHECKSUM:  0xF7F7	Start Address 0x00030000 ->  End Address  0x00079ADE
BOOT CHECKSUM:	0x359A	Start Address 0x00000000 ->  End Address  0x00001CBE
PIA CHECKSUM:	0x34D8 	Start Address 0x00008000 ->  End Address  0x00008BBF

HEX CODE FILE:  T2BMC19.HEX   10/03/03  751,280 bytes

INFOBLOCK INFORMATION RETURNED BY: FWUPDATE T2BMC19.HEX /INFOBLOCK

OP CHECKSUM:			0x5A64	(DIB ONLY)
BOOT CHECKSUM:			0xA173	(DIB ONLY)
PIA HEADER CHECKSUM:	0x4F2C	(DIB ONLY)

REVISION INFORMATION RETURNED BY: FWUPDATE /FWVERSION

Op Code:	v00.19
Boot Code:	v00.15
PIA version: 	1
PIA instance: 	19

FILE VERSION TAGS
ACPIEC_VER						= 	v0.26
ALERT_VER						= 	v0.54.4	
BOOT_VER						= 	v0.19
CHANNEL_VER						= 	v0.47.2
COMMON_VER						= 	v0.14.1
CPU_VER							= 	v0.51.3	
DEBUG_VER						= 	v0.09
DRIVERS_VER						= 	v0.14
EMP_VER							= 	v0.62.4
EXTERNAL_VER					= 	v0.64.1
ICMB_VER						= 	v0.29.1
IPMB_VER						= 	v0.25
IPMI_VER						= 	v0.61.3.3
KCS_VER							= 	v0.39.1
LAN_VER							= 	v0.52.1
MEMALLOC_VER					= 	v0.42.1
MEMERR_VER						= 	v0.62
MISC_VER						= 	v0.64.2.2
NVSTORE_VER						= 	v0.56.1.1
OS_VER							= 	v0.08
PIA_VER							= 	v0.17
PLATFORM_VER					= 	v0.19
POWER_VER						= 	v0.64.1
SAHALEE_VER						= 	v0.39.1	
SCANNING_VER					= 	v0.51
SENSORIPMI_VER					= 	v0.55.3
SENSORS_VER						= 	v0.35
SESSION_VER						= 	v0.49.2
USERINTF_VER					= 	v0.25
UTILITIES_VER					= 	v0.41.1
TMODE_VER						= 	v0.10
OPCODESTAGEDUPDATE_VER			= 	v0.03


TOOLS USED IN BUILD
getbmc.bat	version 1.5
gmake		Version 3.79.1
get 		v6.6.10
PVCS		version 6.6
ARM tools	version 2.51
WinZip		v7.0

----------------------------------------------------------------------------

RELEASE NOTES FOR Tiger2 BMC RELEASE  0.18 - HPC ALPHA2
September 11, 2003

- This BMC18 is the Second HPC (APLHA2) feature set Release.
  This supports 
  	- Save and Restore 
  	- Staging all other three areas (OPFW, PIS, & SDR) 
	- Updating the Staged image to Execution area 
	- Supports Write and Read into UCA area like BMC17
  NOTE: Updating UCA to Private store is outside the scope of this release and will
  be available in the next release - BMC19. Synchronization with Private Store will 
  take place in BMC19 ALPHA3 release.

- This version of BMC (18) will work with old BootCode version 15 also.
- Updating to this version from BMC 0.08 or lower requires Boot Block update.
  Use jumper J3A3 on the MB and switch FROM default 1-2 (Boot protected) TO 
  2-3 (Boot programmable) 
- SDR13 should be used with this BMC (version 18).
      
CHANGES SINCE PREVIOUS VERSION (VER 0.15)
- Boot Code version 16 is delivered with this image like the previous one but its  
  not necessary to upgrade to 16.  Recommend staying with ver 15 boot code. T2BMC18
  will work with Version 15 Boot code.
- New functionality of Staging all the remaining areas and updating them to thier destination
  in execution area is supported.
  																 
* IPMI 1.5 core bug fixes in this release.  
none

* Platform Specific bug fixes in this release.  
"34375"	"Staged Update GetStatus command returns too few bytes"
"34406"	"Staged Update - Register Update requests more than 1 byte"
"UNKNOWN" "UCA update independent of staging image is not possible"

DEPENDENCIES 

* PLD 2 needs to be updated with latest version using PLD update utility. 
  This is needed for BMC Snoop function to work, Otherwise old PLD code still works with BMC12 or later.
* The features added in this release require PLD 1 P/N: A86808-003 (mainboard 401) or later.

KNOWN ISSUES 

* The Hurdle Test results may not be available as its ALpha2 release.

* Updateing from BMC v0.13 or ealier will resultin the loss of some PEF filter settings in private store.

Reference to NETFn Numbers
CHASSIS_REQUEST					0x00
BRIDGE_REQUEST					0x02
SNSR_EVENT_REQUEST				0x04
APP_REQUEST						0x06
FIRMWARE_REQUEST				0x08
STORAGE_REQUEST					0x0a
TRANSPORT_REQUEST				0x0c
INTEL_GENERAL_APP_REQUEST		0x30
INTEL_PLATFORM_SPECIFIC_REQUEST	0x32
INTEL_SOL_TMODE_REQUEST			0x34


LIST OF SUPPORTED APPLICATION COMMANDS (0x06)

Same as previous release.

LIST OF SUPPORTED SENSOR/EVENT COMMANDS	(0x04)

Same as previous release.

LIST OF SUPPORTED FIRMWARE TRANSFER COMMANDS (0x01)

Same as previous release.

LIST OF SUPPORTED CHASSIS COMMANDS

Same as previous release.

LIST OF SUPPORTED INTEL SPECIFIC COMMANDS (0x30)

0xA0 - 	RQ_CmdStagedPrepareForUpdate
0xA1 -	RQ_CmdStagedUpdateOpenArea
0xA2 - 	RQ_CmdStagedUpdateWriteArea
0xA3 -	RQ_CmdStagedUpdateCloseArea
0xA4 -	RQ_CmdStagedUpdateRegisterUpdate
0xA6 -	RQ_CmdStagedUpdateGetStatus
0xA7 -	RQ_CmdStagedUpdateGetCapabilities
0xA8 -	RQ_CmdStagedUpdateReadArea

Same as previous release.

LIST OF SUPPORTED BRIDGE COMMANDS

Same as previous release.

SUPPORTED SENSORS

Sensor#      	Sensor Name

Same as previous release. 

HEX IMAGE INFORMATION

OPCD CHECKSUM:  0x7C51	Start Address 0x00030000 ->  End Address  0x00079722
BOOT CHECKSUM:	0xA3DA	Start Address 0x00000000 ->  End Address  0x00001CA6
PIA CHECKSUM:	0x34D8 	Start Address 0x00008000 ->  End Address  0x00008BBF

HEX CODE FILE:  T2BMC18.HEX   09/11/03  748,991 bytes

INFOBLOCK INFORMATION RETURNED BY: FWUPDATE T2BMC18.HEX /INFOBLOCK

OP CHECKSUM:			0x5A23	(DIB ONLY)
BOOT CHECKSUM:			0xA68B	(DIB ONLY)
PIA HEADER CHECKSUM:	0x502C	(DIB ONLY)

REVISION INFORMATION RETURNED BY: FWUPDATE /FWVERSION

Op Code:	v00.18
Boot Code:	v00.16
PIA version: 	1
PIA instance: 	18

FILE VERSION TAGS
ACPIEC_VER						= 	v0.26	
ALERT_VER						= 	v0.54.4	
BOOT_VER						= 	v0.19	
CHANNEL_VER						= 	v0.47.2  	
COMMON_VER						= 	v0.14.1  	
CPU_VER							= 	v0.51.3 	
DEBUG_VER						= 	v0.09	
DRIVERS_VER						= 	v0.14	
EMP_VER							= 	v0.62.4	
EXTERNAL_VER					= 	v0.64.1	
ICMB_VER						= 	v0.29.1	
IPMB_VER						= 	v0.25	
IPMI_VER						= 	v0.61.3.2	
KCS_VER							= 	v0.39.1	
LAN_VER							= 	v0.52.1	
MEMALLOC_VER					= 	v0.42.1 	
MEMERR_VER						= 	v0.62	
MISC_VER						= 	v0.64.2.1	
NVSTORE_VER						= 	v0.56.1
OS_VER							= 	v0.08	
PIA_VER							= 	v0.17	
PLATFORM_VER					= 	v0.18
POWER_VER						= 	v0.64.1	
SAHALEE_VER						= 	v0.39.1	
SCANNING_VER					= 	v0.51	
SENSORIPMI_VER					= 	v0.55.2	
SENSORS_VER						= 	v0.35	
SESSION_VER						= 	v0.49.2	
USERINTF_VER					= 	v0.25	
UTILITIES_VER					= 	v0.41.1
TMODE_VER						= 	v0.10	
OPCODESTAGEDUPDATE_VER			= 	v0.02


TOOLS USED IN BUILD
getbmc.bat	version 1.5
gmake		Version 3.79.1
get 		v6.6.10
PVCS		version 6.6
ARM tools	version 2.51
WinZip		v7.0

----------------------------------------------------------------------------
RELEASE NOTES FOR Tiger2 BMC RELEASE  0.17 - HPC ALPHA1
August 12, 2003

- This BMC17 is the First HPC APLHA1 feature set Release.
  This supports Save and Restore functions of the HPC feature set. Restore
  at this time will only enable writing into the staging UCA area.
  Synchronization with Private Store will take place in BMC03 ALPHA3 release.
- This version of BMC (17) will work with old BootCode version 15.
- Updating to this version from BMC 0.08 or lower requires Boot Block update.
  Use jumper J3A3 on the MB and switch FROM default 1-2 (Boot protected) TO 
  2-3 (Boot programmable) 
- SDR13 should be used with this BMC (version 17).
      
CHANGES SINCE PREVIOUS VERSION (VER 0.15)
- Boot Code version 16 is delivered with this image but its not necessary 
  to upgrade to 16.  Recommend staying with ver 15 boot code. T2BMC17 will work 
  with Version 15 Boot code.
 																 
* IPMI 1.5 core bug fixes in this release.  

none

* Platform Specific bug fixes in this release.  
"33624"	"EMP: Basic mode connects even when only Terminal Mode is enabled"	"Sev3"
"31591"	"BMC: Cannot exit FTM after OP code corruption/restoration."	"Sev3"
"33535"	"LAN - RMCP Pong shouldn't have been received but was."	"Sev3"
"33928"	"Set Fault Indication to 'Degraded' prevents Set Fault Indication to 'OK'"	"Sev3"
"33886"	"BMC: TCO traffic not available on both Tiger 2 NICs."	"Sev3"
"33925"	"BMC 14 clearing fault level FRB 2 or 3 requires power cycle instead of reset."	"Sev3"
none

DEPENDENCIES 

* PLD 2 needs to be updated with latest version using PLD update utility. 
  This is needed for BMC Snoop function to work, Otherwise old PLD code still works with BMC12 or later.
* The features added in this release require PLD 1 P/N: A86808-003 (mainboard 401) or later.

KNOWN ISSUES 

* The Hurdle Test results to be released later

* Updateing from BMC v0.13 or ealier will resultin the loss of some PEF filter settings in private store.

LIST OF SUPPORTED APPLICATION COMMANDS

Same as previous release.

LIST OF SUPPORTED SENSOR/EVENT COMMANDS

Same as previous release.

LIST OF SUPPORTED FIRMWARE TRANSFER COMMANDS

Same as previous release.

LIST OF SUPPORTED CHASSIS COMMANDS

Same as previous release.

LIST OF SUPPORTED INTEL SPECIFIC COMMANDS (0x32)

Same as previous release.

LIST OF SUPPORTED BRIDGE COMMANDS

Same as previous release.

SUPPORTED SENSORS

Sensor#      	Sensor Name

Same as previous release. 

HEX IMAGE INFORMATION

OPCD CHECKSUM:  0xC39E	Start Address 0x00030000 ->  End Address  0x0007916E
BOOT CHECKSUM:	0xA3DA	Start Address 0x00000000 ->  End Address  0x00001CA6
PIA CHECKSUM:	0x34D8 	Start Address 0x00008000 ->  End Address  0x00008BBF

HEX CODE FILE:  T2BMC17.HEX   08/13/03  745,473 bytes

INFOBLOCK INFORMATION RETURNED BY: FWUPDATE T2BMC17.HEX /INFOBLOCK

OP CHECKSUM:			0x51EE	(DIB ONLY)
BOOT CHECKSUM:			0x91A6	(DIB ONLY)
PIA HEADER CHECKSUM:	0x532C	(DIB ONLY)

REVISION INFORMATION RETURNED BY: FWUPDATE /FWVERSION

Op Code:	v00.17
Boot Code:	v00.15
PIA version: 	1
PIA instance: 	15

FILE VERSION TAGS
ACPIEC_VER			= 	v0.26	
ALERT_VER			= 	v0.54.4	
BOOT_VER			= 	v0.19	
CHANNEL_VER			= 	v0.47.2
COMMON_VER			= 	v0.14.1  	
CPU_VER				= 	v0.51.3 	
DEBUG_VER			= 	v0.09	
DRIVERS_VER			= 	v0.14	
EMP_VER				= 	v0.62.4	
EXTERNAL_VER		= 	v0.64.1	
ICMB_VER			= 	v0.29.1	
IPMB_VER			= 	v0.25	
IPMI_VER			= 	v0.61.3.1	
KCS_VER				= 	v0.39.1	
LAN_VER				= 	v0.52.1	
MEMALLOC_VER		= 	v0.42.1
MEMERR_VER			= 	v0.62	
MISC_VER			= 	v0.64.2.1	
NVSTORE_VER			= 	v0.56.1	
OS_VER				= 	v0.08	
PIA_VER				= 	v0.17	
PLATFORM_VER		= 	v0.17
POWER_VER			= 	v0.64.1	
SAHALEE_VER			= 	v0.39.1	
SCANNING_VER		= 	v0.51	
SENSORIPMI_VER		= 	v0.55.1
SENSORS_VER			= 	v0.35	
SESSION_VER			= 	v0.49.2	
USERINTF_VER		= 	v0.25	
UTILITIES_VER		= 	v0.41.1
TMODE_VER			= 	v0.10	
OPCODESTAGEDUPDATE_VER = v0.01

TOOLS USED IN BUILD
getbmc.bat	version 1.5
gmake		Version 3.79.1
get 		v6.6.10
PVCS		version 6.6
ARM tools	version 2.51
WinZip		v7.0

----------------------------------------------------------------------------
RELEASE NOTES FOR Tiger2 BMC RELEASE  0.16 -RC6 
Place Holder for possible future release.

---------------------------------------------------------------------------------
RELEASE NOTES FOR Tiger2 BMC RELEASE  0.15 -RC5
July 2, 2003

*** Important Note: ***
- This BMC15 is the RC5 Release.
- Updating to this version from BMC 0.08 or lower requires Boot Block update.
  Use jumper J3A3 on the MB and switch FROM default 1-2 (Boot protected) TO 
  2-3 (Boot programmable) 
- SDR13 should be used with this BMC (version 15).
      
CHANGES SINCE PREVIOUS VERSION (VER 0.14)

-Implemented new SDINIT delay feature
-- Model dependant debounce times for front panel NMI, reset 
   and power button configurable in SDR.
-- Enabled SEL logging when INIT is raised by ICH4 and SNC via PLD 1.
- New SDR and FRU file updates.
- SDR13 under FRUSDR 2.0.13 package.

* IPMI 1.5 core bug fixes in this release.  

none

* Platform Specific bug fixes in this release.  

none

DEPENDENCIES 

* PLD 2 needs to be updated with latest version using PLD update utility. 
  This is needed for BMC Snoop function to work, Otherwise old PLD code still works with BMC12 or later.
* The features added in this release require PLD 1 P/N: A86808-003 (mainboard 401) or later.

KNOWN ISSUES 

* The Hurdle Test was Run on this version and no critical issues were found.

* Updateing from BMC v0.13 or ealier will resultin the loss of some PEF filter settings in private store.

LIST OF SUPPORTED APPLICATION COMMANDS

Same as previous release.

LIST OF SUPPORTED SENSOR/EVENT COMMANDS

Same as previous release.

LIST OF SUPPORTED FIRMWARE TRANSFER COMMANDS

Same as previous release.

LIST OF SUPPORTED CHASSIS COMMANDS

Same as previous release.

LIST OF SUPPORTED INTEL SPECIFIC COMMANDS (0x32)

Same as previous release.

LIST OF SUPPORTED BRIDGE COMMANDS

Same as previous release.

SUPPORTED SENSORS

Sensor#      	Sensor Name

Same as previous release. 

HEX IMAGE INFORMATION

OP CfsHECKSUM:  0xC5B0	Start Address 0x00030000 ->  End Address  0x00077146
BOOT CHECKSUM:	0x359A	Start Address 0x00000000 ->  End Address  0x00001CBE
PIA CHECKSUM:	0x733D  Start Address 0x00008000 ->  End Address  0x00008B7B

HEX CODE FILE:  T2BMC15.HEX   07/3/03  725,514 bytes

INFOBLOCK INFORMATION RETURNED BY: FWUPDATE T2BMC14.HEX /INFOBLOCK

OP CHECKSUM:		0x780E  (DIB ONLY)
BOOT CHECKSUM:		0x9481	(DIB ONLY)
PIA HEADER CHECKSUM:	0x1593	(DIB ONLY)

REVISION INFORMATION RETURNED BY: FWUPDATE /FWVERSION

Op Code:	v00.15
Boot Code:	v00.15
PIA version: 	1
PIA instance: 	15

FILE VERSION TAGSfs
ACPIEC_VER			= 	v0.26	
ALERT_VER			= 	v0.54.4	
BOOT_VER			= 	v0.19	
CHANNEL_VER			= 	v0.47  	
COMMON_VER			= 	v0.14  	
CPU_VER				= 	v0.51.3 	
DEBUG_VER			= 	v0.09	
DRIVERS_VER			= 	v0.14	
EMP_VER				= 	v0.62.3	
EXTERNAL_VER			= 	v0.64.1	
ICMB_VER			= 	v0.29.1	
IPMB_VER			= 	v0.25	
IPMI_VER			= 	v0.61.3	
KCS_VER				= 	v0.39.1	
LAN_VER				= 	v0.52.1	
MEMALLOC_VER			= 	v0.42 	
MEMERR_VER			= 	v0.62	
MISC_VER			= 	v0.64.2	
NVSTORE_VER			= 	v0.56	
OS_VER				= 	v0.08	
PIA_VER				= 	v0.17	
PLATFORM_VER			= 	v0.15
POWER_VER			= 	v0.64.1	
SAHALEE_VER			= 	v0.39.1	
SCANNING_VER			= 	v0.51	
SENSORIPMI_VER			= 	v0.55	
SENSORS_VER			= 	v0.35	
SESSION_VER			= 	v0.49.2	
USERINTF_VER			= 	v0.25	
UTILITIES_VER			= 	v0.41	
TMODE_VER			= 	v0.10	

TOOLS USED IN BUILD
getbmc.bat	version 1.5
gmake		Version 3.79.1
get 		v6.6.10
PVCS		version 6.6
ARM tools	version 2.51
WinZip		v7.0

----------------------------------------------------------------------------

RELEASE NOTES FOR Tiger2 BMC RELEASE  0.14 - RC4
June 20, 2003

*** Important Note: ***
- This BMC14 is the RC4 Release.
- Updating to this version from BMC 0.08 or lower requires Boot Block update.
  Use jumper J3A3 on the MB and switch FROM default 1-2 (Boot protected) TO 
  2-3 (Boot programmable) 
- SDR10 or SDR12 should be used with this BMC version of 14.
      
CHANGES SINCE PREVIOUS VERSION (VER 0.13)

- Bug Fixes:
- New SDR and FRU file updates.
   - SDR12 under FRUSDR 2.0.12 package.

* IPMI 1.5 core bug fixes in this release.  

none

* Platform Specific bug fixes in this release.  

"33740","Non critical & critical Processor temperature thresholds too high","Sev2" (This is in SDR12)
"33691","BMC - Fan speed is wrong if Tiger2 comes up with a single PS cord","Sev2"
"33799","BMC: Default PEF Startup Delay too short","Sev3"
"33638","LAN -  Incurred 1 failure(s) after restarting the watchdog.","Sev3"

"33628","CPU: Fault conditions not being indicated","Sev3" 
Note:  This tracker is also included in BMc14 with more CPU failure conditions enabled.


DEPENDENCIES 

* PLD 2 needs to be updated with latest version using PLD update utility. 
  This is needed for BMC Snoop function to work, Otherwise old PLD code still works with BMC12 or later.

KNOWN ISSUES 

* The Hurdle Test was Run on this version and no critical issues were found.

* The default PEF startup delay has been modified in BMC v0.14.  This change increases the default PEF 
  startup delay from 60 seconds to 255 seconds to allow more time to get to SMU to disable PEF if necessary.
  The implication of this PEF change is that the users will loose their PEF filters settings, as it gets 
  overwritten by the default values.

LIST OF SUPPORTED APPLICATION COMMANDS

Same as previous release.

LIST OF SUPPORTED SENSOR/EVENT COMMANDS

Same as previous release.

LIST OF SUPPORTED FIRMWARE TRANSFER COMMANDS

Same as previous release.

LIST OF SUPPORTED CHASSIS COMMANDS

Same as previous release.

LIST OF SUPPORTED INTEL SPECIFIC COMMANDS (0x32)

Same as previous release.

LIST OF SUPPORTED BRIDGE COMMANDS

Same as previous release.

SUPPORTED SENSORS

Sensor#      	Sensor Name

Same as previous release. 

HEX IMAGE INFORMATION

OP CHECKSUM:  	0xBDAC	Start Address 0x00030000 ->  End Address  0x00076CDA
BOOT CHECKSUM:	0x359A	Start Address 0x00000000 ->  End Address  0x00001CBE
PIA CHECKSUM:	0x733D  Start Address 0x00008000 ->  End Address  0x00008B7B

HEX CODE FILE:  T2BMC14.HEX   06/24/03  722,782 bytes

INFOBLOCK INFORMATION RETURNED BY: FWUPDATE T2BMC14.HEX /INFOBLOCK

OP CHECKSUM:		0x797D  (DIB ONLY)
BOOT CHECKSUM:		0x9882	(DIB ONLY)
PIA HEADER CHECKSUM:	0x1693	(DIB ONLY)

REVISION INFORMATION RETURNED BY: FWUPDATE /FWVERSION

Op Code:	v00.14
Boot Code:	v00.15
PIA version: 	1
PIA instance: 	14

FILE VERSION TAGS
ACPIEC_VER			= 	v0.26	
ALERT_VER			= 	v0.54.4	
BOOT_VER			= 	v0.19	
CHANNEL_VER			= 	v0.47  	
COMMON_VER			= 	v0.14  	
CPU_VER				= 	v0.51.3 	
DEBUG_VER			= 	v0.09	
DRIVERS_VER			= 	v0.14	
EMP_VER				= 	v0.62.3	
EXTERNAL_VER			= 	v0.64.1	
ICMB_VER			= 	v0.29.1	
IPMB_VER			= 	v0.25	
IPMI_VER			= 	v0.61.3	
KCS_VER				= 	v0.39.1	
LAN_VER				= 	v0.52.1	
MEMALLOC_VER			= 	v0.42 	
MEMERR_VER			= 	v0.62	
MISC_VER			= 	v0.64.2	
NVSTORE_VER			= 	v0.56	
OS_VER				= 	v0.08	
PIA_VER				= 	v0.17	
PLATFORM_VER			= 	v0.14
POWER_VER			= 	v0.64.1	
SAHALEE_VER			= 	v0.39.1	
SCANNING_VER			= 	v0.51	
SENSORIPMI_VER			= 	v0.55	
SENSORS_VER			= 	v0.35	
SESSION_VER			= 	v0.49.2	
USERINTF_VER			= 	v0.25	
UTILITIES_VER			= 	v0.41	
TMODE_VER			= 	v0.10	

TOOLS USED IN BUILD
getbmc.bat	version 1.5
gmake		Version 3.79.1
get 		v6.6.10
PVCS		version 6.6
ARM tools	version 2.51
WinZip		v7.0

----------------------------------------------------------------------------


RELEASE NOTES FOR Tiger2 BMC RELEASE  0.13 - RC3
June 20, 2003

*** Important Note: ***
- This BMC13 is the RC3 Release.
- Updating to this version from BMC 0.08 or lower requires Boot Block update.
  Use jumper J3A3 on the MB and switch FROM default 1-2 (Boot protected) TO 
  2-3 (Boot programmable) 
- SDR10 or SDR12 should be used with this BMC version of 13.
      
CHANGES SINCE PREVIOUS VERSION (VER 0.12)

- Bug Fixes:
- New SDR and FRU file updates.
   - SDR12 under FRUSDR 2.0.12 package.

* IPMI 1.5 core bug fixes in this release.  

none

* Platform Specific bug fixes in this release.  

"33523"	"BMC:  Should not reset sensor on general chassis intrusion event"
"33546"	"Sel log report voltages 50,51,52,86 with SDR09"
"33571"	"System Reset and SDINIT buttons do not have a delay when pressed"
"33579"	"Dell Specific LED - critical faults not being indicated"
"33514"	"BMC 11 FRB 3 on single processor does not set failure indication or event to SEL"
"33532"	"System Power button do not have a delay when pressed"
"33628"	"BMC :  CPU fault conditions not being indicated"
"33575"	"BMC- not generating ""OK"" event when fan changes to OK"
"33561" "BMC 11 Return when set to OEM Config 1 as Config 2 and Config 2 as Config 1."
"32832" "Platform Specific Commands:  3 extra commands found."

DEPENDENCIES 

* PLD 2 needs to be updated with latest version using PLD update utility. 
  This is needed for BMC Snoop function to work, Otherwise old PLD code still works with BMC12.

KNOWN ISSUES 

* The Hurdle Test was Run on this version and no critical issues were found.

LIST OF SUPPORTED APPLICATION COMMANDS

Same as previous release.

LIST OF SUPPORTED SENSOR/EVENT COMMANDS

Same as previous release.

LIST OF SUPPORTED FIRMWARE TRANSFER COMMANDS

Same as previous release.

LIST OF SUPPORTED CHASSIS COMMANDS

Same as previous release.

LIST OF SUPPORTED INTEL SPECIFIC COMMANDS (0x32)

Same as previous release.

LIST OF SUPPORTED BRIDGE COMMANDS

Same as previous release.

SUPPORTED SENSORS

Sensor#      	Sensor Name

Same as previous release. 

HEX IMAGE INFORMATION

OP CHECKSUM:  	0xD012	Start Address 0x00030000 ->  End Address  0x00076C42
BOOT CHECKSUM:	0x359A	Start Address 0x00000000 ->  End Address  0x00001CBE
PIA CHECKSUM:	0xA3E0  Start Address 0x00008000 ->  End Address  0x00008B63

HEX CODE FILE:  T2BMC13.HEX   06/20/03  722,426 bytes

INFOBLOCK INFORMATION RETURNED BY: FWUPDATE T2BMC13.HEX /INFOBLOCK

OP CHECKSUM:		0x7D14  (DIB ONLY)
BOOT CHECKSUM:		0x9381	(DIB ONLY)
PIA HEADER CHECKSUM:	0xE738	(DIB ONLY)

REVISION INFORMATION RETURNED BY: FWUPDATE /FWVERSION

Op Code:	v00.13
Boot Code:	v00.15
PIA version: 	1
PIA instance: 	13

FILE VERSION TAGS
ACPIEC_VER			= 	v0.26	
ALERT_VER			= 	v0.54.3	
BOOT_VER			= 	v0.19	
CHANNEL_VER			= 	v0.47  	
COMMON_VER			= 	v0.14  	
CPU_VER				= 	v0.51.3 	
DEBUG_VER			= 	v0.09	
DRIVERS_VER			= 	v0.14	
EMP_VER				= 	v0.62.3	
EXTERNAL_VER			= 	v0.64.1	
ICMB_VER			= 	v0.29.1	
IPMB_VER			= 	v0.25	
IPMI_VER			= 	v0.61.3	
KCS_VER				= 	v0.39.1	
LAN_VER				= 	v0.52	
MEMALLOC_VER			= 	v0.42 	
MEMERR_VER			= 	v0.62	
MISC_VER			= 	v0.64.1	
NVSTORE_VER			= 	v0.56	
OS_VER				= 	v0.08	
PIA_VER				= 	v0.17	
PLATFORM_VER			= 	v0.13
POWER_VER			= 	v0.64.1	
SAHALEE_VER			= 	v0.39.1	
SCANNING_VER			= 	v0.51	
SENSORIPMI_VER			= 	v0.55	
SENSORS_VER			= 	v0.35	
SESSION_VER			= 	v0.49.2	
USERINTF_VER			= 	v0.25	
UTILITIES_VER			= 	v0.41	
TMODE_VER			= 	v0.10	

TOOLS USED IN BUILD
getbmc.bat	version 1.5
gmake		Version 3.79.1
get 		v6.6.10
PVCS		version 6.6
ARM tools	version 2.51
WinZip		v7.0

----------------------------------------------------------------------------

RELEASE NOTES FOR Tiger2 BMC RELEASE  0.13 - RC3
May 29, 2003

*** Important Note: ***
- This BMC13 is the RC3 Release.
- Updating to this version from BMC 0.08 or lower requires Boot Block update.
  Use jumper J3A3 on the MB and switch FROM default 1-2 (Boot protected) TO 
  2-3 (Boot programmable) 
- SDR10 should be used with this BMC version of 13.
      
CHANGES SINCE PREVIOUS VERSION (VER 0.12)

- Bug Fixes:
- New SDR and FRU file updates.
   - SDR10 under FRUSDR 2.0.10 package.

* IPMI 1.5 core bug fixes in this release.  

none

* Platform Specific bug fixes in this release.  

"33523"	"BMC:  Should not reset sensor on general chassis intrusion event"
"33546"	"Sel log report voltages 50,51,52,86 with SDR09"
"33571"	"System Reset and SDINIT buttons do not have a delay when pressed"
"33579"	"Dell Specific LED - critical faults not being indicated"
"33514"	"BMC 11 FRB 3 on single processor does not set failure indication or event to SEL"
"33532"	"System Power button do not have a delay when pressed"
"33628"	"BMC :  CPU fault conditions not being indicated"
"33575"	"BMC- not generating ""OK"" event when fan changes to OK"
"33561" "BMC 11 Return when set to OEM Config 1 as Config 2 and Config 2 as Config 1."
"32832" "Platform Specific Commands:  3 extra commands found."

DEPENDENCIES 

* PLD 2 needs to be updated with latest version using PLD update utility. 
  This is needed for BMC Snoop function to work, Otherwise old PLD code still works with BMC12.

KNOWN ISSUES 

* The Hurdle Test was Run on this version and no critical issues were found.

LIST OF SUPPORTED APPLICATION COMMANDS

Same as previous release.

LIST OF SUPPORTED SENSOR/EVENT COMMANDS

Same as previous release.

LIST OF SUPPORTED FIRMWARE TRANSFER COMMANDS

Same as previous release.

LIST OF SUPPORTED CHASSIS COMMANDS

Same as previous release.

LIST OF SUPPORTED INTEL SPECIFIC COMMANDS (0x32)

Same as previous release.

LIST OF SUPPORTED BRIDGE COMMANDS

Same as previous release.

SUPPORTED SENSORS

Sensor#      	Sensor Name

Same as previous release. 

HEX IMAGE INFORMATION

OP CHECKSUM:  	0xD012	Start Address 0x00030000 ->  End Address  0x00076C42
BOOT CHECKSUM:	0x359A	Start Address 0x00000000 ->  End Address  0x00001CBE
PIA CHECKSUM:	0xA3E0  Start Address 0x00008000 ->  End Address  0x00008B63

HEX CODE FILE:  T2BMC13.HEX   05/29/03  722,426 bytes

INFOBLOCK INFORMATION RETURNED BY: FWUPDATE T2BMC13.HEX /INFOBLOCK

OP CHECKSUM:		0x85FD  (DIB ONLY)
BOOT CHECKSUM:		0xA06A	(DIB ONLY)
PIA HEADER CHECKSUM:	0xE738	(DIB ONLY)

REVISION INFORMATION RETURNED BY: FWUPDATE /FWVERSION

Op Code:	v00.13
Boot Code:	v00.15
PIA version: 	1
PIA instance: 	13

FILE VERSION TAGS
ACPIEC_VER			= 	v0.26	
ALERT_VER			= 	v0.54.3	
BOOT_VER			= 	v0.19	
CHANNEL_VER			= 	v0.47  	
COMMON_VER			= 	v0.14  	
CPU_VER				= 	v0.51.3 	
DEBUG_VER			= 	v0.09	
DRIVERS_VER			= 	v0.14	
EMP_VER				= 	v0.62.3	
EXTERNAL_VER			= 	v0.64.1	
ICMB_VER			= 	v0.29.1	
IPMB_VER			= 	v0.25	
IPMI_VER			= 	v0.61.3	
KCS_VER				= 	v0.39.1	
LAN_VER				= 	v0.52	
MEMALLOC_VER			= 	v0.42 	
MEMERR_VER			= 	v0.62	
MISC_VER			= 	v0.64.1	
NVSTORE_VER			= 	v0.56	
OS_VER				= 	v0.08	
PIA_VER				= 	v0.17	
PLATFORM_VER			= 	v0.13
POWER_VER			= 	v0.64.1	
SAHALEE_VER			= 	v0.39.1	
SCANNING_VER			= 	v0.51	
SENSORIPMI_VER			= 	v0.55	
SENSORS_VER			= 	v0.35	
SESSION_VER			= 	v0.49.2	
USERINTF_VER			= 	v0.25	
UTILITIES_VER			= 	v0.41	
TMODE_VER			= 	v0.10	

TOOLS USED IN BUILD
getbmc.bat	version 1.5
gmake		Version 3.79.1
get 		v6.6.10
PVCS		version 6.6
ARM tools	version 2.51
WinZip		v7.0

----------------------------------------------------------------------------

RELEASE NOTES FOR Tiger2 BMC RELEASE  0.12 - RC2
May 15, 2003

*** Important Note: ***
- This BMC12 is the RC2 Release.
- Updating to this version from BMC 0.08 or lower requires Boot Block update.
  Use jumper J3A3 on the MB and switch FROM default 1-2 (Boot protected) TO 
  2-3 (Boot programmable) 
- SDR09 should be used with this BMC version of 12.
      
CHANGES SINCE PREVIOUS VERSION (VER 0.11)

- Bug Fixes:
- New SDR and FRU file updates.
   - SDR09 under FRUSDR 2.0.09 package.

* IPMI 1.5 core bug fixes in this release.  

none

* Platform Specific bug fixes in this release.  

"CCB-171" Systems Fault LED Amber to light up for system degraded, (No blinking Amber) - For IBM
 (Get CCB POR CHANGE REQUEST from T2 eroom)
"33319"  "Get Current ACPI Power State returning incorrect values"  
"33114"  "Set SM Signal Functions - not all are working"  
"33408"  "Fan operation does not match the Tiger2 Thermal & Acoustics System Description"  
"33418"	 "Fan failure speed up/down couple times with SDR8"


DEPENDENCIES 

* PLD 2 needs to be updated with latest version using PLD update utility. 
  This is needed for BMC Snoop function to work, Otherwise old PLD code still works with BMC12.

KNOWN ISSUES 

* The Hurdle Test was Run on this version and no critical issues were found.

LIST OF SUPPORTED APPLICATION COMMANDS

Same as previous release.

LIST OF SUPPORTED SENSOR/EVENT COMMANDS

Same as previous release.

LIST OF SUPPORTED FIRMWARE TRANSFER COMMANDS

Same as previous release.

LIST OF SUPPORTED CHASSIS COMMANDS

Same as previous release.

LIST OF SUPPORTED INTEL SPECIFIC COMMANDS (0x32)

Same as previous release.

LIST OF SUPPORTED BRIDGE COMMANDS

Same as previous release.

SUPPORTED SENSORS

Sensor#      	Sensor Name

Same as previous release. 

HEX IMAGE INFORMATION

OP CHECKSUM:  	0xD168	Start Address 0x00030000 ->  End Address  0x00076C0E
BOOT CHECKSUM:	0x359A	Start Address 0x00000000 ->  End Address  0x00001CBE
PIA CHECKSUM:	0x2DB4  Start Address 0x00008000 ->  End Address  0x00008B5B

HEX CODE FILE:  T2BMC12.HEX   05/15/03  722,219 bytes

INFOBLOCK INFORMATION RETURNED BY: FWUPDATE T2BMC10.HEX /INFOBLOCK

OP CHECKSUM:		0x8A38  (DIB ONLY)
BOOT CHECKSUM:		0xA370	(DIB ONLY)
PIA HEADER CHECKSUM:	0x5E7C	(DIB ONLY)

REVISION INFORMATION RETURNED BY: FWUPDATE /FWVERSION

Op Code:	v00.12
Boot Code:	v00.15
PIA version: 	1
PIA instance: 	12

FILE VERSION TAGS
ACPIEC_VER			= 	v0.26	
ALERT_VER			= 	v0.54.3	
BOOT_VER			= 	v0.19	
CHANNEL_VER			= 	v0.47  	
COMMON_VER			= 	v0.14  	
CPU_VER				= 	v0.51.3 	
DEBUG_VER			= 	v0.09	
DRIVERS_VER			= 	v0.14	
EMP_VER				= 	v0.62.3	
EXTERNAL_VER		        = 	v0.64.1	
ICMB_VER			= 	v0.29.1	
IPMB_VER			= 	v0.25	
IPMI_VER			= 	v0.61.3	
KCS_VER				= 	v0.39.1	
LAN_VER				= 	v0.52	
MEMALLOC_VER		        = 	v0.42 	
MEMERR_VER			= 	v0.62	
MISC_VER			= 	v0.64.1	
NVSTORE_VER			= 	v0.56	
OS_VER				= 	v0.08	
PIA_VER				= 	v0.17	
PLATFORM_VER		        = 	v0.11
POWER_VER			= 	v0.64.1	
SAHALEE_VER			= 	v0.39.1	
SCANNING_VER	         	= 	v0.51	
SENSORIPMI_VER	          	= 	v0.55	
SENSORS_VER			= 	v0.35	
SESSION_VER			= 	v0.49.2	
USERINTF_VER		        = 	v0.25	
UTILITIES_VER		        = 	v0.41	
TMODE_VER			= 	v0.10	

TOOLS USED IN BUILD
getbmc.bat	version 1.5
gmake		Version 3.79.1
get 		v6.6.10
PVCS		version 6.6
ARM tools	version 2.51
WinZip		v7.0

----------------------------------------------------------------------------

RELEASE NOTES FOR Tiger2 BMC RELEASE  0.11 - RC1
May 1, 2003 

*** Important Note: ***
- This BMC11 is the RC1 Release.
- Updating to this version from BMC 0.08 or lower requires Boot Block update.
  Use jumper J3A3 on the MB and switch FROM default 1-2 (Boot protected) TO 
  2-3 (Boot programmable) 
- SDR08 should be used with this BMC version of 11.
      
CHANGES SINCE PREVIOUS VERSION (VER 0.10)

- Bug Fixes:
- New SDR and FRU file updates.
  - SDR08 under FRUSDR 2.0.08 package.
  - New T2PCIRSR05.FRU file to fix wrong Device ID in the header block.

* IPMI 1.5 core bug fixes in this release.  

"33146" "BMC8 Set NMI Source command can set bits 2 and 3 with good CC, but shouldn't" 

* Platform Specific bug fixes in this release.  

"33143" "BMC08 Chassis Intrusion in EPS, but Get Chassis Capabilities 0 Chassis provided"
"32870" "T2 fan speeds are incorrect" - Now Compliant with the Latest Thermal and Acoustics Spec.
"33151"	"BMC 8 FRB 2 causes FRB3 with single processor multiple no processor disabled."
"32727"	"BMC: Incorrect data returned in GetSelfTest Results"
"32209"	"FRUSDR - Power Supply 2 As/De mismatch with EPS"
"32210"	"FRUSDR - Power Supply 3 'Presence Detected' deassertion mismatch with EPS"
"32208"	"FRUSDR - System Event sensor  - 'OEM System Boot Event' As/De mismatch with EPS"
"33393"	"Set PEF Configuration Parameter 3 to 0 (no delay) fails"
"32690"	"Sighting:  Force 5v SB get 5v SB & 3.3v SB SEL entry"
"32698"	"With BMC05 the system does not power up"

DEPENDENCIES 

* PLD 2 needs to be updated with latest version using PLD update utility. 
  This is needed for BMC Snoop function to work, Otherwise old PLD code still works with BMC11.

KNOWN ISSUES 

* The Hurdle Test was Run on this version and no critical issues were found.

LIST OF SUPPORTED APPLICATION COMMANDS

Same as previous release.

LIST OF SUPPORTED SENSOR/EVENT COMMANDS

Same as previous release.

LIST OF SUPPORTED FIRMWARE TRANSFER COMMANDS

Same as previous release.

LIST OF SUPPORTED CHASSIS COMMANDS

Same as previous release.

LIST OF SUPPORTED INTEL SPECIFIC COMMANDS (0x32)

LIST OF SUPPORTED BRIDGE COMMANDS

Same as previous release.

SUPPORTED SENSORS

Sensor#      	Sensor Name

Same as previous release. 

HEX IMAGE INFORMATION

OP CHECKSUM:  	0x1069	Start Address 0x00030000 ->  End Address  0x00076C12
BOOT CHECKSUM:	0x359A	Start Address 0x00000000 ->  End Address  0x00001CBE
PIA CHECKSUM:	0x2DB4  Start Address 0x00008000 ->  End Address  0x00008B5B

HEX CODE FILE:  T2BMC11.HEX   05/01/03  722,227 bytes

INFOBLOCK INFORMATION RETURNED BY: FWUPDATE T2BMC10.HEX /INFOBLOCK

OP CHECKSUM:		0x9134  (DIB ONLY)
BOOT CHECKSUM:		0xAA6F	(DIB ONLY)
PIA HEADER CHECKSUM:	0x5F7C	(DIB ONLY)

REVISION INFORMATION RETURNED BY: FWUPDATE /FWVERSION

Op Code:	v00.11
Boot Code:	v00.15
PIA version: 	1
PIA instance: 	11

FILE VERSION TAGS
ACPIEC_VER			= 	v0.26	
ALERT_VER			= 	v0.54.3	
BOOT_VER			= 	v0.19	
CHANNEL_VER			= 	v0.47  	
COMMON_VER			= 	v0.14  	
CPU_VER				= 	v0.51.3 	
DEBUG_VER			= 	v0.09	
DRIVERS_VER			= 	v0.14	
EMP_VER				= 	v0.62.3	
EXTERNAL_VER			= 	v0.64.1	
ICMB_VER			= 	v0.29.1	
IPMB_VER			= 	v0.25	
IPMI_VER			= 	v0.61.3	
KCS_VER				= 	v0.39.1	
LAN_VER				= 	v0.52	
MEMALLOC_VER			= 	v0.42 	
MEMERR_VER			= 	v0.62	
MISC_VER			= 	v0.64.1	
NVSTORE_VER			= 	v0.56	
OS_VER				= 	v0.08	
PIA_VER				= 	v0.17	
PLATFORM_VER			= 	v0.11
POWER_VER			= 	v0.64.1	
SAHALEE_VER			= 	v0.39.1	
SCANNING_VER			= 	v0.51	
SENSORIPMI_VER			= 	v0.55	
SENSORS_VER			= 	v0.35	
SESSION_VER			= 	v0.49.2	
USERINTF_VER			= 	v0.25	
UTILITIES_VER			= 	v0.41	
TMODE_VER			= 	v0.10	

TOOLS USED IN BUILD
getbmc.bat	version 1.5
gmake		Version 3.79.1
get 		v6.6.10
PVCS		version 6.6
ARM tools	version 2.51
WinZip		v7.0

----------------------------------------------------------------------------
RELEASE NOTES FOR Tiger2 BMC RELEASE  0.10 - Beta 3
April 23, 2003 

*** Important Note: ***
- This BMC10 is the Beta Exit Release.
- Updating to this version from BMC 0.08 or lower require Boot Block update.
  Use jumper J3A3 on the MB and switch FROM default 1-2 (Boot protected) TO 
  2-3 (Boot programmable) 
- SDR07 should be used with this BMC version.
      
CHANGES SINCE PREVIOUS VERSION (VER 0.09)
- Tiger4 late bug fixes (from BMC19 & 20) are included as much as possible
  for an early testing and exposure.

- Bug Fixes:
- New SDR and FRU file updates.
  - SDR07 under FRUSDR 2.0.07 package.

* IPMI 1.5 core bug and Platform Specific bug fixes in this release.  

"33038" "Add RQ_GetAddrFRBSetting command"  
"32835" "Get LED Status platform specific command."  
"32837" "COM2 not functional while BMC in Update mode"  
"33164" "Chassis Intrusion Switch Debug"  
"33037" "Wrong beep code for zero processors"
"33303" "Termainl Mode not working"  
"33038" "Add RQ_GetAddrFRBSetting command"
"33098"	"BMC 08 Thermal Trip on single processor 0 causes FRB 3 also on the processor ."
"33114"	"Set SM Signal Functions - not all are working"
"33143"	"BMC08 Chassis Intrusion in EPS, but Get Chassis Capabilities 0 Chassis provided"
"32808"	"BMC- Set Sensor Event Enable data on start up setting reserved bits"
"32835"	"BMC:  Get LED Status platform specific command."
"33000"	"BMC - System reset after finished flashing to BMC08"
"33157"	"Get Device ID returning incorrect Product ID number"


DEPENDENCIES 

* PLD 2 needs to be updated with latest version using PLD update utility. 
  This is needed for BMC Snoop function to work, Otherwise old PLD code still works with BMC10.

KNOWN ISSUES 

* The BMC Snoop function (talking to BMC with special escape sequence while the mux 
  is on the system side) is believed to be a cause for Sev1 Terminal Mode bug. So FWEval 
  needs to verify the resolution.

* The Hurdle Test was Run on this version and no critical issues were found.

LIST OF SUPPORTED APPLICATION COMMANDS

Same as previous release.

LIST OF SUPPORTED SENSOR/EVENT COMMANDS

Same as previous release.

LIST OF SUPPORTED FIRMWARE TRANSFER COMMANDS

Same as previous release.

LIST OF SUPPORTED CHASSIS COMMANDS

Same as previous release.

LIST OF SUPPORTED INTEL SPECIFIC COMMANDS (0x32)

LIST OF SUPPORTED BRIDGE COMMANDS

Same as previous release.

SUPPORTED SENSORS

Sensor#      	Sensor Name

Same as previous release. 

HEX IMAGE INFORMATION

OP CHECKSUM:  	0xF3D9	Start Address 0x00030000 ->  End Address  0x00076C12
BOOT CHECKSUM:	0x359A	Start Address 0x00000000 ->  End Address  0x00001CBE
PIA CHECKSUM:	0x2DB4  Start Address 0x00008000 ->  End Address  0x00008B5B

HEX CODE FILE:  T2BMC10.HEX   04/23/03  722,227 bytes

INFOBLOCK INFORMATION RETURNED BY: FWUPDATE T2BMC10.HEX /INFOBLOCK

OP CHECKSUM:		0x7E46  (DIB ONLY)
BOOT CHECKSUM:		0x997F	(DIB ONLY)
PIA HEADER CHECKSUM:	0x607C	(DIB ONLY)

REVISION INFORMATION RETURNED BY: FWUPDATE /FWVERSION

Op Code:	v00.10
Boot Code:	v80.15
PIA version: 	1
PIA instance: 	10

FILE VERSION TAGS
ACPIEC_VER			= 	v0.26	
ALERT_VER			= 	v0.54.3	
BOOT_VER			= 	v0.19	
CHANNEL_VER			= 	v0.47  	
COMMON_VER			= 	v0.14  	
CPU_VER				= 	v0.51.3 	
DEBUG_VER			= 	v0.09	
DRIVERS_VER			= 	v0.14	
EMP_VER				= 	v0.62.3	
EXTERNAL_VER		= 	v0.64.1	
ICMB_VER			= 	v0.29.1	
IPMB_VER			= 	v0.25	
IPMI_VER			= 	v0.61.3	
KCS_VER				= 	v0.39.1	
LAN_VER				= 	v0.52	
MEMALLOC_VER		= 	v0.42 	
MEMERR_VER			= 	v0.62	
MISC_VER			= 	v0.64	
NVSTORE_VER			= 	v0.56	
OS_VER				= 	v0.08	
PIA_VER				= 	v0.17	
PLATFORM_VER		= 	v0.10
POWER_VER			= 	v0.64.1	
SAHALEE_VER			= 	v0.39.1	
SCANNING_VER		= 	v0.51	
SENSORIPMI_VER		= 	v0.55	
SENSORS_VER			= 	v0.35	
SESSION_VER			= 	v0.49.2	
USERINTF_VER		= 	v0.25	
UTILITIES_VER		= 	v0.41	
TMODE_VER			= 	v0.10	

TOOLS USED IN BUILD
getbmc.bat	version 1.5
gmake		Version 3.79.1
get 		v6.6.10
PVCS		version 6.6
ARM tools	version 2.51
PKZIP		v2.50

----------------------------------------------------------------------------
RELEASE NOTES FOR Tiger2 BMC RELEASE  0.09 - Beta 2
April 14, 2003 

*** Important Note: ***
- Change is in the Boot code only.  Operational Code is identical to BMC08.
- This BMC09 is the BMC Boot code Freeze Release meant for Beta System or higher only.
- Updating to this version from BMC 0.08 require Boot Block update.
  New BOOT Block is version# 14.
  Use jumper J3A3 on the MB and switch FROM default 1-2 (Boot protected) TO 
  2-3 (Boot programmable) 
- SDR06 should be used with this BMC version.
      
CHANGES SINCE PREVIOUS VERSION (VER 0.08)
**NEW - Enhancement Request**
- Intel Platform command GetChassisModeSettings (NetFn: 0x32, CMD = 0x41) is made available 
  under Boot Code for BIOS use.
**NEW - Enhancement Request**
- This release of BMC Boot code will switch BIOS Firmware Hub based on previous Lock stored 
  under NV memory.

- Enhancement Fixes:
  33293: "Need an Intel Plat command to get Chassis mode setting."
  33294: "BMC Boot Code need to select BIOS FWH based on previous Lock."

DEPENDENCIES 

* PLD code for PLD 1 and PLD 2 must be the latest version for the PLD update 
  feature to work. Contact Hardware DE for PLD code.
  (PLD files can be extracted from \\esvdp01\common\Proj\Tiger2\Technical_Data\Boardset\PLDs\Alpha)

KNOWN ISSUES 

* The Hurdle Test was Run on this version and no critical issues were found.

LIST OF SUPPORTED APPLICATION COMMANDS

Same as previous release.

LIST OF SUPPORTED SENSOR/EVENT COMMANDS

Same as previous release.

LIST OF SUPPORTED FIRMWARE TRANSFER COMMANDS

Same as previous release.

LIST OF SUPPORTED CHASSIS COMMANDS

Same as previous release.

LIST OF SUPPORTED INTEL SPECIFIC COMMANDS (0x32)

Same as previous release.

LIST OF SUPPORTED BRIDGE COMMANDS

Same as previous release.

SUPPORTED SENSORS

Sensor#      	Sensor Name

Same as previous release. 

HEX IMAGE INFORMATION

OP CHECKSUM:  	0xC910	Start Address 0x00030000 ->  End Address  0x00076D02
BOOT CHECKSUM:	0x8CA7	Start Address 0x00000000 ->  End Address  0x00001CA2
PIA CHECKSUM:	0x5D6A	Start Address 0x00008000 ->  End Address  0x00008B55

HEX CODE FILE:  T2BMC09.HEX   04/14/03   722,811 bytes

INFOBLOCK INFORMATION RETURNED BY: FWUPDATE T2BMC09.HEX /INFOBLOCK

OP CHECKSUM:			0x7959 	(DIB ONLY)
BOOT CHECKSUM:			0x9898	(DIB ONLY)
PIA HEADER CHECKSUM:	0x37D8	(DIB ONLY)

REVISION INFORMATION RETURNED BY: FWUPDATE /FWVERSION

Op Code:		v00.09
Boot Code:		v80.14
PIA version: 		1
PIA instance: 		9

FILE VERSION TAGS
ACPIEC_VER		= v0.26	
ALERT_VER		= v0.54.2	
BOOT_VER		= v0.19	
CHANNEL_VER		= v0.47  	
COMMON_VER		= v0.14  	
CPU_VER			= v0.51.3 	
DEBUG_VER		= v0.09	
DRIVERS_VER		= v0.14	
EMP_VER			= v0.62.3	
EXTERNAL_VER	= v0.64.1	
ICMB_VER		= v0.29.1	
IPMB_VER		= v0.25	
IPMI_VER		= v0.61.3	
KCS_VER			= v0.39.1	
LAN_VER			= v0.52	
MEMALLOC_VER	= v0.42 	
MEMERR_VER		= v0.62	
MISC_VER		= v0.64	
NVSTORE_VER		= v0.56	
OS_VER			= v0.08	
PIA_VER			= v0.17	
PLATFORM_VER	= v0.09
POWER_VER		= v0.64.1	
SAHALEE_VER		= v0.39.1	
SCANNING_VER	= v0.51	
SENSORIPMI_VER	= v0.55	
SENSORS_VER		= v0.35	
SESSION_VER		= v0.49.2	
USERINTF_VER	= v0.25	
UTILITIES_VER	= v0.41	
TMODE_VER		= v0.10	

TOOLS USED IN BUILD
getbmc.bat	version 1.5
gmake		Version 3.79.1
get 		v6.6.10
PVCS		version 6.6
ARM tools	version 2.51
PKZIP		v2.50

----------------------------------------------------------------------------
RELEASE NOTES FOR Tiger2 BMC RELEASE  0.08 - Beta 1
March 11, 2003 

*** Important Note: ***
- This BMC08 is the Beta Candidate Release and meant for Beta System or higher only.
- Updating to this version from BMC 0.01 require Boot Block update.
  Use jumper J3A3 on the MB and switch FROM default 1-2 (Boot protected) TO 
  2-3 (Boot programmable) 
- SDR06 should be used with this BMC version.
      
CHANGES SINCE PREVIOUS VERSION (VER 0.07)
**NEW**
- New Multi Zone Fan Speed Control system
  Refer to "Thermal and Acoustics System Description" Ver 0.6 Dated: Jan 24, 2003
  New SDR (SDR06) to go with for configuring the Fan control system.
**NEW**
- New Front Panel LED Driver and system behaviour based on OEM selection.
  Refer to Cross Platform Features - Front Panel Standards 1.1
**NEW**
- Tiger4 late bug fixes (from BMC17, 18, & 19) are included as much as possible for 
  an early testing and exposure.

- Bug Fixes:
- New SDR and FRU file updates.
  - SDR06 under FRUSDR 2.0.06 package.

* IPMI 1.5 core bug and Platform Specific bug fixes in this release.  

  32700: "Thermal trip on CPU2's line (CPU2 not populated) causes a thermal trip on CPU1"
  32825: "BMC fails to dial up when alerting to the dial page."
  32855: "Pager communication does not work."
  32858: "No response to 'Sessionless' commands via serial"
  32859: "No SOL data when Serial Channel is enabled"
  32838: "BMC09 No SEL event generated with single processor and FRB3 timeout, but beeps."
  32852: "BAD PIROM on PROC not logged"
  32158: "Sensors 0x25 and 0x26 seemed to be tied to the same part."  
  32708: "FRB3: With 1 CPU the BMC ignores the FRB3 error."
  32694: "Tach Fan in Boost with no temp triggered"
  32707: "Secure Mode Setting to prevent disk write not functioning"
  32709: "FRB3:  System doesn't always boot completely after an FRB3 error"
  32806: "Hot swap replacement of power supply causes fans to operate in wrong setting"
  32834: "Pulling out a hotswap fan puts multiple Fan #3x Lower critical assertions"
  32604: "Sensor 23 providing SEL event across AC power cycles"  
  31595: "BMC Lun10b Routing fails for message sent via Master Write-Read I2C"

  //
  // Issues & resolution from Tiger 4 migrated to T2.
  //
  32823: "Failed return value of Activate SOL Command."
  32824: "PEF Module sometimes takes action when OEM SEL Record is logged."
  32826: "Firmware- default password shouldn't be encrypted" 
  32827: "AlertManager - BMC does not generate the alert when SEL is full."
  32828: "SOL - SOL redirection message becomes undecodable"
  32829: "BMC:  SM signal support and definition"
  32830: "Gen Fault LED not controllable with SetSMSignal command"
  32831: "BMC: ACPI status not working properly"
  32837: "COM2 not functional while BMC in Update mode"
  32838: "BMC09 No SEL event generated with single processor and FRB3 timeout, but beeps."
  32840: "BMC:  Processor fan boost sensors read zero for uninstalled processors."
  32852: "BAD PIROM on PROC not logged"
  32853: "Processor temps don't come out of Non Critical state."
  32858: "No response to 'Sessionless' commands via serial"
  32859: "No SOL data when Serial Channel is enabled"
  32849: "Receive Message flag is prematurely deasserted"

DEPENDENCIES 

* PLD code for PLD 1 and PLD 2 must be the latest version for the PLD update 
  feature to work. Contact Hardware DE for PLD code.
  (PLD files can be extracted from \\esvdp01\common\Proj\Tiger2\Technical_Data\Boardset\PLDs\Alpha)

* This version of BMC has the following features enabled.
- Enabled for 1MB flash part.
- FRB
- PLD Update  
- All sensors (as indicated in the SDR03) 
- EMP and EMP mux switching function.
- Serial Over LAN - (SOL)
- Terminal Mode (TM)
- Command Line Interface (CLI)
- Multi Zone Fan Speed Control
- Front Panel LED Behaviour based on OEM selection.

KNOWN ISSUES 

* The Hurdle Test was Run on this version and no critical issues were found.

LIST OF SUPPORTED APPLICATION COMMANDS

Same as previous release.

LIST OF SUPPORTED SENSOR/EVENT COMMANDS

Same as previous release.

LIST OF SUPPORTED FIRMWARE TRANSFER COMMANDS

Same as previous release.

LIST OF SUPPORTED CHASSIS COMMANDS

Same as previous release.

LIST OF SUPPORTED INTEL SPECIFIC COMMANDS (0x32)

Same as previous release.
- Added GetChassisModelSetting command 0x41 to retireve OEM selection from BMC.

LIST OF SUPPORTED BRIDGE COMMANDS

Same as previous release.

SUPPORTED SENSORS

Sensor#      	Sensor Name

Same as previous release. 

HEX IMAGE INFORMATION

OP CHECKSUM:  	0xC910	Start Address 0x00030000 ->  End Address  0x00076D02
BOOT CHECKSUM:	0x2FEA	Start Address 0x00000000 ->  End Address  0x00001C22
PIA CHECKSUM:	0x5D6A	Start Address 0x00008000 ->  End Address  0x00008B55

HEX CODE FILE:  T2BMC08.HEX   03/11/03  722,503  bytes

INFOBLOCK INFORMATION RETURNED BY: FWUPDATE T2BMC08.HEX /INFOBLOCK

OP CHECKSUM:		0xA914  	(DIB ONLY)
BOOT CHECKSUM:		0x8858	(DIB ONLY)
PIA HEADER CHECKSUM:	0x38D8	(DIB ONLY)

REVISION INFORMATION RETURNED BY: FWUPDATE /FWVERSION

Op Code:		v00.08
Boot Code:		v80.13
PIA version: 	1
PIA instance: 	8

FILE VERSION TAGS
ACPIEC_VER		= v0.26	
ALERT_VER		= v0.54.2	
BOOT_VER		= v0.19	
CHANNEL_VER		= v0.47  	
COMMON_VER		= v0.14  	
CPU_VER		= v0.51.3 	
DEBUG_VER		= v0.09	
DRIVERS_VER		= v0.14	
EMP_VER		= v0.62.3	
EXTERNAL_VER	= v0.64.1	
ICMB_VER		= v0.29.1	
IPMB_VER		= v0.25	
IPMI_VER		= v0.61.3	
KCS_VER		= v0.39.1	
LAN_VER		= v0.52	
MEMALLOC_VER	= v0.42 	
MEMERR_VER		= v0.62	
MISC_VER		= v0.64	
NVSTORE_VER		= v0.56	
OS_VER		= v0.08	
PIA_VER		= v0.17	
PLATFORM_VER	= v0.08
POWER_VER		= v0.64.1	
SAHALEE_VER		= v0.39.1	
SCANNING_VER	= v0.51	
SENSORIPMI_VER	= v0.55	
SENSORS_VER		= v0.35	
SESSION_VER		= v0.49.2	
USERINTF_VER	= v0.25	
UTILITIES_VER	= v0.41	
TMODE_VER		= v0.10	

TOOLS USED IN BUILD
getbmc.bat	version 1.5
gmake		Version 3.79.1
get 		v6.6.10
PVCS		version 6.6
ARM tools	version 2.51
PKZIP		v2.50

----------------------------------------------------------------------------
RELEASE NOTES FOR Tiger2 BMC RELEASE  0.07 - Beta
February 25, 2003 

*** Important Note: ***
- Updating to this version from BMC 0.01 require Boot Block update.
  Use jumper J3A3 on the MB and switch FROM default 1-2 (Boot protected) TO 
  2-3 (Boot programmable) 
- SDR05 should be used with this BMC version.
      
CHANGES SINCE PREVIOUS VERSION (VER 0.06)
**NEW**
- New Multi Zone Fan Speed Control system
  Refer to "Thermal and Acoustics System Description" Ver 0.6 Dated: Jan 24, 2003
  New SDR (SDR05) to go with for configuring the Fan control system.
**NEW**
- New Front Panel LED Driver and system behaviour
  Refer to Cross Platform Features - Front Panel Standards 1.1
  
- Bug Fixes:

- New SDR and FRU file updates.

* IPMI 1.5 core bug fixes.  
  NONE 

* Platform Specific trackers fixed in this release:
  - "Tracker#31594 - AC Cycle causes unexpected SEL events.
  - "Tracker#31599 - FRU: PCI Riser FRU file does not load on fab 2.
  - "Tracker#31601 - BMC: Sensors out of normal range under normal conditions.
  - "Tracker#32119 - SEL: SEL Clear returns 0xFF when erase in progress.




DEPENDENCIES 

* PLD code for PLD 1 and PLD 2 must be the latest version for the PLD update 
  feature to work. Contact Hardware DE for PLD code.
  (PLD files can be extracted from \\esvdp01\common\Proj\Tiger2\Technical_Data\Boardset\PLDs\Alpha)

* This version of BMC has the following features enabled.
- Enabled for 1MB flash part.
- FRB
- PLD Update  
- All sensors (as indicated in the SDR03) 
- EMP and EMP mux switching function.
- Serial Over LAN - (SOL)
- Terminal Mode (TM)
- Command Line Interface (CLI)
- Multi Zone Fan Speed Control
- Front Panel LED Behaviour

KNOWN ISSUES 

* The Hurdle Test was Run on this version and the no critical issues were found.

LIST OF SUPPORTED APPLICATION COMMANDS

Same as previous release.

LIST OF SUPPORTED SENSOR/EVENT COMMANDS

Same as previous release.

LIST OF SUPPORTED FIRMWARE TRANSFER COMMANDS

Same as previous release.

LIST OF SUPPORTED CHASSIS COMMANDS

Same as previous release.

LIST OF SUPPORTED INTEL SPECIFIC COMMANDS

Same as previous release.

LIST OF SUPPORTED BRIDGE COMMANDS

Same as previous release.

SUPPORTED SENSORS

Sensor#      	Sensor Name

Same as previous release. 

HEX IMAGE INFORMATION

OP CHECKSUM:  	0x73D0	Start Address 0x00030000 ->  End Address  0x00076C2A
BOOT CHECKSUM:	0x2FEA	Start Address 0x00000000 ->  End Address  0x00001C22
PIA CHECKSUM:	0xE7DB	Start Address 0x00008000 ->  End Address  0x00008B2D

HEX CODE FILE:  T2BMC07.HEX   02/25/03  721,903  bytes

INFOBLOCK INFORMATION RETURNED BY: FWUPDATE T2BMC07.HEX /INFOBLOCK

OP CHECKSUM:		0x8248  (DIB ONLY)
BOOT CHECKSUM:		0x982F	(DIB ONLY)
PIA HEADER CHECKSUM:	0xAFDF	(DIB ONLY)

REVISION INFORMATION RETURNED BY: FWUPDATE /FWVERSION

Op Code:	v00.07
Boot Code:	v80.13
PIA version: 	1
PIA instance: 	5

FILE VERSION TAGS
ACPIEC_VER		= 	v0.26
ALERT_VER		= 	v0.54
BOOT_VER		= 	v0.19
CHANNEL_VER		= 	v0.47
COMMON_VER		= 	v0.14
CPU_VER			= 	v0.51
DEBUG_VER		= 	v0.09
DRIVERS_VER		= 	v0.14
EMP_VER			= 	v0.62
EXTERNAL_VER		= 	v0.64
ICMB_VER		= 	v0.29
IPMB_VER		= 	v0.25
IPMI_VER		= 	v0.61
KCS_VER			= 	v0.39.1
LAN_VER			= 	v0.52
MEMALLOC_VER		= 	v0.42
MEMERR_VER		= 	v0.62
MISC_VER		= 	v0.64
NVSTORE_VER		= 	v0.56
OS_VER			= 	v0.08
PIA_VER			= 	v0.17
PLATFORM_VER		= 	v0.07
POWER_VER		= 	v0.64
SAHALEE_VER		= 	v0.39
SCANNING_VER		= 	v0.51
SENSORIPMI_VER		= 	v0.55
SENSORS_VER		= 	v0.35
SESSION_VER		= 	v0.49
USERINTF_VER		= 	v0.25
UTILITIES_VER		= 	v0.41
TMODE_VER		= 	v0.10

TOOLS USED IN BUILD
getbmc.bat	version 1.5
gmake		Version 3.79.1
get 		v6.6.10
PVCS		version 6.6
ARM tools	version 2.51
PKZIP		v2.50

-----------------------------------------------------------------------------------------------


RELEASE NOTES FOR Tiger2 BMC RELEASE  0.06 - ALPHA3
February 6, 2003 (ww6.4) 

*** Important Note: ***
- Previous release of BMC namely, BMC-05 has been withdrawn. This release will 
  be derelicted.
- BMC04 has been substituted with this release of BMC06 to support and meet the 
  HSC-05's timing needs.  BMC04 will retire though it will work with HSC03 (T4 HSC)
- BMC04 should be abandoned and all ALPHA system users should jump to BMC06 with an 
  important note to "SEEK HSC-05 FLASH PART" from the program (Contact Ken Lee).
- SDR03+ should be used with this BMC version.
- Sensor #1D (SNSR_MB_5V_SB), #21(SNSR_MAIN_SNC_TEMP), #22(SNSR_MAIN_SIOH_TEMP) 
  disabled due to hardware issue.  Needs Fab3 MB board to enable.
- Updating to this version from BMC 0.01 require Boot Block update.
  Use jumper J3A3 on the MB and switch FROM default 1-2 (Boot protected) TO 
  2-3 (Boot programmable) 
      
CHANGES SINCE PREVIOUS VERSION (VER 0.04)
**NEW**
- Added the much needed time delay for HSC to come out of Reset and talk to BMC
  succcessfully without going out in the weeds. (Long term solution in the works w/ Qlogic)
  
- Bug Fixes:

- New SDR and FRU file updates.

* IPMI 1.5 core bug fixes.  
  NONE 

* Platform Specific trackers fixed in this release:
  - "Tracker#32268 - Sev1 - HSC Firmware Stuck in FWTransfere mode.

DEPENDENCIES 

* PLD code for PLD 1 and PLD 2 must be the latest version for the PLD update 
  feature to work. Contact Hardware DE for PLD code.
  (PLD files can be extracted from \\esvdp01\common\Proj\Tiger2\Technical_Data\Boardset\PLDs\Alpha)

* This 0.05 version of BMC has the following features enabled.
- Enabled for 1MB flash part.
- FRB 
- All sensors (as indicated in the SDR03) 
- EMP and EMP mux switching function.
- Serial Over LAN - (SOL)
- Terminal Mode (TM)
- Command Line Interface (CLI)

KNOWN ISSUES 

* The Hurdle Test was Run on this version and the no critical issues were found.

LIST OF SUPPORTED APPLICATION COMMANDS

Same as previous release.

LIST OF SUPPORTED SENSOR/EVENT COMMANDS

Same as previous release.

LIST OF SUPPORTED FIRMWARE TRANSFER COMMANDS

Same as previous release.

LIST OF SUPPORTED CHASSIS COMMANDS

Same as previous release.

LIST OF SUPPORTED INTEL SPECIFIC COMMANDS

Same as previous release.

LIST OF SUPPORTED BRIDGE COMMANDS

Same as previous release.

SUPPORTED SENSORS

Sensor#      	Sensor Name

Same as previous release except for sensor #1D, #21, and #22. These are disabled.

HEX IMAGE INFORMATION

OP CHECKSUM:  	0xCEE8	Start Address 0x00030000 ->  End Address  0x0007687E
BOOT CHECKSUM:	0x2FEA	Start Address 0x00000000 ->  End Address  0x00001C22
PIA CHECKSUM:	0x2696	Start Address 0x00008000 ->  End Address  0x00008AF5

HEX CODE FILE:  T2BMC06.HEX   02/06/03  719,479  bytes

INFOBLOCK INFORMATION RETURNED BY: FWUPDATE T2BMC06.HEX /INFOBLOCK

OP CHECKSUM:			0x8CEE  (DIB ONLY)
BOOT CHECKSUM:			0xA627	(DIB ONLY)
PIA HEADER CHECKSUM:	0x8CEE	(DIB ONLY)

REVISION INFORMATION RETURNED BY: FWUPDATE /FWVERSION

Op Code:	v00.06
Boot Code:	v80.13
PIA version: 	1
PIA instance: 	6

FILE VERSION TAGS
ACPIEC_VER		= 	v0.26
ALERT_VER		= 	v0.54
BOOT_VER		= 	v0.19
CHANNEL_VER		= 	v0.47
COMMON_VER		= 	v0.14
CPU_VER			= 	v0.51
DEBUG_VER		= 	v0.09
DRIVERS_VER		= 	v0.14
EMP_VER			= 	v0.62
EXTERNAL_VER	= 	v0.64
ICMB_VER		= 	v0.29
IPMB_VER		= 	v0.25
IPMI_VER		= 	v0.61
KCS_VER			= 	v0.39.1
LAN_VER			= 	v0.52
MEMALLOC_VER	= 	v0.42
MEMERR_VER		= 	v0.62
MISC_VER		= 	v0.64
NVSTORE_VER		= 	v0.56
OS_VER			= 	v0.08
PIA_VER			= 	v0.17
PLATFORM_VER	= 	v0.06
POWER_VER		= 	v0.64
SAHALEE_VER		= 	v0.39
SCANNING_VER	= 	v0.51
SENSORIPMI_VER	= 	v0.55
SENSORS_VER		= 	v0.35
SESSION_VER		= 	v0.49
USERINTF_VER	= 	v0.25
UTILITIES_VER	= 	v0.41
TMODE_VER		= 	v0.10

TOOLS USED IN BUILD
getbmc.bat	version 1.5
gmake		Version 3.79.1
get 		v6.6.10
PVCS		version 6.6
ARM tools	version 2.51
PKZIP		v2.50

----------------------------------------------------------------------------
RELEASE NOTES FOR Tiger2 BMC RELEASE  0.05 - ALPHA3
February 3, 2003 (ww6.1) 

*** Important Note: ***
- Updating to this version from BMC 0.01 require Boot Block update.
  Use jumper J3A3 on the MB and switch FROM default 1-2 (Boot protected) TO 
  2-3 (Boot programmable) 
- SDR04 should be used with this BMC version.
- Sensor #1D (SNSR_MB_5V_SB), #21(SNSR_MAIN_SNC_TEMP), #22(SNSR_MAIN_SIOH_TEMP) 
  disabled due to hardware issue.  Needs Fab3 MB board to enable.
      
CHANGES SINCE PREVIOUS VERSION (VER 0.04)
**NEW**
- New Multi Zone Fan Speed Control system
  Refer to "Thermal and Acoustics System Description" Ver 0.6 Dated: Jan 24, 2003
  New SDR (SDR04) to go with for configuring the Fan control system.
**NEW**
- New Front Panel LED Driver and system behaviour
  Refer to Cross Platform Features - Front Panel Standards 1.1
  
- Bug Fixes:

- New SDR and FRU file updates.

* IPMI 1.5 core bug fixes.  
  NONE 

* Platform Specific trackers fixed in this release:
  - "Tracker#31594 - AC Cycle causes unexpected SEL events.
  - "Tracker#31599 - FRU: PCI Riser FRU file does not load on fab 2.
  - "Tracker#31601 - BMC: Sensors out of normal range under normal conditions.
  - "Tracker#32119 - SEL: SEL Clear returns 0xFF when erase in progress.

DEPENDENCIES 

* PLD code for PLD 1 and PLD 2 must be the latest version for the PLD update 
  feature to work. Contact Hardware DE for PLD code.
  (PLD files can be extracted from \\esvdp01\common\Proj\Tiger2\Technical_Data\Boardset\PLDs\Alpha)

* This 0.05 version of BMC has the following features enabled.
- Enabled for 1MB flash part.
- FRB 
- All sensors (as indicated in the SDR03) 
- EMP and EMP mux switching function.
- Serial Over LAN - (SOL)
- Terminal Mode (TM)
- Command Line Interface (CLI)
- Multi Zone Fan Speed Control
- Front Panel LED Behaviour

KNOWN ISSUES 

* The Hurdle Test was Run on this version and the no critical issues were found.

LIST OF SUPPORTED APPLICATION COMMANDS

Same as previous release.

LIST OF SUPPORTED SENSOR/EVENT COMMANDS

Same as previous release.

LIST OF SUPPORTED FIRMWARE TRANSFER COMMANDS

Same as previous release.

LIST OF SUPPORTED CHASSIS COMMANDS

Same as previous release.

LIST OF SUPPORTED INTEL SPECIFIC COMMANDS

Same as previous release.

LIST OF SUPPORTED BRIDGE COMMANDS

Same as previous release.

SUPPORTED SENSORS

Sensor#      	Sensor Name

Same as previous release except for sensor #1D, #21, and #22. These are disabled.

HEX IMAGE INFORMATION

OP CHECKSUM:  	0xC4BD	Start Address 0x00030000 ->  End Address  0x00076BF6
BOOT CHECKSUM:	0x2FEA	Start Address 0x00000000 ->  End Address  0x00001C22
PIA CHECKSUM:	0xE7DB	Start Address 0x00008000 ->  End Address  0x00008B2D

HEX CODE FILE:  T2BMC05.HEX   02/03/03  721,773  bytes

INFOBLOCK INFORMATION RETURNED BY: FWUPDATE T2BMC05.HEX /INFOBLOCK

OP CHECKSUM:		0x8976  (DIB ONLY)
BOOT CHECKSUM:		0x9F27	(DIB ONLY)
PIA HEADER CHECKSUM:	0xB1DF	(DIB ONLY)

REVISION INFORMATION RETURNED BY: FWUPDATE /FWVERSION

Op Code:	v00.05
Boot Code:	v80.13
PIA version: 	1
PIA instance: 	5

FILE VERSION TAGS
ACPIEC_VER		= 	v0.26
ALERT_VER		= 	v0.54
BOOT_VER		= 	v0.19
CHANNEL_VER		= 	v0.47
COMMON_VER		= 	v0.14
CPU_VER			= 	v0.51
DEBUG_VER		= 	v0.09
DRIVERS_VER		= 	v0.14
EMP_VER			= 	v0.62
EXTERNAL_VER		= 	v0.64
ICMB_VER		= 	v0.29
IPMB_VER		= 	v0.25
IPMI_VER		= 	v0.61
KCS_VER			= 	v0.39.1
LAN_VER			= 	v0.52
MEMALLOC_VER		= 	v0.42
MEMERR_VER		= 	v0.62
MISC_VER		= 	v0.64
NVSTORE_VER		= 	v0.56
OS_VER			= 	v0.08
PIA_VER			= 	v0.17
PLATFORM_VER		= 	v0.05
POWER_VER		= 	v0.64
SAHALEE_VER		= 	v0.39
SCANNING_VER		= 	v0.51
SENSORIPMI_VER		= 	v0.55
SENSORS_VER		= 	v0.35
SESSION_VER		= 	v0.49
USERINTF_VER		= 	v0.25
UTILITIES_VER		= 	v0.41
TMODE_VER		= 	v0.10

TOOLS USED IN BUILD
getbmc.bat	version 1.5
gmake		Version 3.79.1
get 		v6.6.10
PVCS		version 6.6
ARM tools	version 2.51
PKZIP		v2.50

-----------------------------------------------------------------------------------------------

RELEASE NOTES FOR Tiger2 BMC RELEASE  0.04 - ALPHA2
January 20, 2003 (ww4.1) 

Note: - BMC03 has been ABANDONED due to Processors going Off-line. Refer to 
        Tracker#32229
      - Updating to this version from BMC 0.01 require Boot Block update.
      
CHANGES SINCE PREVIOUS VERSION (VER 0.03)
Previous BMC03 has been abandoned due to Processors going Off-line. Refer to 
Tracker#32229
This is the third ALPHA 2 Release since Tiger2 resurection. This is still the 
Initial Version of firmware for BMC Tiger2.

* IPMI 1.5 core bug fixes.  

NONE - Initial release.

* Platform Specific trackers fixed in this release:
  "Tracker#32229  CPU lost when doing a fwupdate verify and soft reset"
  resolved since last release.

DEPENDENCIES 

* PLD code for PLD 1 and PLD 2 must be the latest version for the PLD update 
  feature to work. Contact Hardware DE for PLD code.
  (PLD files can be extracted from \\esvdp01\common\Proj\Tiger2\Technical_Data\Boardset\PLDs\Alpha)

* This 0.04 version of BMC has the following features enabled.
 - Enabled for 1MB flash part.
 - FRB 
 - All sensors (as indicated in the SDR03) 
 - EMP and EMP mux switching function.
 - Serial Over LAN - (SOL)
 - Terminal Mode (TM)
 - Command Line Interface (CLI)

KNOWN ISSUES 

* The Hurdle Test was Run on this version and the known issues are as follows;
  - LEDs are as per Cross Platform Features 1.1 specification and not implemented
    yet.  Will be available in Alpha3 release.
  - Fan Management per Thermal and Accoustic specification is not implemented yet.

LIST OF SUPPORTED APPLICATION COMMANDS

Same as previous release.

LIST OF SUPPORTED SENSOR/EVENT COMMANDS

Same as previous release.

LIST OF SUPPORTED FIRMWARE TRANSFER COMMANDS

Same as previous release.

LIST OF SUPPORTED CHASSIS COMMANDS

Same as previous release.

LIST OF SUPPORTED INTEL SPECIFIC COMMANDS

Same as previous release.

LIST OF SUPPORTED BRIDGE COMMANDS

Same as previous release.

SUPPORTED SENSORS

Sensor#      	Sensor Name

Same as previous release.

HEX IMAGE INFORMATION

OP CHECKSUM:  	0xDD09	Start Address 0x00030000 ->  End Address  0x00076852
BOOT CHECKSUM:	0x30EA	Start Address 0x00000000 ->  End Address  0x00001C22
PIA CHECKSUM:	0x2696	Start Address 0x00008000 ->  End Address  0x00008AF5

HEX CODE FILE:  T2BMC04.HEX   01/20/03  719,378  bytes

INFOBLOCK INFORMATION RETURNED BY: FWUPDATE T2BMC04.HEX /INFOBLOCK

OP CHECKSUM:			0x9313  (DIB ONLY)
BOOT CHECKSUM:			0xB01D	(DIB ONLY)
PIA HEADER CHECKSUM:	0x7460	(DIB ONLY)

REVISION INFORMATION RETURNED BY: FWUPDATE /FWVERSION

Op Code:	v00.04
Boot Code:	v80.13
PIA version: 	1
PIA instance: 	4

FILE VERSION TAGS
ACPIEC_VER		= 	v0.26
ALERT_VER		= 	v0.54
BOOT_VER		= 	v0.19
CHANNEL_VER		= 	v0.47
COMMON_VER		= 	v0.14
CPU_VER			= 	v0.51
DEBUG_VER		= 	v0.09
DRIVERS_VER		= 	v0.14
EMP_VER			= 	v0.62
EXTERNAL_VER  	= 	v0.64
ICMB_VER		= 	v0.29
IPMB_VER		= 	v0.25
IPMI_VER		= 	v0.61
KCS_VER			= 	v0.39.1
LAN_VER			= 	v0.52
MEMALLOC_VER  	= 	v0.42
MEMERR_VER		= 	v0.62
MISC_VER		= 	v0.64
NVSTORE_VER		= 	v0.56
OS_VER			= 	v0.08
PIA_VER			= 	v0.17
PLATFORM_VER  	= 	v0.04
POWER_VER		= 	v0.64
SAHALEE_VER		= 	v0.39
SCANNING_VER  	= 	v0.51
SENSORIPMI_VER	= 	v0.55
SENSORS_VER		= 	v0.35
SESSION_VER		= 	v0.49
USERINTF_VER  	= 	v0.25
UTILITIES_VER 	= 	v0.41
TMODE_VER		= 	v0.10

TOOLS USED IN BUILD
getbmc.bat	version 1.5
gmake		Version 3.79.1
get 		v6.6.10
PVCS		version 6.6
ARM tools	version 2.51
PKZIP		v2.50

-----------------------------------------------------------------------------------------------
RELEASE NOTES FOR Tiger2 BMC RELEASE  0.03 - ALPHA2
December 13, 2002 (ww50.5) 
Revised - N/A

Note: Updating to this version from BMC 0.01 require Boot Block update.

CHANGES SINCE PREVIOUS VERSION (VER 0.02)
This is the Second ALPHA 2 Release since Tiger2 resurection. This is still the 
Initial Version of firmware for BMC Tiger2.

* IPMI 1.5 core bug fixes.  

NONE - Initial release.

* Platform Specific trackers fixed in this release:

None - Initial release.

DEPENDENCIES 

* PLD code for PLD 1 and PLD 2 must be the latest version for the PLD update 
  feature to work. Contact Hardware DE for PLD code.
  (PLD files can be extracted from \\esvdp01\common\Proj\Tiger2\Technical_Data\Boardset\PLDs\Alpha)

* This 0.03 version of BMC has the following features enabled.
 - Enabled for 1MB flash part.
 - FRB 
 - All sensors (as indicated in the SDR03) 
 - EMP and EMP mux switching function.
 - Serial Over LAN - (SOL)
 - Terminal Mode (TM)
 - Command Line Interface (CLI)

KNOWN ISSUES 

* The Hurdle Test was Run on this version and the known issues are as follows;
  - LEDs are as per Cross Platform Features 1.1 specification and not implemented
    yet.  Will be available in Alpha3 release.

LIST OF SUPPORTED APPLICATION COMMANDS

Same as previous release.

LIST OF SUPPORTED SENSOR/EVENT COMMANDS

Same as previous release.

LIST OF SUPPORTED FIRMWARE TRANSFER COMMANDS

Same as previous release.

LIST OF SUPPORTED CHASSIS COMMANDS

Same as previous release.

LIST OF SUPPORTED INTEL SPECIFIC COMMANDS

Same as previous release.

LIST OF SUPPORTED BRIDGE COMMANDS

Same as previous release.

SUPPORTED SENSORS

Sensor#      	Sensor Name

Same as previous release.

HEX IMAGE INFORMATION

OP CHECKSUM:  	0x82E7	Start Address 0x00030000 ->  End Address  0x00076882
BOOT CHECKSUM:	0x30EA	Start Address 0x00000000 ->  End Address  0x00001C22
PIA CHECKSUM:	0x2696	Start Address 0x00008000 ->  End Address  0x00008AF5

HEX CODE FILE:  T2BMC03.HEX   12/13/02  719,269  bytes

INFOBLOCK INFORMATION RETURNED BY: FWUPDATE T2BMC02.HEX /INFOBLOCK

OP CHECKSUM:		0x8E4D  (DIB ONLY)
BOOT CHECKSUM:		0xAC27  (DIB ONLY)
PIA HEADER CHECKSUM:	0x7560	(DIB ONLY)

REVISION INFORMATION RETURNED BY: FWUPDATE /FWVERSION

Op Code:	v00.03
Boot Code:	v80.13
PIA version: 	1
PIA instance: 	3

FILE VERSION TAGS
ACPIEC_VER		= 	v0.26
ALERT_VER		= 	v0.54
BOOT_VER		= 	v0.19
CHANNEL_VER		= 	v0.47
COMMON_VER		= 	v0.14
CPU_VER			= 	v0.51
DEBUG_VER		= 	v0.09
DRIVERS_VER		= 	v0.14
EMP_VER			= 	v0.62
EXTERNAL_VER		= 	v0.64
ICMB_VER		= 	v0.29
IPMB_VER		= 	v0.25
IPMI_VER		= 	v0.61
KCS_VER			= 	v0.39.1
LAN_VER			= 	v0.52
MEMALLOC_VER		= 	v0.42
MEMERR_VER		= 	v0.62
MISC_VER		= 	v0.64
NVSTORE_VER		= 	v0.56
OS_VER			= 	v0.08
PIA_VER			= 	v0.17
PLATFORM_VER		= 	v0.03
POWER_VER		= 	v0.64
SAHALEE_VER		= 	v0.39
SCANNING_VER		= 	v0.51
SENSORIPMI_VER		= 	v0.55
SENSORS_VER		= 	v0.35
SESSION_VER		= 	v0.49
USERINTF_VER		= 	v0.25
UTILITIES_VER		= 	v0.41
TMODE_VER		= 	v0.10

TOOLS USED IN BUILD
getbmc.bat	version 1.5
gmake		Version 3.79.1
get 		v6.6.10
PVCS		version 6.6
ARM tools	version 2.51
PKZIP		v2.50

-----------------------------------------------------------------------------------------------
RELEASE NOTES FOR Tiger2 BMC RELEASE  0.02 - ALPHA1 
November 22, 2002 (ww47.5) Revised November 25, 2002 (ww48.1)

Note: Updating to this version from BMC 0.01 require Boot Block update.

CHANGES SINCE PREVIOUS VERSION (VER 0.01)
This is the initial ALPHA (PowerOn) 1 Release since Tiger2 resurection.

* IPMI 1.5 core bug fixes.  

NONE

* Platform Specific trackers fixed in this release:

None

DEPENDENCIES 

* PLD code for PLD 1 and PLD 2 must be the latest version for the PLD update 
  feature to work. Contact Hardware DE for PLD code.
  (PLD files can be extracted from \\esvdp01\common\Proj\Tiger2\Technical_Data\Boardset\PLDs\Alpha)

* This 0.02 version of BMC has the following features enabled.
 - Nov 25 revision - Enabled for 1MB flash part. (Nov 22 release was for 512KB part)
 - FRB 
 - All sensors (as indicated in the SDR02) except PDB sensors are enabled.
	- PDB sensors are Fan sensors (Tach and Presence), and Power Supply sensors.
	  This is due to the fact that PDB is not available until WW49
 - EMP and EMP mux switching function.
 - Serial Over LAN - (SOL)
 - Terminal Mode (TM)
 - Command Line Interface (CLI)

KNOWN ISSUES 

* The Hurdle Test was Run on this version and the known issues are as follows;
  - LEDs are as per Cross Platform Features 1.1 specification and not implemented
    yet.  Will be available in Alpha3 release.

IOL

ActSessCmd    0x06    0x3A   0x0100   Unknown      No       0     6359
GetLEDStatus  0x32    0x40   0x0104   Unknown     Yes       0       62

IOS

GetLEDStatus  0x32    0x40   0x0104   Unknown     Yes       0       32

SMS

GetLEDStatus  0x32    0x40   0x0104   Unknown     Yes       0       16

I2C Full Test

UndefinedCommand  0x30    0x84     0xFF    Broken      No      10       16
UndefinedCommand  0x30    0x85     0xFF    Broken      No      24       31
  

LIST OF SUPPORTED APPLICATION COMMANDS

01h	Get Device ID
04h	Get Self Test Results
06h	Set ACPI Power State - cmd is avail, but full functionality not guaranteed
07h	Get ACPI Power State
22h	Reset Watchdog Timer
24h	Set Watchdog Timer
25h	Get Watchdog Timer
2Eh	Set BMC Global Enables
2Fh	Get BMC Global Enables
30h	Clear Message Flags
31h	Get Message Flags
33h	Get Message
34h	Send Message
35h	Read Event Message Buffer
37h	Get System GUID
38h	Get Channel Authentication Capabilities
39h	Get Session Challenge
3Ah	Activate Session
3Bh	Set Session Privilege Level
3Ch	Close Session
3Dh	Get Session Info
3Fh	Get AuthCode
40h	Set Channel Access
41h	Get Channel Access
42h	Get Channel Info
43h	Set User Access
44h	Get User Access
45h	Set User Name
46h	Get User Name
47h	Set User Password
52h	Master Write-Read I2C

LIST OF SUPPORTED STORAGE COMMANDS

10h	Get FRU Inventory Area Info
11h	Read FRU Inventory Data
12h	Write FRU Inventory Data
20h	Get SDR Repository Info
21h	Get SDR Repository Allocation Info
22h	Reserve SDR Repository
23h	Get SDR
25h	Partial Add SDR
27h	Clear SDR Repository
28h	Get SDR Repository Time
29h	Set SDR Repository Time
2Ah	Enter SDR Repository Update Mode
2Bh	Exit SDR Repository Update Mode
2Ch	Run Initialization Agent
40h	Get SEL Info
41h	Get SEL Allocation Info
42h	Reserve SEL
43h	Get SEL Entry
44h	Add SEL Entry
45h	Partial Add SEL Entry
46h	Delete SEL Entry
47h	Clear SEL
48h	Get SEL Time
49h	Set SEL Time

LIST OF SUPPORTED SENSOR/EVENT COMMANDS

01h	Get Event Receiver
02h	Platform Event Message
10h	Get PEF Capabilities
11h	Arm PEF Postpone Timer
12h	Set PEF Configuration Parameters
13h	Get PEF Configuration Parameters
14h	Set Last Processed Event ID
15h	Get Last Processed Event ID
16h	Alert Immediate
17h	PET Acknowledge
25h	Get Sensor Hysteresis
27h	Get Sensor Threshold
29h	Get Sensor Event Enable
2Ah	Re-arm Sensor Events
2Bh	Get Sensor Event Status
2Dh	Get Sensor Reading

LIST OF SUPPORTED FIRMWARE TRANSFER COMMANDS

00	Enter Firmware Transfer Mode	
01	Firmware Program
02	Firmware Read
03	Get Firmware Range Checksum
04	Exit Firmware Transfer Mode
05	Set Program Segment

LIST OF SUPPORTED CHASSIS COMMANDS

00h	Get Chassis Capabilities
01h	Get Chassis Status
02h	Chassis Control
04h	Chassis Identify
05h	Set Chassis capabilities
06h	Set Power Restore Policy
07h	Get System Restart Cause
08h	Set System Boot Options -  cmd is avail, but full functionality not guaranteed
09h	Get System Boot Options
0Fh	Get POH Counter

LIST OF SUPPORTED INTEL SPECIFIC COMMANDS

13h	Get SM Signal
14h	Set SM Signal
16h	Read Self Test
18h	Write BMC Port
19h	Read BMC Port
1Ah	Write BMC Memory
1Bh	Read BMC Memory
1Eh	Set Secure Mode Operation - only FP buttons
1Fh	Get Secure Mode Operation
20h	Get Power Supply State
40h	Resolved IP Address
41h	Set System GUID
47h	Log POST Code
53h	Get Front Panel CMOS Clear Options
54h	Set Front Panel CMOS Clear Options
57h	Set Fault Indication
60h	Get Config Info
61h	Get Config Data
62h	Set Config Data
82h	Get ACPI Configuration Mode
83h	Set ACPI Configuration Mode
90h	Get Chassis Name
91h	Set Chassis Name
DCh	Get Current ACPI Power State
E6h	Get NMI Source
EBh	Write Miscellaneous Configuration
ECh	Read Miscellaneous Configuration
EEh	Get All SEL Entry
F7h	NMI Enable/Disable
F8h	Set POST Progress
F9h	Get POST Progress

LIST OF SUPPORTED TRANSPORT COMMANDS

01h	Set LAN Configuration Parameters
02h	Get LAN Configuration Parameters
03h	Suspend BMC ARPs
04h	Get IP/UDP/RMCP Statistics
10h	Set Serial/Modem Configuration
11h	Get Serial/Modem Configuration
12h	Set Serial/Modem Mux
18h	Serial/Modem Connection Active
19h	Callback
1Ah	Set User Callback Options
1Bh	Get User Callback Options

LIST OF SUPPORTED BRIDGE COMMANDS
00h	Get Bridge State
01h	Set Bridge State
02h	Get ICMB Address
03h	Set ICMB Address
04h	Set Bridge Proxy/Address
05h	Get Bridge Statistics
06h	Get ICMB Capabilities
07h	Clear Bridge Statistics
08h	Get Bridge Proxy Address
10h	Prepare For Discovery
11h	Get Addresses
12h	Set Discovered
13h	Get Chassis Device ID
14h	Set Chassis Device ID
20h	Bridge Request
21h	Bridge Message
30h	Get Event Count
31h	Set Event Destination
32h	Set Event Reception State
33h	Send ICMB Event Message
34h	Get Event Destination
35h	Get Event Reception State

SUPPORTED SENSORS

Sensor#      	Sensor Name

(BMC Sensors)
SNSR_PWR_UNIT_STATUS		0x01
SNSR_PWR_UNIT_REDUND		0x02
SNSR_WATCHDOG			0x03
SNSR_PLAT_SECURITY		0x04
SNSR_PHYSICAL_SECURITY		0x05
SNSR_POST_ERROR			0x06
SNSR_FP_DIAG_INT		0x07
SNSR_MEMORY			0x08
SNSR_EV_LOG_DISABLE		0x09
SNSR_SYS_EVENT			0x0A

Baseboard Voltage Sensors
SNSR_MB_1P25V			0x10	
SNSR_MB_1P5V			0x11	
SNSR_MB_1P8V			0x12	
SNSR_MB_3P3V			0x13	
SNSR_MB_3P3V_SB			0x14	
SNSR_MB_5V 			0x15	
SNSR_MB_12V 			0x16	
SNSR_MB_M12V			0x17	
Sahalee Voltage Sensors
SNSR_MB_1P2V			0x18	
SNSR_MB_1P3V			0x19	
SNSR_MB_1P5V_SB			0x1A	
SNSR_MB_2P5V			0x1B	
SNSR_MB_2P5V_SB			0x1C	
SNSR_MB_5V_SB			0x1D	

Baseboard Temperature Sensors
SNSR_MAIN_BRD_TEMP		0x20	
SNSR_MAIN_SNC_TEMP	  	0x21 	
SNSR_MAIN_SIOH_TEMP	  	0x22	
SNSR_PERI_BRD_AMB_TEMP  	0x23	
SNSR_PCI_RSR_TEMP	  	0x24	
SNSR_CPU_AREA_TEMP 		0x25	
SNSR_MEM_AREA_TEMP 		0x26	

Analog Chassis Fan Sensor
SNSR_ANALOG_FAN_1  		0x30 
SNSR_ANALOG_FAN_2  		0x31
SNSR_ANALOG_FAN_3   		0x32
SNSR_ANALOG_FAN_4   		0x33
SNSR_ANALOG_FAN_5   		0x34
SNSR_ANALOG_FAN_6   		0x35

Aliased Baseboard Temperature Sensors -- Fan Boost
SNSR_FANBST_MAIN_BRD_TEMP	0x40
SNSR_FANBST_MAIN_SNC_TEMP	0x41
SNSR_FANBST_MAIN_SIOH_TEMP	0x42
SNSR_FANBST_PERI_BRD_AMB_TEMP  	0x43
SNSR_FANBST_PCI_RSR_TEMP	0x44
SNSR_FANBST_CPU_AREA_TEMP  	0x45
SNSR_FANBST_MEM_AREA_TEMP 	0x46

SCSI Voltage Termination Sensors
SNSR_SCSIA_TERMV0		0x50
SNSR_SCSIA_TERMV1		0x51
SNSR_SCSIA_TERMV2		0x52
SNSR_SCSIB_TERMV0		0x53
SNSR_SCSIB_TERMV1		0x54
SNSR_SCSIB_TERMV2		0x55

Power Supply, D2D, PWRGD Sensors (16)
SNSR_PWRSUPPLY_1 		0x60
SNSR_PWRSUPPLY_2 		0x61
SNSR_PWRSUPPLY_3 		0x62

Power Supply Ok ORED
SNSR_PS_OK_ORED			0x63

Fan Present sensors
SNSR_FAN1_PRESENT 		0x70
SNSR_FAN2_PRESENT		0x71
SNSR_FAN3_PRESENT		0x72
SNSR_FAN4_PRESENT	  	0x73
SNSR_FAN5_PRESENT	  	0x74
SNSR_FAN6_PRESENT	  	0x75

Interlock sensors
SNSR_SYS_BRD_INTERLOCK		0x77

INIT signal state sensor
SNSR_INIT_SIGNAL_STATE		0x7A

Processor Sensors
SNSR_CPU1_STATUS		0x80
SNSR_CPU2_STATUS		0x81
SNSR_CPU1_TEMP			0x82
SNSR_CPU2_TEMP			0x83
SNSR_FANBST_CPU1	 	0x84
SNSR_FANBST_CPU2	 	0x85
SNSR_CPU1_PPOD_GD		0x86
SNSR_CPU2_PPOD_GD		0x87

Type 11h - FRU Locator record for Proc 1 SECC FRU
Type 11h - FRU Locator record for Proc 2 SECC FRU
Type 11h - FRU Locator record for Proc 1 OEM FRU
Type 11h - FRU Locator record for Proc 2 OEM FRU
Type 11h - FRU Locator record for BMC/Main Brd FRU
Type 11h - FRU Locator record for PCI Riser FRU
Type 11h - FRU Locator record for Peripheral Brd FRU

HEX IMAGE INFORMATION

OP CHECKSUM:  	0xD1EE	Start Address 0x00030000 ->  End Address  0x00076442
BOOT CHECKSUM:	0x30EA	Start Address 0x00000000 ->  End Address  0x00001C22
PIA CHECKSUM:	0x9786	Start Address 0x00008000 ->  End Address  0x00008AC9

HEX CODE FILE:  T2BMC02.HEX   11/25/02  716,805  bytes

INFOBLOCK INFORMATION RETURNED BY: FWUPDATE T2BMC02.HEX /INFOBLOCK

OP CHECKSUM:		0x8513  (DIB ONLY)
BOOT CHECKSUM:		0x940D  (DIB ONLY)
PIA HEADER CHECKSUM:	0x0678	(DIB ONLY)

REVISION INFORMATION RETURNED BY: FWUPDATE /FWVERSION

Op Code:	v00.02
Boot Code:	v80.13
PIA version: 	1
PIA instance: 	2

FILE VERSION TAGS
ACPIEC_VER		= 	v0.26
ALERT_VER		= 	v0.54
BOOT_VER		= 	v0.19
CHANNEL_VER		= 	v0.47
COMMON_VER		= 	v0.14
CPU_VER			= 	v0.51
DEBUG_VER		= 	v0.09
DRIVERS_VER		= 	v0.14
EMP_VER			= 	v0.62
EXTERNAL_VER		= 	v0.64
ICMB_VER		= 	v0.29
IPMB_VER		= 	v0.25
IPMI_VER		= 	v0.61
KCS_VER			= 	v0.39.1
LAN_VER			= 	v0.52
MEMALLOC_VER		= 	v0.42
MEMERR_VER		= 	v0.62
MISC_VER		= 	v0.64
NVSTORE_VER		= 	v0.56
OS_VER			= 	v0.08
PIA_VER			= 	v0.17
PLATFORM_VER		= 	v0.02
POWER_VER		= 	v0.64
SAHALEE_VER		= 	v0.39
SCANNING_VER		= 	v0.51
SENSORIPMI_VER		= 	v0.55
SENSORS_VER		= 	v0.35
SESSION_VER		= 	v0.49
USERINTF_VER		= 	v0.25
UTILITIES_VER		= 	v0.41
TMODE_VER		= 	v0.10

TOOLS USED IN BUILD
getbmc.bat	version 1.5
gmake		Version 3.79.1
get 		v6.6.10
PVCS		version 6.6
ARM tools	version 2.51
PKZIP		v2.50
