[English]
README.TXT             MATROX GRAPHICS INC.              2002.11.05

                Matrox PowerDesk for Windows NT 4.0 
                           Rev. 5.07.001


Contents
========

- Release description
- Installation
- Using Matrox PowerDesk
- Hardware-accelerated 3D
- Notes, problems, and limitations
- Matrox TV output


Release description
===================

This is the Matrox Windows NT Display Driver. It supports 
Microsoft Windows NT for x86 CPU's, version 4.0 (Build 1381 -- or 
later).

This product includes:

- Display driver
- Matrox PowerDesk for Windows NT 4.0


Installation
============

To install Matrox PowerDesk, start the "Setup" program included 
with it, then follow the on-screen instructions.

The setup program will only install software if a Matrox graphics 
card model supported by the setup program is installed in your 
computer.


Using Matrox PowerDesk
======================

Changing resolution, selecting a monitor, and using the Matrox 
PowerDesk is covered in the "online.doc" file. You can view this 
file with WordPad.


Hardware-accelerated 3D
=======================

For 3D hardware acceleration, the Matrox Windows NT 4.0 display 
driver supports the OpenGL interface with 2 driver types -- MCD 
("Mini Client Driver") and ICD ("Installable Client Driver"). The 
Matrox Millennium, Millennium II, Mystique, Mystique 220, and 
G100-based graphics cards have MCD support. The Matrox G200-based, 
G400-based and later graphics cards have ICD support. (An ICD has 
more potential for optimization than an MCD.)

3D hardware acceleration has the following restrictions:

- Currently no acceleration is available when multiple cards are 
  in use.

- The MCD/ICD does not support 8 bpp (256 colors) and 24 bpp 
  (16777216 colors) modes. 16 bpp (64 K colors) and 32 bpp 
  (16777216 colors) modes are the ones that can be 
  hardware-accelerated.

- Limitations to the available resolutions are to be expected. All 
  3D modes require extra memory to handle double buffering and/or 
  Z-buffering, and this memory is no longer available for display.


Notes, problems, and limitations
================================

- Service Pack 4 or later recommended

  To avoid potential problems, we recommend you install Service 
  Pack 4 (or later) for Windows NT 4.0.

- Computers with more than one PCI bus

  It is possible that a switch to a full-screen Command Prompt, or 
  any change of mode, will result in a blue-screen crash if a card 
  is installed on a PCI bus other than bus 0. The problem is under 
  investigation. Moving the card to a different PCI slot is a 
  possible workaround.

  There are systems where Windows NT reports conflicts between 
  adapters installed beyond the PCI bridge. In this case, the 
  Matrox miniport driver can't access its own card. If your system 
  appears unable to find the card, try moving it to a different 
  PCI slot.

  Installing Microsoft Service Pack 4 (or later) for Windows NT 
  4.0 should fix many of these problems.

- DirectDraw with virtual desktops

  Some DirectDraw programs don't work properly with virtual 
  desktops. We recommend you run DirectDraw programs with a normal 
  desktop.

- 3D-Maze screen saver

  Display problems may appear while using the "3D-Maze" screen 
  saver. These may happen after Microsoft Service Pack 2 for 
  Windows NT 4.0 is installed. These display problems are 
  apparently fixed by Service Pack 4 (or later).

- Running Winstone 97

  The CenterPOPUP feature should be disabled (which is the default 
  setting) when running the Winstone 97 benchmark. Some tests may 
  report a time-out error if CenterPOPUP is used.

- Limitation with multiple graphics cards

  Windows NT 4.0 supports a maximum of about 280 different display 
  modes (combinations of resolution, color palette and refresh 
  rate settings). You may encounter this limit if you have more 
  than one Matrox graphics card installed in your computer.

  If the Matrox "VESA settings" option button is selected when 
  there are multiple Matrox cards in your computer, you're even 
  more likely to encounter the Windows NT 4.0 limit in the number 
  of display modes. This is because the "VESA settings" option 
  supports several different refresh rates for each display 
  resolution and color palette setting.

  If you have more than one Matrox graphics card in your computer, 
  we recommend you not use the "VESA settings" option. Note that 
  changing your refresh rate through the Microsoft "Display 
  Properties" dialog box activates the "VESA settings" option.

- 3D Studio MAX 1.2

  If you have problems running 3D Studio MAX 1.2 using the Matrox 
  HEIDI driver, try disabling the "Use bus mastering" check box 
  under "General settings". To access this check box, click 
  "Start" > "Settings" > "Control Panel" > "Matrox Display 
  Properties" (double-click) > "Performance".

- 3D Studio MAX 2.0

  Switching between HEIDI software emulation and OpenGL 
  acceleration while 3D Studio MAX 2.0 is running, may cause the 
  viewports to flicker while playing animations. This problem may 
  also happen if display settings (resolution or color palette) 
  are changed while 3D Studio MAX is running. If you experience 
  these problems, try closing 3D Studio MAX, changing your display 
  settings (resolution or color palette), and then restarting 3D 
  Studio MAX.

- 15-bit color palette support

  A 15-bit color palette is no longer supported.

- OpenGL support

  Note the following limitations related to the OpenGL (3D) driver 
  included with your Matrox display driver:

    - If you have a newer Matrox product or your Matrox software 
      was provided by the manufacturer of your computer, full 
      OpenGL support may be disabled with your Matrox display 
      driver. For a Matrox display driver with full OpenGL support 
      enabled, see the Matrox Web site (www.matrox.com/mga). (If 
      your Matrox product was provided by the manufacturer of your 
      computer, check the Web site of that manufacturer for a 
      display driver. A display driver provided by the 
      manufacturer of your computer is more likely to be tested 
      with your computer model.)

    - In multi-display mode under Windows NT 4.0, OpenGL 
      acceleration is only available if DualHead graphics hardware 
      is the only graphics hardware you're using. (Multi-display 
      OpenGL acceleration isn't supported with Matrox MMS products 
      or with more than one graphics card in your computer.)

    - Using 3D Studio MAX 2.0, you may experience problems with 
      the viewports being improperly redrawn. If this happens, 
      simply click in a viewport to properly update their display. 
      This problem isn't present with version 2.5 (or later) of 3D 
      Studio MAX.

- System memory requirements

  Because of a limitation in Windows NT 4.0, you may experience 
  problems if your computer doesn't have more system memory than 
  the total amount of graphics memory used in your computer. To 
  determine the amount of graphics memory used in your computer, 
  add the total amount of graphics memory on each installed Matrox 
  graphics product in your computer.

  Depending on your total amount of graphics memory, here are some 
  recommended amounts of system memory for Windows NT 4.0:

    |  Graphics memory   |    System memory   |
    |      (total)       |    (recommended)   |
    +--------------------+--------------------+
    |      32 MB         |    64 MB or more   |
    |      64 MB         |   128 MB or more   |
    |     128 MB         |   192 MB or more   |
    |     160 MB         |   256 MB or more   |

- Full-screen DOS support with multiple graphics chip

  If you have more than 10 graphics chips in your system (for 
  example, 3 Matrox MMS-Quad cards), your system may stop 
  responding when running a DOS program in full-screen mode. If 
  your DOS program supports it, run it in a DOS window.


Matrox TV output
================

Certain models of Matrox graphics cards support TV output. With TV 
output support, you can view or record your computer display with 
a TV or video recorder connected to your graphics card.

Recommendation
--------------
- While playing games using TV output, we recommend you use a 640 
  x 480 display resolution. This is because the resolution 
  capabilities of TVs are lower than most computer monitors. If 
  you use a higher display resolution (800 x 600 or 1024 x 768), 
  the display on your TV may not look as sharp as the display of 
  your computer monitor -- that is, some of the extra detail may 
  be harder to see on your TV.

- For Matrox G100/G200 graphics cards with TV output support: 
  Matrox default advanced TV output settings are good for viewing 
  most computer graphics (for example, computer games or your 
  Windows desktop) on most TVs. Based on broadcast standards, 
  there are advanced TV output settings that are better suited for 
  viewing full-screen video (for example, from a video file). 
  These settings are:

  NTSC
     - Brightness: 180
     - Contrast: 234
     - Saturation: 137
     - Hue: 0

  PAL
     - Brightness: 167
     - Contrast: 255
     - Saturation: 138
     - Hue: 0

  Note: For ideal settings, you may also need to adjust the 
  settings on your TV. The default brightness, contrast, 
  saturation and hue settings on most consumer video devices are 
  higher than broadcast standards. These settings are usually okay 
  for viewing video but may not look okay with computer graphics. 
  (This is why Matrox default TV output settings are lower than 
  what's ideal for video.) For more information on how to adjust 
  settings on your TV, see your TV manual.

More information
----------------
For more information on display settings, see your Matrox manual 
and online documentation. For information on how to change the 
display resolution of a game you're using, see its documentation.

Note: The Matrox zoom and virtual desktop features aren't 
supported in TV output mode. Also, TV output mode isn't supported 
if you have more than one Matrox graphics card in your computer.

Note: For TV output with full-screen DOS display modes under 
Windows NT 4.0, only text display modes (02h, 03h) are supported.
