<        Installation instructions for OS/2 Device Driver FixPak XR_D002















        

        
        



        September 21, 2000

        
        Build level 10.042
        
        
        
        This FixPak applies to:
        
        XR_3005 Warp Server
        XR_3006 Warp Server SMP
        XR_4000 Warp v4
        XR_4010 WSOD Rel 1
        XR_4010 WSOD Rel 2
        XR_4500 WSeB SMP
        XR_4500 WSeB UNI
        
        Requires Corrective Service Facility release F.143 or later
        
        OS/2 Fix Distribution
        Personal System Products
        Austin, Tx
        
        
        (c) Copyright International Business Machines Corporation, 1981, 1998.
        All rights Reserved.

        September 21, 2000 - Warp 3 FixPak XR_D002




                   September 21, 2000 - Warp 3 FixPak XR_D002

   CONTENTS


     1.0 Terms and Conditions  . . . . . . . . . . . . . . . . . . . . . . 1

     2.0 Do not use your system  . . . . . . . . . . . . . . . . . . . . . 2

     3.0 Installation Notes  . . . . . . . . . . . . . . . . . . . . . . . 3
       3.0.1 New SYSLEVEL.BDD  . . . . . . . . . . . . . . . . . . . . . . 3
       3.0.2 Relocated OS/2 file support   . . . . . . . . . . . . . . . . 3
       3.0.3 Please use Fixtool f.143 or later   . . . . . . . . . . . . . 4
       3.0.4 IBM1S506 Device Driver useage   . . . . . . . . . . . . . . . 4
       3.0.5 Updated Corrective Service Facility (CSF)   . . . . . . . . . 5
       3.0.6 CSF0208 No products were found  . . . . . . . . . . . . . . . 5
       3.0.7 CSF0248 Archive path is shared between mismatched   . . . . . 5
       3.0.8 CSF0249 Error opening or creating archive file.   . . . . . . 6
       3.0.9 Configuration Installation Distribution ( CID )   . . . . . . 6
       3.0.10 Read-Only files  . . . . . . . . . . . . . . . . . . . . . . 6

     4.0 Post Installation Notes   . . . . . . . . . . . . . . . . . . . . 7
       4.0.1 Slow mouse acceleration   . . . . . . . . . . . . . . . . . . 7
       4.0.2 New version of IBM1S506.ADD   . . . . . . . . . . . . . . . . 7
       4.0.3 TRAP 000E with Removeable Media   . . . . . . . . . . . . . . 7
       4.0.4 Setting IRQ9 processing in config.sys for VPIC.SYS  . . . . . 8
       4.0.5 Intermittent pause with IBM Thinkpad 760E/ED/ELD/EL   . . . . 8
       4.0.6 APM users   . . . . . . . . . . . . . . . . . . . . . . . . . 9
       4.0.7 Fixed IDE Hard Drive and Removable Media Support  . . . . . . 9

     5.0 New Function   . . . . . . . . . . . . . . . . . . . . . . . . . 10

     6.0 Corrective Service Facility  . . . . . . . . . . . . . . . . . . 11
       6.0.1 Required CSF level   . . . . . . . . . . . . . . . . . . . . 11
       6.0.2 Where you can find CSF code  . . . . . . . . . . . . . . . . 11
       6.0.3 Creating FixPak diskettes  . . . . . . . . . . . . . . . . . 11

     7.0 Installation Process   . . . . . . . . . . . . . . . . . . . . . 13
     7.1 Before installation  . . . . . . . . . . . . . . . . . . . . . . 13
     7.2 Method 1: Install from booted OS/2 partition.    . . . . . . . . 13
     7.3 Method 2: Boot from Corrective Service Disk 1.   . . . . . . . . 15
     7.4 Additional Corrective Service Facility information   . . . . . . 15

     8.0 CSD level of SYSLEVEL.OS2  . . . . . . . . . . . . . . . . . . . 16

     9.0 Where Fixes can be found   . . . . . . . . . . . . . . . . . . . 17

     10.0 FixPak Corrective Service levels and disk layouts   . . . . . . 18

     11.0 Space Utilization   . . . . . . . . . . . . . . . . . . . . . . 26

     12.0 Recovering FixPak ARCHIVE and BACKUP space  . . . . . . . . . . 27


   
                                                                Contents  ii


                   September 21, 2000 - Warp 3 FixPak XR_D002

   1.0 TERMS AND CONDITIONS

   Important - please read the following terms and conditions.

   Downloading the Service Fixes included in FixPak XR_D002 for OS/2 Warp 3
   indicates your acceptance of the following terms and conditions:

   1. You must be, and agree that you are, a current licensee of OS/2 Warp
      3.
   2. You may make copies of the OS/2 Service Fixes equal to the number of
      licensed copies of OS/2 Warp 3 you possess.
   3. You may only use the OS/2 Warp 3 Service Fixes included with FixPak
      XR_D002 for maintenance purposes.
   4. All other terms and conditions of your OS/2 Warp 3 license agreements
      apply to the Service Fixes; however, this does not extend any warranty
      and/or services, including but not limited to the "Initial
      Installation" period, outlined in such agreements.



































   
                                                     Terms and Conditions  1


                   September 21, 2000 - Warp 3 FixPak XR_D002

   2.0 DO NOT USE YOUR SYSTEM

   Once you begin a FixPak installation, do not try to use your system for
   any other purpose. Doing so may yield unexpected problems which can cause
   the FixPak installation to fail.















































   
                                                   Do not use your system  2


                   September 21, 2000 - Warp 3 FixPak XR_D002

   3.0 INSTALLATION NOTES



   3.0.1 NEW SYSLEVEL.BDD

   This Fixpak requires a SYSLEVEL.BDD file to be located in the
   \OS2\INSTALL directory of any drive that is to be serviced.  A new
   Fixtool exit called FIXTPREP.EXE is included with this Fixpak. It will
   create a new SYSLEVEL.BDD file in each OS/2 bootable drive if the
   following requirements are met:

   1. \OS2\INSTALL\SYSLEVEL.BDD does not exist
   2. \OS2\INSTALL\SYSLEVEL.FPK exists
   3. \OS2\INSTALL\SYSLEVEL.OS2 is at the following level:
      þ  Fixpak 32 or later for Warp 3
      þ  Fixpak 4 or later for Warp 4
      þ  Fixpak 4 or later for WSOD release 1
      þ  Any level of WSOD release 2

   If yes, then a \OS2\INSTALL\SYSLEVEL.BDD is created which will allow this
   Fixpak to install on this drive.


   3.0.2 RELOCATED OS/2 FILE SUPPORT

   This FixPak will service directories based on the location of supported
   SYSLEVEL.BDD.  Please check your system to make sure extra copies of
   these files are not located in directories other than:

     \OS2\INSTALL\SYSLEVEL.OS2 on the boot drive of your OS/2 partition(s)


   If additional copies of these files are found in other locations on your
   hard disk then CSF will try to service files as follows:

   For SYSLEVEL.OS2















   
                                                       Installation Notes  3


                   September 21, 2000 - Warp 3 FixPak XR_D002

     ..\..\   all files in a directory two levels above (toward the root).
              This should be the root directory of your boot drive.
     ..\*     all files in a directory one level above (toward the root) and
              all subdirectories below. This should be the OS2 directory and
              subdirectories.


   If you have moved OS/2 files or directories, do the following
   in order to have them serviced:

   1. Create a file named USERDIRS.BDD in the \OS2\INSTALL directory of the
      OS\2 Warp partition to be serviced.


      In this file, place the full path to the directory you want to be
      serviced. Examples would be:

        C:\JSI\*
        D:\JSI\SH\*



      Be sure to include the trailing * (asterisk) after the last backslash.

   Note: Leave this file for any future OS/2 Device Driver FixPaks you
   might apply.


   3.0.3 PLEASE USE FIXTOOL F.143 OR LATER


   Use Corrective Service Facility (FIXTOOL) build F.143 or later for this
   Device Driver Fixpak and all future Device Driver Fixpaks.


   3.0.4 IBM1S506 DEVICE DRIVER USEAGE


   It is important to use IBMIDECD.FLT with the IBM1S506.ADD driver.
   If you are using the /BM or !BM parameters to enable or disable busmaster;
   you MUST specify the adapter with /A:x. You can also specify the unit on
   that adapter with /U:z.
   For example:

       BASEDEV=IBM1S506.ADD /A:0 /U:0 /!BM or /A:0 /!BM to disable BUS Master DMA
       BASEDEV=IBM1S506.ADD /A:0 /U:0 /BM or /A:0 /BM to enable



   Use the /V parameter to view what mode the drives are set to. For example:


   
                                                       Installation Notes  4


                   September 21, 2000 - Warp 3 FixPak XR_D002

       BASEDEV=IBM1S506.ADD /V /A:0 /U:0 /!BM




   3.0.5 UPDATED CORRECTIVE SERVICE FACILITY (CSF)


   Use CSF level f.143 or later for all Fixpaks.  It is contained in CS_143.EXE.
   This is a self-extracting ZIP file.  It is not and does not contain bootable
   disks.


   See the READ.ME file for instructions on how to boot with diskettes along
   with a lot of other useful information.


   3.0.6 CSF0208 NO PRODUCTS WERE FOUND


   This means no SYSLEVEL files was found that had a CSD Level, COMPID, Version and Type that matched
   any of the SYSLEVEL files supported by this FixPak. Run the SYSLEVEL command and record the output
   for SYSLEVEL.OS2 in the OS2/INSTALL directory on your boot drive. Compare this data with the data
   contained in the README.1ST file on FixPak disk 1.


   To recover from this, rename the existing SYSLEVEL.OS2 file to SYSL.OS2 and copy SYSLEVEL.OS2 from
   your Warp 4 installation DISK 1.


   3.0.7 CSF0248 ARCHIVE PATH IS SHARED BETWEEN MISMATCHED

   1. The Archive path you specified (or was previously specified) contains
      files from a different release of OS/2. You need to specify a different
      Archive path.
   2. You have a bad SYSLEVEL.OS2 or SYSLEVEL.MPM file. Both must have the same
      Current CSD Level, Version, Type and Component ID if you point both FixPak
      Archives to the same location.


      Check \OS2\INSTALL\SYSLEVEL.OS2 and \MMOS2\INSTALL\SYSLEVEL.MPM. If either is
      wrong, place the last FixPak disk in A: and run
      FIXSYSL.CMD to correct SYSLEVEL.OS2
      problems or SYSZMPM.CMD to fix SYSLEVEL.MPM problems.








   
                                                       Installation Notes  5


                   September 21, 2000 - Warp 3 FixPak XR_D002

   3.0.8 CSF0249 ERROR OPENING OR CREATING ARCHIVE FILE.


   Typically this means the FixPak Archive directory has been deleted but the
   files that point to it still exist. You need to delete the LOGF000.BDD and
   LOGSTART.BDD files from your OS2/INSTALL directory.  LOGSTART.BDD has the
   R/O attribute set and it needs to be reset before the file can be deleted.
   There may also be a LOGARCH.OS2 file that needs to be deleted.


   This can also occur for Multi Media Presentation Manager/2 (MMPM). You would
   then need to delete the LOGF0000.MPM and LOGSTART.MPM files from the
   \MMOS2\INSTALL directory and possibly LOGARCH.MPM if it exists.


   3.0.9 CONFIGURATION INSTALLATION DISTRIBUTION ( CID )

   Read the README.CID on Disk # 1 for an example of how to set up
   a response file to do a CID install.


   3.0.10 READ-ONLY FILES


   If you installed OS/2 Warp 3.0 from a CD-ROM, some files being updated
   may have the Read-Only attribute set. This will cause the update
   program to ask you if you want the files replaced. Answer OK.

























   
                                                       Installation Notes  6


                   September 21, 2000 - Warp 3 FixPak XR_D002

   4.0 POST INSTALLATION NOTES



   4.0.1 SLOW MOUSE ACCELERATION


   Some systems may experience a slow mouse acceleration after this FixPak
   has been installed. If you experience this problem, restore MOUSE.SYS,
   VMOUSE.SYS, and POINTDD.SYS from your BACKUP directory.


   4.0.2 NEW VERSION OF IBM1S506.ADD


   This FixPak contains a new version of IBM1S506.ADD. This version has special
   features for flushing the buffers when shutting down OS/2. There was a new,
   undocumented parameter added on the IBM1S506.ADD BASEDEV line in CONFIG.SYS.

    /!SHUTDOWN  - Disable spin down of drives

   This parameter disables the new feature that has been determined to cause some
   disk drives not to respond when the system is rebooted from any state but a
   physical power on (use of the CTRL-ALT-DEL keys either before or after the
   SHUTDOWN icon is used).
   If your system is experiencing such a problem, please add the /!SHUTDOWN
   parameter to your CONFIG.SYS.

   In the next release of IBM1S506.ADD, /!SHUTDOWN will be the default behavior,
   and a /SHUTDOWN will be added to enable the feature.


   4.0.3 TRAP 000E WITH REMOVEABLE MEDIA


   This trap will happen to anyone who uses DevIoCtl that does things like
   EJECT, PROTECT, etc for Removeable Media and has removed all FAT cache from
   CONFIG.SYS.


   Workaround is to add DISKCACHE=64,LW to CONFIG.SYS.


   This problem will be fixed in Fixpak 41 and above.








   
                                                  Post Installation Notes  7


                   September 21, 2000 - Warp 3 FixPak XR_D002

   4.0.4 SETTING IRQ9 PROCESSING IN CONFIG.SYS FOR VPIC.SYS


   Some applications like PCAS (and some terminal emulators) have problems
   sharing IRQ9 in a VDM.  Since the DOS Virtual Device drivers are not loaded
   out of CONFIG.SYS, a new device driver VPICPARM.SYS has been added starting
   with Warp 3 FixPak 38 and Warp 4 FixPak 8.

   To prevent sharing of IRQ9 in a VDM, add the following statement in
   config.sys:

      device=x:\os2\mdos\vpicparm.sys irq9_off
      (x: is your OS/2 boot drive)



   Next, in the settings for the program that requires exclusive access to IRQ9,
   set the DOS setting HW_SHARE_IRQ9 to ON.


   When you next boot your system, VDMs will not share IRQ9.


   4.0.5 INTERMITTENT PAUSE WITH IBM THINKPAD 760E/ED/ELD/EL


   If you have an IBM Thinkpad 760E/ED/ELD/EL that exhibits sluggish harddisk behavior
   (pausing intermittently with hard drive light on) after this FixPak has been applied,
   add the /!BM parameter to the BASEDEV=IBM1S506.ADD statement (if present) in  your
   CONFIG.SYS.  This will disable the Bus Mastering function whose default has been changed
   from OFF to ON.


   If your CONFIG.SYS has the statement

   BASEDEV=PIIXIDE.ADD



   you must remark out the statement by inserting REM as the first characters on the line
   as shown below.

   REM BASEDEV=PIIXIDE.ADD
   BASEDEV=IBM1S506.ADD /A:0 /!BM /U:1 /ATAPI /FORCE








   
                                                  Post Installation Notes  8


                   September 21, 2000 - Warp 3 FixPak XR_D002

   4.0.6 APM USERS


   APM users will need to add the following statement after the
   DEVICE=\OS2\BOOT\APM.SYS statement in their CONFIG.SYS:

      RUN=\OS2\BOOT\APMDAEMN.EXE



   This will complete the fix for APAR JR09869.


   4.0.7 FIXED IDE HARD DRIVE AND REMOVABLE MEDIA SUPPORT


   FixPak 35 (FP35) for Warp 3 and FixPak 6 (FP6) for Warp 4 extended support for
   fixed Enhanced IDE drives to sizes up to 8.4GB and added new caching HPFS and
   FAT file system support for removable media drives such as SCSI Syquest Syjet
   1.5GB portable hard drive and the Iomega jaz 1GB and 2GB personal hard drives.


   See the README.RMS file on the first FixPak diskette for complete information
   on large IDE Hard Drive and Removable Media Support.




























   
                                                  Post Installation Notes  9


                   September 21, 2000 - Warp 3 FixPak XR_D002

   5.0 NEW FUNCTION


   It is our policy not to include new function in FixPaks. However, as with
   any policy there
   may be exceptions. If any exception occurs in the future,
   we will communicate them to you in this section of the README.1ST.













































   
                                                            New Function  10


                   September 21, 2000 - Warp 3 FixPak XR_D002

   6.0 CORRECTIVE SERVICE FACILITY



   6.0.1 REQUIRED CSF LEVEL


   You must use release level F.143 or later of the OS/2 Corrective Service
   Facility to install this FixPak.
   Check the BUILD.LVL file for the level you are using.
   If it does not have a BUILD.LVL file then it is old and
   cannot be used.


   6.0.2 WHERE YOU CAN FIND CSF CODE


   The latest Corrective Service Facility code is available
   from:


   ftp://service.boulder.ibm.com/ps/products/os2/fixtool/


   Select the required language then the latest fixtool release (CS?143 at the
   time this Fixpak was released).


   The .TXT file has instructions.  The .EXE is a self-extracting ZIP file that
   contains the CSF code.  See the READ.ME file contained in .EXE for
   information on how to use the new CSF.


   6.0.3 CREATING FIXPAK DISKETTES


   Use LOADDSKF.EXE to create the diskettes. For each disk image, place
   a 2MB HD (1.44MB formatted) diskette in A:.

   Warning: DO NOT use a 1MB (720KB formatted) diskette because you might have problems
   trying to install this FixPak.


   For each diskette image in the FixPak, do the following:


   Enter LOADDSKF XR_D002.?DK A: /F  (? can be 1 through 9, A through Z).


   Label the diskette as


   
                                             Corrective Service Facility  11


                   September 21, 2000 - Warp 3 FixPak XR_D002

         FixPak XR_D002
   Corrective Service Diskette ?
          (CSF DISK ?)

















































   
                                             Corrective Service Facility  12


                   September 21, 2000 - Warp 3 FixPak XR_D002

   7.0 INSTALLATION PROCESS



   7.1 BEFORE INSTALLATION


   Before installing any FixPak, run CHKDSK /F against
   all drives on your system to correct any file system errors that might be
   present. You cannot do this while OS/2 is active. You must shut down and
   run CHKDSK by one of the following methods:

   þ  Boot from your Installation and DISK 1 diskettes
      you used to install OS/2 with.
      If your file system is HPFS, then put the diskette with CHKDSK and
      UHPFS.DLL on it in your A: drive before issuing the CHKDSK command.
   þ  Boot from the Utilities disk you created via the "Create Utility
      Diskettes" icon in the System Setup folder.
   þ  Boot from a different OS/2 partition.



   7.2 METHOD 1: INSTALL FROM BOOTED OS/2 PARTITION.

   This method allows you to select the products (partitions) to be serviced.


   This is the method you should use if you have more than one OS/2 partition
   and want to control which one is serviced.

   Note: You can use a diskette drive other than A: with this method. If your
   3.5" diskette drive is B:, use B: where A: is mentioned in the following steps.
   (this method only).

   1. Insert CSF DISK Diskette 1 in drive A.
   2. Open an OS/2 window or full-screen session.
   3. Type A:\SERVICE and press the Enter key.

      Note: You could also use the "Drives" object for A: and double click on the
      "SERVICE.EXE" Icon to start the install.
   4. Follow the displayed instructions. When prompted to insert Corrective
      Service Diskette 1 (not CSF DISK Diskette 1), place FixPak XR_D002
      Corrective Service Diskette 1 in drive A. Repeat for the rest of the FixPak
      disks when requested to do so.

      Note: It can take a considerable length of time for the Corrective Service
      Facility to scan your hard disk for serviceable files. In some cases, it has
      taken as long as 40 minutes. Please be patient and allow this process to
      complete.
   5. If this is the first OS/2 Warp FixPak you have applied to
      this system, then enter the path to the ARCHIVE directory

   
                                                    Installation Process  13


                   September 21, 2000 - Warp 3 FixPak XR_D002

      where a copy of replaced files
      will be stored (for example, D:\ARCHIVE).

      Note: This ARCHIVE directory is not related to the ARCHIVES directory
      built into OS/2 Warp 3.0. Please specify a different path.
      You must specify a different ARCHIVE directory for each product to
      be serviced.


      If this is not the first OS/2 Warp FixPak, then enter the path
      to the BACKUP directory
      where a copy of replaced files will be stored (for example,
      D:\BACKUP).

      Note: You must specify a different BACKUP directory for each product to
      be serviced.


      For either case, make sure there is sufficient space available on the
      drive you specify. Even though these files are kept in compressed
      (PACK2) format, they require between 7 and 12 MB of disk space.
   6. Click on "OK".
   7. You will see an "Application in use" dialog box showing a list of
      locked files that cannot be serviced while the system is running.
      You are given two choices - to Continue or Reboot. Select
      Continue.
   8. During the installation process you might see messages about Archiving,
      Updating and Deferring service.
      þ  Archiving saves a compressed copy of the original file in the
         ARCHIVE or BACKUP path you specified.
      þ  Updating means the original files are replaced with the new
         ones from this FixPak.
      þ  Deferring service means the file to be updated is currently in use
         by the system and cannot be updated. The new files from the FixPak
         are placed in unpacked format
         in the \IBMCSFLK\FIX directory on the drive with the most free space.
         They are processed by the locked file device
         driver during reboot after you shut down the system.
   9. Select NO for a redisplay of the "Product List" after
      the first part of the FixPak application process has completed if this
      message is displayed.
   10.Click Cancel and Exit to close the Corrective Service Facility window
      if necessary.
   11.Shut down and reboot your system.

      You will see the following during reboot of the system
      if you applied service to the
      OS/2 partition you were booted from.




   
                                                    Installation Process  14


                   September 21, 2000 - Warp 3 FixPak XR_D002

      The locked file driver is loaded.

             Processing locked files

             Processing complete



      The system will do one automatic reboot after the Locked File Device Driver
      has completed.



   7.3 METHOD 2: BOOT FROM CORRECTIVE SERVICE DISK 1.


   This method does not prompt the user for any information. No interaction with
   the user takes place other than requests to put the next diskette in drive A.
   All serviceable partitions on your system will be updated automatically. Be
   especially careful of extra SYSLEVEL.OS2 or SYSLEVEL.MPM files when using
   this method because they can cause CSF to apply service to directories you do
   not want serviced.

   1. Shut down your OS/2 system.
   2. Insert CSF DISK Diskette 1 in drive A.
   3. Press Ctrl+Alt+Del to boot the disk in drive A.


   Service will be applied to ALL partitions that contain a version of OS/2
   that is supported by this FixPak. See the section "FixPak Corrective
   Service Notes" for the CSD levels this FixPak applies to.

   Note: It can take a considerable length of time for the Corrective Service
   Facility to scan your hard disk for serviceable files. In some cases it has
   taken as long as 40 minutes. Please be patient and allow this process to
   complete.


   7.4 ADDITIONAL CORRECTIVE SERVICE FACILITY INFORMATION


   Additional information on the Corrective Service Facility is available
   from the README.INF file on the first Corrective Service
   Facility disk. To view this file, place CSF disk 1 in drive A and enter
   VIEW A:\README.INF.







   
                                                    Installation Process  15


                   September 21, 2000 - Warp 3 FixPak XR_D002

   8.0 CSD LEVEL OF SYSLEVEL.OS2


   The Current CSD level for the "IBM OS/2 Base Operating System" will
   not be changed by installation of this FixPak even though the
   SERVICE.LOG file indicates it will. This FixPak is not a Service Level
   change. It upgrades the existing service level (XR_3005); therefore
   the SYSLEVEL is not changed.


   All fix information is recorded in SERVICE.LOG. Look at the file

      \OS2\INSTALL\SERVICE.LOG



   on your boot drive for information relating to the installation of
   FixPaks on your system.


   Additionally, you can use
   the VER /R command to see the current revision of OS/2 installed. The
   response will look like the following for this FixPak:

   The Operating System/2 Version is 3.00
   Revision 8.265



   The first page of this document has a line that looks like:

   Build Level: n.nnn



   That is the number you should see for this FixPak when you issue the
   VER /R command.















   
                                               CSD level of SYSLEVEL.OS2  16


                   September 21, 2000 - Warp 3 FixPak XR_D002

   9.0 WHERE FIXES CAN BE FOUND

   You can find other files, such as new drivers or fixes for specific
   video cards, from the following locations:

   þ  CompuServe - Subscribers can download fixes from the OS/2 Support
      Forum (GO OS2SUPPO).
   þ  IBM OS/2 BBS - Subscribers can download fixes from the Software
      Download Library. U.S. customers who are not subscribers can call
      1-800-547-1283 for information on how to subscribe.
   þ  Internet - Customers with access to Internet services can download
      fixes using the following methods:

         Anonymous FTP to "ftp.software.ibm.com" (IP Address 198.17.57.67)
         FixPaks are located in the "/ps/products/os2/fixes" directory.

         World Wide Web (WWW) access via:
           IBM Software Manufacturing Solutions ftp://service.boulder.ibm.com
           Full path is ftp://service.boulder.ibm.com/ps/products/os2/


   þ  Prodigy - Subscribers can download fixes from the OS2CLUB in the
      Download Library, IBM Files, Fixes area. Files are updated weekly and are
      available on Friday.
   þ  PCC BBS - Customers can call the IBM Personal Computer Company BBS in
      Raleigh, NC, and download fixes from the public area. You can access this
      BBS at 1-919-517-0001.
   þ  America On Line - Subscribers can download fixes from the OS/2 Area.
























   
                                                Where Fixes can be found  17


                   September 21, 2000 - Warp 3 FixPak XR_D002

   10.0 FIXPAK CORRECTIVE SERVICE LEVELS AND DISK LAYOUTS

   Build Level: 10.042

   Product location on CSD:  A:\FIX\BDD.1
   Product name:  "IBM OS/2 Base Device Drivers"
   Standard Edition  3.01
   Fixpak name:   XR_D002_   (Country = Generic)
   Pre-requisite CSD Level:  XR_3005_
   System Id:  1000
   Component Id:  562274700
   Archive is ON for this product.
   ________________________________________________________________________
   Product name:  "IBM OS/2 Base Device Drivers"
   Standard Edition  3.02
   Fixpak name:   XR_D002_   (Country = Generic)
   Pre-requisite CSD Level:  XR_3006_
   System Id:  1000
   Component Id:  5639A5500
   Archive is ON for this product.
   ________________________________________________________________________
   Product name:  "IBM OS/2 Base Device Drivers"
   Standard Edition  4.00
   Fixpak name:   XR_D002_   (Country = Generic)
   Pre-requisite CSD Level:  XR_4000_
   System Id:  1000
   Component Id:  5639A6100
   Archive is ON for this product.
   ________________________________________________________________________
   Product name:  "IBM OS/2 Base Device Drivers"
   Standard Edition  4.01
   Fixpak name:   XR_D002_   (Country = Generic)
   Pre-requisite CSD Level:  XR_4010_
   System Id:  1000
   Component Id:  5639A6100
   Archive is ON for this product.
   ________________________________________________________________________
   Product name:  "IBM OS/2 Base Device Drivers"
   Standard Edition  4.01
   Fixpak name:   XR_D002_   (Country = Generic)
   Pre-requisite CSD Level:  XR_4010_
   System Id:  1000
   Component Id:  5639A6120
   Archive is ON for this product.
   ________________________________________________________________________
   Product name:  "IBM OS/2 Base Device Drivers"
   Standard Edition  4.50
   Fixpak name:   XR_D002_   (Country = Generic)
   Pre-requisite CSD Level:  XR_4500_
   System Id:  1000
   Component Id:  5639A6150

   
                       FixPak Corrective Service levels and disk layouts  18


                   September 21, 2000 - Warp 3 FixPak XR_D002

   Archive is ON for this product.
   ________________________________________________________________________
   Product name:  "IBM OS/2 Base Device Drivers"
   Standard Edition  4.50
   Fixpak name:   XR_D002_   (Country = Generic)
   Pre-requisite CSD Level:  XR_4500_
   System Id:  1000
   Component Id:  5639A5550
   Archive is ON for this product.
   ________________________________________________________________________

   Default directories:

           ..\..\
           ..\*
           ..\..\MMOS2
           ..\..\MMOS2\*
           ..\..\VT
           ..\..\VT\*
           ..\..\PSFONTS
           ..\..\PSFONTS\*
           ..\..\LANGUAGE
           ..\..\LANGUAGE\*
   Will create the following directories
      ..\..\OS2\BOOT   Stub File:  @BOOTDIR

      ..\..\OS2\MDOS   Stub File:  @MDOSDIR

      ..\..\OS2   Stub File:  @OS2DIR

      ..\..\OS2\DLL   Stub File:  @DLLDIR

      ..\..\OS2\SYSTEM   Stub File:  @SYSTDIR

      ..\..\OS2\SYSTEM\TRACE   Stub File:  @TRACDIR


   Files contained in Fixpak for product:

   Filename      Name on CSD   Disk#  Date        Time   Size     Checksum
   ------------  ------------  -----  ----------  -----  -------  --------
   152XPRES.EXE  152XPRES.EX_    2    05/23/2000  08:51     3125  1665685B
   154XPRES.EXE  154XPRES.EX_    2    05/23/2000  08:48     3245  457B03D0
   164XPRES.EXE  164XPRES.EX_    2    05/23/2000  08:49     2773  5542512B
   174XPRES.EXE  174XPRES.EX_    2    05/23/2000  08:50     2933  31BCFEF1
   7770PRES.EXE  7770PRES.EX_    2    05/23/2000  08:52     3141  5A2E6504
   7870PRES.EXE  7870PRES.EX_    2    07/12/1999  15:09     3703  1B7A2864
   AHA152X.ADD   AHA152X.AD_     1    06/16/2000  10:32    44224  B15E9FF8
   AHA154X.ADD   AHA154X.AD_     2    06/16/2000  10:31    20646  707FC129
   AHA164X.ADD   AHA164X.AD_     2    06/16/2000  10:31    20038  71ACD883
   AHA174X.ADD   AHA174X.AD_     2    06/16/2000  10:31    18030  E0EF11A1

   
                       FixPak Corrective Service levels and disk layouts  19


                   September 21, 2000 - Warp 3 FixPak XR_D002

   AHA6360.SNP   AHA6360.SN_     1    06/16/2000  11:10    27383  C8F27DF6
   AIC7770.ADD   AIC7770.AD_     1    06/16/2000  10:32    42574  6E72912C
   AIC7870.ADD   AIC7870.AD_     1    07/12/1999  15:15   134280  F9946E33
   AIC7870.SNP   AIC7870.SN_     2    06/16/2000  11:12     9104  130DA95F
   AIC78U2.ADD   AIC78U2.AD_     1    07/12/1999  15:10   138892  2E6A7A90
   APM.SYS       APM.SY_         2    06/16/2000  12:20    12687  55A99A9A
   APMDAEMN.EXE  APMDAEMN.EX_    2    05/23/2000  10:29     2733  E4F844BD
   AUDMPIO.DRV   AUDMPIO.DR_     2    04/27/1999  18:18     7264  525E2669
   BSAUDIO.SNP   BSAUDIO.SN_     2    06/16/2000  11:13     5752  5D96699F
   BSAUDRES.DLL  BSAUDRES.DL_    2    04/27/1999  18:24     1380  36784494
   BTKPRES.EXE   BTKPRES.EX_     2    05/23/2000  08:57     2941  9DE788A7
   BTSCSI.ADD    BTSCSI.AD_      1    06/16/2000  10:36    26569  98CE9D59
   BUSAUDIO.SYS  BUSAUDIO.SY_    2    06/16/2000  11:15    31965  B5F66D1C
   CD_BOOT.FLT   CD_BOOT.FL_     2    06/16/2000  10:39     5658  DED15477
   CMD640X.ADD   CMD640X.AD_     1    06/16/2000  10:37    36038  65C8D37B
   CMPXCHG8.SYS  CMPXCHG8.SY_    2    12/01/1999  17:56     2634  74883773
   COM.SYS       COM.SY_         2    06/16/2000  10:46    18719  F9E73666
   CS31BA11.DRV  CS31BA11.DR_    1    04/27/1999  18:21   104208  086DC6A0
   DELIVERY.SYS  DELIVERY.SY_    2    05/23/2000  08:46     3806  D71B14A6
   DELIVPRC.EXE  DELIVPRC.EX_    2    12/01/1999  12:12     2733  4F2BFB9A
   DETNE2.SYS    DETNE2.SY_      2    07/17/2000  16:59     5666  F4130B62
   DPT20XX.ADD   DPT20XX.AD_     1    06/16/2000  10:36    24700  AF365485
   DPTPRES.EXE   DPTPRES.EX_     2    06/16/2000  10:36     3463  A603FE8D
   ES688DD.SYS   ES688DD.SY_     1    04/27/1999  18:18    40448  9967D16D
   ES688WIN.386  ES688WIN.38_    2    04/27/1999  18:18    14197  6198A0E7
   ES688WIN.DRV  ES688WIN.DR_    1    04/27/1999  18:18    64336  EBD4EE78
   ESSVSD88.DLL  ESSVSD88.DL_    2    04/27/1999  18:28     1140  8DD7BA00
   EXTDSKDD.SYS  EXTDSKDD.SY_    2    05/23/2000  09:47     1682  A197AE4B
   FD16-700.ADD  FD16-700.AD_    1    06/16/2000  10:33    34160  708E5E68
   FD16-700.EXE  FD16-700.EX_    2    06/16/2000  10:33     3725  8513B331
   FD7000EX.ADD  FD7000EX.AD_    2    06/16/2000  10:34    20758  4915741C
   FD7000EX.EXE  FD7000EX.EX_    2    06/16/2000  10:34     2801  FCFCDA26
   FD8XX.ADD     FD8XX.AD_       1    06/16/2000  10:34    29952  BCB1542C
   FD8XX.EXE     FD8XX.EX_       2    06/16/2000  10:35     3263  46AE3842
   FLASHPT.ADD   FLASHPT.AD_     1    06/16/2000  10:36    57125  01B2E58D
   FLASHPT.SNP   FLASHPT.SN_     2    06/16/2000  11:07     4161  9B0DD4D3
   I2OXPORT.SYS  I2OXPORT.SY_    2    06/16/2000  10:38    10760  99BF7F6E
   IBM16AFS.EXE  IBM16AFS.EX_    2    06/16/2000  10:35     3177  86856B23
   IBM1FLPY.ADD  IBM1FLPY.AD_    1    06/16/2000  10:28    35434  848C94D7
   IBM1S506.ADD  IBM1S506.AD_    1    06/16/2000  10:41    58806  690F1A1F
   IBM2ADSK.ADD  IBM2ADSK.AD_    2    06/16/2000  10:29     9934  A823BD13
   IBM2AMB1.SYS  IBM2AMB1.SY_    2    06/16/2000  10:51    12453  954B9732
   IBM2CAD1.SYS  IBM2CAD1.SY_    2    06/16/2000  10:53    12495  BA10082F
   IBM2CMQ1.SYS  IBM2CMQ1.SY_    2    06/16/2000  10:50    10101  822AFC2C
   IBM2FLPY.ADD  IBM2FLPY.AD_    2    06/16/2000  10:29    14428  88CCB4EE
   IBM2MAT1.SYS  IBM2MAT1.SY_    2    06/16/2000  10:53    10083  B5DAE02F
   IBM2NCR1.SYS  IBM2NCR1.SY_    2    06/16/2000  10:52    10063  6AE07E50
   IBM2NEC1.SYS  IBM2NEC1.SY_    2    06/16/2000  10:51    10063  CEBC11AE
   IBM2SCPR.EXE  IBM2SCPR.EX_    2    12/01/1999  12:10     3051  FD59358F
   IBM2SCSI.ADD  IBM2SCSI.AD_    1    05/23/2000  08:44    33147  C0E89D3D
   IBM2SS02.SYS  IBM2SS02.SY_    2    06/16/2000  11:32    22835  E310FF0B

   
                       FixPak Corrective Service levels and disk layouts  20


                   September 21, 2000 - Warp 3 FixPak XR_D002

   IBM2ZEN1.SYS  IBM2ZEN1.SY_    2    06/16/2000  10:50    10047  25F22ED6
   IBM2ZOS1.SYS  IBM2ZOS1.SY_    2    06/16/2000  10:52    10079  131B64E9
   IBMATAPI.FLT  IBMATAPI.FL_    1    06/16/2000  11:43    31128  153FE589
   IBMIDECD.FLT  IBMIDECD.FL_    1    06/16/2000  10:42    24320  5013C61B
   IBMINT13.I13  IBMINT13.I1_    2    06/16/2000  10:30     9986  CE5AE8DD
   IBMKBD.SYS    IBMKBD.SY_      2    05/23/2000  09:25     8562  DC2C3057
   ICMEMCDD.SYS  ICMEMCDD.SY_    2    06/16/2000  10:57    13932  D932D382
   ICMEMFMT.EXE  ICMEMFMT.EX_    1    06/16/2000  10:57    50932  E8E19320
   ICMEMMTD.SYS  ICMEMMTD.SY_    2    06/16/2000  10:57     7788  10CD6DF6
   IPSRAID.ADD   IPSRAID.AD_     2    07/12/1999  15:10    20130  20DF07D2
   JAZZDD.SYS    JAZZDD.SY_      1    06/16/2000  11:15    44522  E30077BD
   KBDBASE.SYS   KBD-AX.SY_      1    12/04/1999  03:18    28205  165B73C3
   KBDBASE.SYS   KBD-106.SY_     1    12/04/1999  03:17    30765  6169525D
   KBDBASE.SYS   KBD-101.SY_     1    12/04/1999  03:14    31517  263AC477
   KBDBASE.SYS   KBDBASE.SY_     1    12/01/1999  13:09    24989  BEBD3244
   LMS205.ADD    LMS205.AD_      1    06/16/2000  10:42    36386  BB8F7B17
   LMS206.ADD    LMS206.AD_      1    06/16/2000  10:43    38742  268FAEEE
   MITFX001.ADD  MITFX001.AD_    2    06/16/2000  10:40    20502  B4537BA7
   MMMIXER.DLL   MMMIXER.DL_     2    04/27/1999  18:20    22800  9244CE32
   MOUSE.SYS     MOUSE.SY_       1    06/26/2000  11:22    23945  1AD3D86C
   MSBUS01.SYS   MSBUS01.SY_     2    05/23/2000  09:21     1294  17B428FA
   MSINP01.SYS   MSINP01.SY_     2    05/23/2000  09:21     1411  FA370B23
   MSSER01.SYS   MSSER01.SY_     2    05/23/2000  09:21     1761  A70D5967
   MSSER02.SYS   MSSER02.SY_     2    05/23/2000  09:18     2198  5E597421
   MVPROAUD.DRV  MVPROAUD.DR_    2    04/27/1999  18:21    24608  2A62310F
   MVPRODD.SYS   MVPRODD.SY_     1    06/16/2000  11:16    52444  E482C2B0
   OPL3.DRV      OPL3.DR_        1    04/27/1999  18:32    56384  1BF02A0C
   OS2ASPI.DMD   OS2ASPI.DM_     2    06/16/2000  10:25    11232  A947B2B1
   OS2CDROM.DMD  OS2CDROM.DM_    1    05/23/2000  09:04    32152  CEB520C3
   OS2SCSI.DMD   OS2SCSI.DM_     2    05/23/2000  08:36    11612  8E823F7D
   PCIBUS.SNP    PCIBUS.SN_      2    06/16/2000  11:04     2496  60C52D67
   PCLOGIC.SYS   PCLOGIC.SY_     2    06/16/2000  10:45     3692  A83137F8
   PCMOU02.SYS   PCMOU02.SY_     2    05/23/2000  09:18     2306  F393073B
   PDIMOU01.SYS  PDIMOU01.SY_    2    05/23/2000  09:20     1388  713F92FF
   PDIMOU02.SYS  PDIMOU02.SY_    2    05/23/2000  09:17     2018  4FFAFF52
   PDITOU01.SYS  PDITOU01.SY_    2    06/16/2000  11:00    13642  CE64A8D3
   PDITOU02.SYS  PDITOU02.SY_    2    06/16/2000  11:01    13234  69C51A9D
   POINTDD.SYS   POINVGA2.SY_    2    05/23/2000  09:40     3814  7C6F4E80
   POINTDD.SYS   POINTDD.SY_     2    05/23/2000  09:40     3814  7C6F5920
   PRINT01.SYS   PRINT01.SY_     2    07/17/2000  17:52    12718  D9B1C8B3
   PRINT02.SYS   PRINT02.SY_     2    07/17/2000  17:52    11878  51F1AFAB
   RESERVE.SYS   RESERVE.SY_     2    07/17/2000  16:58     5704  88B2B515
   RESOURCE.SYS  RESOURCE.SY_    1    06/16/2000  10:22    55402  5ABF98CE
   RMAUDIO.SYS   RMAUDIO.SY_     2    06/16/2000  11:15    26273  C44003AF
   RMINFO.DLL    RMINFO.DL_      1    05/23/2000  08:28    22847  0943C3D9
   RMVIEW.EXE    RMVIEW.EX_      1    05/23/2000  08:29    32505  4FE3620F
   SB16D2.SYS    SB16D2.SY_      1    04/27/1999  18:32    64424  7A460B63
   SBAWE32.DRV   SBAWE32.DR_     1    04/27/1999  18:21    48640  FAF180A1
   SBAWED2.SYS   SBAWED2.SY_     1    04/27/1999  18:16   101700  A1E8AEEA
   SBCD2.ADD     SBCD2.AD_       2    06/16/2000  10:39    18824  B3DE07C9
   SBD2.SYS      SBD2.SY_        1    06/16/2000  11:16    41388  A9C4F9D9

   
                       FixPak Corrective Service levels and disk layouts  21


                   September 21, 2000 - Warp 3 FixPak XR_D002

   SBP2D2.SYS    SBP2D2.SY_      1    06/16/2000  11:17    46508  DF1836C0
   SBPD2.SYS     SBPD2.SY_       1    06/16/2000  11:17    43948  8650C415
   SGAUDVDD.SYS  SGAUDVDD.SY_    2    04/27/1999  18:16     6144  A117BFC1
   SONY31A.ADD   SONY31A.AD_     1    06/16/2000  10:40    32742  A66FF37D
   SONY535.ADD   SONY535.AD_     2    06/16/2000  10:41    19538  5737592F
   TESTCFG.SYS   TESTCFG.SY_     2    06/16/2000  10:58     9808  97E91FE0
   TMV1PRES.EXE  TMV1PRES.EX_    2    12/01/1999  12:01     3017  755A208F
   TMV1SCSI.ADD  TMV1SCSI.AD_    2    06/16/2000  10:26    21660  166D4BE6
   TOUCH.SYS     TOUCH.SY_       2    05/23/2000  09:43    20090  97B505DD
   USBAUDIO.SYS  USBAUDIO.SY_    1    06/16/2000  11:43    29492  B654943A
   USBCOM.SYS    USBCOM.SY_      2    06/16/2000  11:43    19513  72318D0C
   USBD.SYS      USBD.SY_        2    06/16/2000  11:43    18504  1BCA482C
   USBHID.SYS    USBHID.SY_      2    06/16/2000  11:43    12894  13648C3A
   USBKBD.SYS    USBKBD.SY_      2    06/16/2000  11:43    12334  805768DC
   USBMON.EXE    USBMON.EX_      1    07/07/2000  18:58    20105  1DDC0E12
   USBMOUSE.SYS  USBMOUSE.SY_    1    06/16/2000  11:43    11920  E5762393
   USBPRT.HLP    USBPRT.HL_      2    07/07/2000  08:58     6293  E153F57C
   USBPRT.PDR    USBPRT.PD_      1    07/07/2000  18:58    39763  0613814B
   USBUHCD.SYS   USBUHCD.SY_     1    06/16/2000  11:43    23726  82E75CB0
   USBUHCD2.SYS  USBUHCD2.SY_    1    06/16/2000  11:43    23726  7E0ECA81
   VAPM.SYS      VAPM.SY_        2    05/23/2000  10:07     1120  A04433E8
   VASPI.SYS     VASPI.SY_       2    05/23/2000  09:46     8992  3B6A7E14
   VCDROM.SYS    VCDROM.SY_      2    05/23/2000  10:07     6880  BD43B4AD
   VCOM.SYS      VCOM.SY_        2    05/23/2000  10:08    12384  5794F387
   VDISK.SYS     VDISK.SY_       2    05/23/2000  09:46     2920  AE4FF180
   VDSK.SYS      VDSK.SY_        2    05/23/2000  10:09    10384  FFE6A018
   VFLPY.SYS     VFLPY.SY_       2    05/23/2000  10:09     6064  A48C27B9
   VIDRMS.SYS    VIDRMS.SY_      2    06/16/2000  11:15    29073  C73A5674
   VIDVBC.SYS    VIDVBC.SY_      2    06/16/2000  11:20    28501  B8F9A306
   VISION02.SYS  VISION02.SY_    2    05/23/2000  09:18     2294  5A46BF17
   VKBD.SYS      VKBD101.SY_     1    12/07/1999  11:02    54523  0F722B79
   VKBD.SYS      VKBD106.SY_     1    12/07/1999  11:02    54334  9633257A
   VKBD.SYS      VKBD.SY_        1    05/22/2000  15:34    25655  42176C9F
   VLPT.SYS      VLPT.SY_        2    06/16/2000  11:14    10081  743EE4C5
   VMOUSE.SYS    VMOUSE.SY_      2    05/23/2000  10:10    18704  A30D8284
   VSNDSYS.386   VSNDSYS.38_     1    04/27/1999  18:32    64026  D9563A28
   VTOUCH.SYS    VTOUCH.SY_      2    12/01/1999  14:05    13660  335C712D

   ************************************************************************
   Product location on CSD:  A:\FIX\BDD.2
   Product name:  "IBM OS/2 Base Device Drivers"
   Standard Edition  3.01
   Fixpak name:   XR_D002_   (Country = Generic)
   Pre-requisite CSD Level:  XR_3005_
   System Id:  1000
   Component Id:  562274700
   Archive is ON for this product.
   ________________________________________________________________________

   Default directories:


   
                       FixPak Corrective Service levels and disk layouts  22


                   September 21, 2000 - Warp 3 FixPak XR_D002

           ..\..\
           ..\*
           ..\..\MMOS2
           ..\..\MMOS2\*
           ..\..\VT
           ..\..\VT\*
           ..\..\PSFONTS
           ..\..\PSFONTS\*
           ..\..\LANGUAGE
           ..\..\LANGUAGE\*

   Files contained in Fixpak for product:

   Filename      Name on CSD   Disk#  Date        Time   Size     Checksum
   ------------  ------------  -----  ----------  -----  -------  --------
   AUTODRV2.SYM  AUTODRV2.SY_    2    06/16/2000  10:48     2500  D93F6681
   COM.SYS       COM.SY_         2    06/16/2000  12:37    18799  8A4763CA
   IBM2SS01.SYS  IBM2SS01.SY_    2    06/16/2000  10:49    13203  41742A78
   PCM2ATA.ADD   PCM2ATA.AD_     2    06/16/2000  10:56    23280  0105C549
   PCMCIA.SYS    PCMCIA.SY_      2    06/16/2000  10:47    47622  4A03DC41
   SS2PCIC1.SYS  SS2PCIC1.SY_    2    06/16/2000  10:49    10549  E1EA1B5A
   SS2TCIC1.SYS  SS2TCIC1.SY_    2    06/16/2000  10:49    12595  DAA0C369

   ************************************************************************
   Product location on CSD:  A:\FIX\BDD.3
   Product name:  "IBM OS/2 Base Device Drivers"
   Standard Edition  3.02
   Fixpak name:   XR_D002_   (Country = Generic)
   Pre-requisite CSD Level:  XR_3006_
   System Id:  1000
   Component Id:  5639A5500
   Archive is ON for this product.
   ________________________________________________________________________

   Default directories:

           ..\..\
           ..\*
           ..\..\MMOS2
           ..\..\MMOS2\*
           ..\..\VT
           ..\..\VT\*
           ..\..\PSFONTS
           ..\..\PSFONTS\*
           ..\..\LANGUAGE
           ..\..\LANGUAGE\*

   Files contained in Fixpak for product:

   Filename      Name on CSD   Disk#  Date        Time   Size     Checksum
   ------------  ------------  -----  ----------  -----  -------  --------

   
                       FixPak Corrective Service levels and disk layouts  23


                   September 21, 2000 - Warp 3 FixPak XR_D002

   AUTODRV2.SYS  AUTODRV2.SY_    2    06/16/2000  10:48    10862  8325D19D
   COM.SYS       COM.SY_         2    06/16/2000  10:46    18719  F9E73666
   IBM2SS01.SYS  IBM2SS01.SY_    2    06/16/2000  10:49    13203  41742A78
   PCM2ATA.ADD   PCM2ATA.AD_     2    06/16/2000  10:56    23280  0105C549
   PCMCIA.SYS    PCMCIA.SY_      2    06/16/2000  10:47    47622  4A03DC41
   SS2PCIC1.SYS  SS2PCIC1.SY_    2    06/16/2000  10:49    10549  E1EA1B5A
   SS2TCIC1.SYS  SS2TCIC1.SY_    2    06/16/2000  10:49    12595  DAA0C369

   ************************************************************************
   Product location on CSD:  A:\FIX\BDD.4
   Product name:  "IBM OS/2 Base Device Drivers"
   Standard Edition  3.01
   Fixpak name:   XR_D002_   (Country = Generic)
   Pre-requisite CSD Level:  XRJ3005_
   System Id:  1000
   Component Id:  562274700
   Archive is ON for this product.
   ________________________________________________________________________
   Product name:  "IBM OS/2 Base Device Drivers"
   Standard Edition  3.02
   Fixpak name:   XR_D002_   (Country = Generic)
   Pre-requisite CSD Level:  XRJ3006_
   System Id:  1000
   Component Id:  5639A5500
   Archive is ON for this product.
   ________________________________________________________________________
   Product name:  "IBM OS/2 Base Device Drivers"
   Standard Edition  4.00
   Fixpak name:   XR_D002_   (Country = Generic)
   Pre-requisite CSD Level:  XRJ4000_
   System Id:  1000
   Component Id:  5639A6100
   Archive is ON for this product.
   ________________________________________________________________________
   Product name:  "IBM OS/2 Base Device Drivers"
   Standard Edition  4.01
   Fixpak name:   XR_D002_   (Country = Generic)
   Pre-requisite CSD Level:  XRJ4010_
   System Id:  1000
   Component Id:  5639A6100
   Archive is ON for this product.
   ________________________________________________________________________
   Product name:  "IBM OS/2 Base Device Drivers"
   Standard Edition  4.01
   Fixpak name:   XR_D002_   (Country = Generic)
   Pre-requisite CSD Level:  XRJ4010_
   System Id:  1000
   Component Id:  5639A6120
   Archive is ON for this product.
   ________________________________________________________________________
   Product name:  "IBM OS/2 Base Device Drivers"

   
                       FixPak Corrective Service levels and disk layouts  24


                   September 21, 2000 - Warp 3 FixPak XR_D002

   Standard Edition  4.50
   Fixpak name:   XR_D002_   (Country = Generic)
   Pre-requisite CSD Level:  XRJ4500_
   System Id:  1000
   Component Id:  5639A6150
   Archive is ON for this product.
   ________________________________________________________________________
   Product name:  "IBM OS/2 Base Device Drivers"
   Standard Edition  4.50
   Fixpak name:   XR_D002_   (Country = Generic)
   Pre-requisite CSD Level:  XRJ4500_
   System Id:  1000
   Component Id:  5639A5550
   Archive is ON for this product.
   ________________________________________________________________________

   Default directories:

           ..\..\..\..\..\IBMLAN\RPL\BB10.JP\OS2
           ..\..\..\..\..\IBMLAN\RPL\BB20.JP\OS2

   Files contained in Fixpak for product:

   Filename      Name on CSD   Disk#  Date        Time   Size     Checksum
   ------------  ------------  -----  ----------  -----  -------  --------
   106BASE.SYS   106BASE.SY_     2    12/04/1999  03:17    30765  8914525B
   AXBASE.SYS    AXBASE.SY_      2    12/04/1999  03:18    28205  6F2AA485
   POINVGA2.SYS  POINVGA2.SY_    2    05/23/2000  09:40     3814  19818238
   USBASE.SYS    USBASE.SY_      2    12/04/1999  03:14    31517  3ED81A5D
   VKBD106.SYS   VKBD106.SY_     2    12/07/1999  11:02    54334  F261C971
   VKBDUS.SYS    VKBDUS.SY_      2    12/07/1999  11:02    54523  3F9865B1





















   
                       FixPak Corrective Service levels and disk layouts  25


                   September 21, 2000 - Warp 3 FixPak XR_D002

   11.0 SPACE UTILIZATION


   The FixPak installation process requires free space on the following drives:

   Space needed
                  Drive

   Up to 2MB
                  C:

   Up to 2MB
                  Boot drive (4MB if boot is C:)

   Up to 22MB
                  Drive with most free space, holds deferred files if A:SERVICE method
                  used.

   Up to 4MB
                  FixPak Archive/Backup for product with CSD level of XR_3005

   Up to 4MB
                  FixPak Archive/Backup for product with CSD level of XR_3006

   Up to 4MB
                  FixPak Archive/Backup for product with CSD level of XR_4000

   Up to 4MB
                  FixPak Archive/Backup for product with CSD level of XR_4010

   Up to 4MB
                  FixPak Archive/Backup for product with CSD level of XR_4500

   Note: The lines labeled "FixPak Archive/Backup for product with CSD level of"
   will be on the drive you specify and will occupy up to the size indicated for
   the Archive and for the Backup directories. If, for example, the indicated
   size is 30MB then the space actually occupied on the drive can be up to 60MB.















   
                                                       Space Utilization  26


                   September 21, 2000 - Warp 3 FixPak XR_D002

   12.0 RECOVERING FIXPAK ARCHIVE AND BACKUP SPACE

   Warning: Make sure you read and understand the following before
   removing the Archive and Backup files and directories.


   You can recover the space used for FixPak Archive and Backup files as
   long as you understand that doing this prevents you from being able to
   backout to the previous Backup or Archive level. If it becomes
   necessary at a later time to backout a FixPak, the only way you can do
   this is to reinstall Warp.


   Do the following to delete the FixPak Backup and Archive files and
   remove the files used by CSF to keep track of what service has been
   applied to your system.

   1.  Delete every instance of the following files on your system
       (search every drive and every directory they contain).
       þ   LOGF0000.*   (can be OS2 or MPM)
       þ   LOGSTART.*   (can be OS2 or MPM)
       þ   LOGARCH.*    (can be OS2 or MPM)
       þ   CSF_*.*
       þ   FIXSTART
   2.  Delete the files in the FixPak Archive and Backup directories on
       your harddisk.
   3.  Remove the FixPak Archive and Backup directories with the RMDIR
       command.
























   
                              Recovering FixPak ARCHIVE and BACKUP space  27
