| Search | in

Support
Quick Path
| Support Home
| Login | Profile | My Page | Help
| TP General - OS/2 Warp 4 updated installation diskettes
TP General - OS/2 Warp 4 updated installation diskettes
To receive automatic notification of driver updates click 'Profile' above.
Applicable Countries
World-Wide
Description
These update diskettes replace the "Install Disk 1" and "Install Disk 2" that comes with the OS/2 Warp version 4 Package, and are to be used only during the installation process. These diskettes are not to be used to update the installed OS/2 Warp version 4 components already on your system. This release supports the systems: - ThinkPad 380XD, 385XD, 380Z - ThinkPad 390, 390E, 390X - ThinkPad i Series 1720, i Series 1721 - ThinkPad 560X, 560Z - ThinkPad 600, 600E, 600X - ThinkPad 770, 770E, 770ED, 770X, 770Z To determine if you have to use the OS/2 Warp Version 4 Install Disk 1 Update and Install Disk 2 Update or not, refer to the "Summary of Changes" section.
Supported Machines
All
File Details
Version | n/a
Release Date | 2000-01-27
File link |  | File size |  | File description
warp4iu.txt |  | 5,082 |  | README file for the OS/2 Warp Version 4 Install Update Diskettes (v1.04)
warp4iu1.exe |  | 929,213 |  | OS/2 Warp Version 4 Install Update Disk 1 (v1.04) [DSKEXE]
warp4iu2.exe |  | 1,055,338 |  | OS/2 Warp Version 4 Install Update Disk 2 (v1.00) [DSKEXE]
Additional Information
Click here for instructions and limitations on downloading and creating the diskette . This Additional Information field contains the following sections: I. What these diskettes do II. Summary of changes III. Installation instructions for OS/2 Warp version 4 IV. Installation instructions for OS/2 Warp version 3 I. What these diskettes do IBM ThinkPad OS/2 Warp Version 4 Install Disk 1 Update: The IBM ThinkPad OS/2 Warp Version 4 Install Disk 1 Update is a replacement of IBM OS/2 Warp Version 4 Install Disk 1. This disk fixes the following problems. - OS/2 Warp Version 4 cannot be installed on hard disks that have over 4.3GB capacity. - When ThinkPad 600, 600E, 770, 770E, 770ED, 770X, or 770Z is docked to SelectaDock III and an IDE device in SelectaDock III is assigned to secondary IDE channel, the IDE device is not recognized. - When ThinkPad 600, 600E, 770, 770E, 770ED, 770X, or 770Z is docked to SelectaDock I/II, the system with OS/2 Warp Version 4 installed stops in the middle of its start up. - OS/2 Warp Version 4 cannot be installed on hard disks that have over 8.4GB capacity. - When a certain type of DVD-ROM drive is installed, OS/2 Warp 4 takes very long time to boot. IBM ThinkPad OS/2 Warp Version 4 Install Disk 2 Update: The IBM ThinkPad OS/2 Warp Version 4 Install Disk 2 Update is a replacement of IBM OS/2 Warp Version 4 Install Disk 2. This disk fixes the following problem. - OS/2 Warp V4 installation intermittently fails due to MOUSE$ error. II. Summary of changes OS/2 Warp Version 4 Install Disk 1 Update version 1.00 -(New) COPYFROMFLOPPY=1 added in CONFIG.SYS. - (Fix)IBM1S506.ADD updated. OS/2 Warp Version 4 Install Disk 1 Update version 1.01 -(Fix) IBM1S506.ADD updated. OS/2 Warp Version 4 Install Disk 1 Update version 1.02 -(Fix) IBM1S506.ADD, IBMIDECD.FLT, OS2DASD.DMD updated OS/2 Warp Version 4 Install Disk 1 Update version 1.04 -(Fix) IBM1S506.ADD, IBMIDECD.FLT, OS2DASD.DMD updated OS/2 Warp Version 4 Install Disk 2 Update version 1.00 -(New) DOSCALL1.DLL updated. III. Installation instructions for OS/2 Warp version 4 OS/2 Warp Version 4 comes with three diskettes for installation. These update disks are replacements for "Disk 1" and "Disk 2". Install OS/2 Warp Version 4 from the original Install Disk. When you are prompted to insert Disk 1, use 'Install Disk1 Update'. When you are prompted to insert Disk 2, use 'Install Disk2 Update'. Continue installing OS/2 Warp Version 4. IV. Installation instructions for OS/2 Warp version 3 The information is available from the following web site: http://service.software.ibm.com/os2ddpak/index.htm When the home page appears, do the following. (The procedure is subject to change without prior notice) Click on "Yes, I agree. Show the Device Category List..." Click on "OS/2 Component Updates". Click on "Installation Diskette Update". Click on "Greater Than 8.4GB IDE Hardfile Support". Follow the instructions
Year 2000 Information
Document ID: YAST-3MARH8
Last Modified: 2000-02-01
Copyright © 2000 IBM Corporation
Worldwide Support
Privacy | Legal | Contact