| Home | Products & services | Support & downloads | My account

Select a language
PC support home
Warranty lookup
| Related links:
|  | Survey
|  | Support phone list
|  | Business Partner support
|  | IBM PC Institute
|  | IBM Publications Center
|  | Find a Business Partner
PC support home | Login | Profile | My page | Ask an expert | Help
TP General - OS/2 Warp 4 updated installation diskettes
To receive automatic notification of driver updates click Profile above.
Applicable countries/regions
Worldwide
Description
These update diskettes replace the "Install Disk 1" and "Install Disk 2" that comes with the OS/2 Warp version 4 Package, and are to be used only during the installation process. These diskettes are not to be used to update the installed OS/2 Warp version 4 components already on your system. This release supports the systems: - ThinkPad 380XD, 385XD, 380Z - ThinkPad 390, 390E, 390X - ThinkPad i Series 1720, i Series 1721 - ThinkPad 560X, 560Z - ThinkPad 600, 600E, 600X - ThinkPad 770, 770E, 770ED, 770X, 770Z - ThinkPad T20, T21, T22, T23 To determine if you have to use the OS/2 Warp Version 4 Install Disk 1 Update and Install Disk 2 Update or not, refer to the "Summary of Changes" section.
Supported machines
ThinkPad 380XD(ALL), ThinkPad 380Z(ALL), ThinkPad 385XD(ALL), ThinkPad 390(ALL), ThinkPad 390E(ALL), ThinkPad 390X(ALL), ThinkPad 560X(ALL), ThinkPad 560Z(ALL), ThinkPad 600(ALL), ThinkPad 600E(ALL), ThinkPad 600X(ALL), ThinkPad 770(ALL), ThinkPad 770E/ED(ALL), ThinkPad 770X(ALL), ThinkPad 770Z(ALL), ThinkPad T20(ALL), ThinkPad T21(ALL), ThinkPad T22(ALL), ThinkPad i Series 172x(ALL)
File details
Version | See File Descriptions
Release Date | 2001/08/04
File link |  | File size |  | File description
warp4iu.txt |  | 11,057 |  | README for OS/2 Warp Version 4 Install Update Disk 1 version 1.06 and for OS/2 Warp Version 4 Install Update Disk 2 version 1.02
warp4iu1.EXE |  | 930,265 |  | version 1.06 - OS/2 Warp Version 4 Install Update Disk 1 [DSKEXE]
warp4iu2.EXE |  | 1,055,396 |  | version 1.02 - OS/2 Warp Version 4 Install Update Disk 2 [DSKEXE]
Additional information
Click here for instructions and limitations on downloading and creating the diskette. This Additional Information field contains the following sections: I. What these diskettes do II. Summary of changes III. Installation instructions for OS/2 Warp version 4 IV. Installation instructions for OS/2 Warp version 4.51 V. Installation instructions for OS/2 Warp version 3 I. What these diskettes do IBM ThinkPad OS/2 Warp Version 4 Install Disk 1 Update: The IBM ThinkPad OS/2 Warp Version 4 Install Disk 1 Update is a replacement of IBM OS/2 Warp Version 4 Install Disk 1. This disk fixes the following problems: When ThinkPad 600, 600E, 600X, 770, 770E, 770ED, 770X, or 770Z is docked to SelectaDock III and an IDE device in SelectaDock III is assigned to secondary IDE channel, the IDE device is not recognized. When ThinkPad 600, 600E, 600X, 770, 770E, 770ED, 770X, or 770Z is docked to SelectaDock I/II, the system with OS/2 Warp Version 4 installed stops in the middle of its start up. OS/2 Warp Version 4 cannot be installed on hard disks that have over 8.4GB capacity. When a certain type of DVD-ROM drive is installed, OS/2 Warp 4 takes a long time to boot. When OS/2 Warp 4 is installed in a HPFS partition on ThinkPad T20, T21, or T22, Trap D may occur. OS/2 Warp Version 4 cannot be installed on hard disks that have over 30GB capacity. When VGA or VGA GRADD device driver is selected and installed on IBM ThinkPad T21 SXGA+ (1400 x 1050) resolution model or T22 SXGA+ resolution model, opening DOS fullscreen command prompt or OS/2 fullscreen command prompt gets screen blank. If an external monitor is connected, it displays an image correctly. IBM ThinkPad OS/2 Warp Version 4 Install Disk 2 Update: The IBM ThinkPad OS/2 Warp Version 4 Install Disk 2 Update is a replacement of IBM OS/2 Warp Version 4 Install Disk 2. This disk fixes the following problem. OS/2 Warp V4 installation intermittently fails due to MOUSE$ error. When OS/2 Warp 4 is installed in a HPFS partition on ThinkPad T20, T21, T22, Trap D may occur. When VGA or VGA GRADD device driver is selected and installed on IBM ThinkPad T21 SXGA+ (1400 x 1050) resolution model or T22 SXGA+ resolution model, opening DOS fullscreen command prompt or OS/2 fullscreen command prompt gets screen blank. If an external monitor is connected, it displays an image correctly II. Summary of changes OS/2 Warp Version 4 Install Disk 1 Update version 1.00 -(New) COPYFROMFLOPPY=1 added in CONFIG.SYS. - (Fix) IBM1S506.ADD updated. OS/2 Warp Version 4 Install Disk 1 Update version 1.01 -(Fix) IBM1S506.ADD updated. OS/2 Warp Version 4 Install Disk 1 Update version 1.02 -(Fix) IBM1S506.ADD, IBMIDECD.FLT, OS2DASD.DMD updated OS/2 Warp Version 4 Install Disk 1 Update version 1.04 -(Fix) IBM1S506.ADD, IBMIDECD.FLT, OS2DASD.DMD updated OS/2 Warp Version 4 Install Disk 1 Update version 1.05 -(New) IBM1S506.ADD updated -(Fix) SCREEN01.SYS updated OS/2 Warp Version 4 Install Disk 1 Update version 1.06 -(New) IBM1S506.ADD updated -(Fix) IBMIDECD.FLT updated -(Fix) OS2DASD.DMD updated -(Fix) SCREEN01.SYS updated -(New) IBM ThinkPad T23 support OS/2 Warp Version 4 Install Disk 2 Update version 1.00 -(New) DOSCALL1.DLL updated. OS/2 Warp Version 4 Install Disk 2 Update version 1.01 -(Fix) SCREEN01.SYS, SETVGA.CMD updated - (New) FIXVGA.CMD OS/2 Warp Version 4 Install Disk 2 Update version 1.02 -(Fix) SCREEN01.SYS updated -(Fix) FIXVGA.CMD updated -(Fix) FIXVGA added -(Fix) SETVGA.CMD removed III. Installation instructions for OS/2 Warp version 4 OS/2 Warp Version 4 comes with three diskettes for installation. These update disks are replacements for Disk 1 and Disk 2. Install OS/2 Warp Version 4 from the original Install Disk. When you are prompted to insert Disk 1, use Install Disk1 Update. When you are prompted to insert Disk 2, use Install Disk2 Update. Continue installing OS/2 Warp Version 4 until you are prompted to restart your computer for the first time. When you are prompted to restart your computer, do not proceed. Press F3 to go to the command prompt screen. At the command prompt screen, type the following command to run the batch file. The batch file is available on Install Disk2 update. A:\FIXVGA.CMD x: where, x: denotes the boot drive of OS/2 Warp Version 4. In other words, the drive letter to which you are installing OS/2 Warp Version 4. Type EXIT and press the Enter key to go back to the previous screen. Remove the diskette from the floppy drive. Press the Enter key to restart your computer. Continue installing OS/2 Warp Version 4. When you complete the installation, open OS/2 command prompt screen. Insert 'Install Disk2 Update' in the floppy drive. At the command prompt screen, type the following command to run the batch file. A:\FIXVGA.CMD x: where, x: denotes the boot drive of OS/2 Warp Version 4. Remove the diskette from the floppy drive. Type EXIT, then press the Enter key to close the command prompt screen. Properly shutdown OS/2 Warp Version 4, and restart your computer. Proceed to install OS/2 Warp Version 4 FixPack and device drivers. NOTES: When you install any versions of OS/2 Warp Version 4 Base FixPak and OS/2 Warp Base Device Driver FixPak at version XR_D001, you may be prompted whether you want to replace IBM1S506.ADD module or not. Then choose No to not replace IBM1S506.ADD module or your computer will not be able to identify the IDE controller in IBM ThinkPad Dock. If you accidentally choose Yes and the module is replaced, then copy IBM1S506.ADD module from the 'Install Disk1 Update' to \OS2\BOOT directory of your computer after you complete the FixPak installation. It is strongly recommended to run FIXVGA.CMD batch file whenever you change display driver to "VGA" or "VGAGRADD" if your model of IBM ThinkPad computer is IBM ThinkPad T21 SXGA+ (1400 x 1050) resolution model or IBM ThinkPad T22 SXGA+ resolution model. IV. Installation instructions for OS/2 Warp version 4.51 For OS/2 Warp Convenience Package Version 4.51, you do not have to use these diskettes. Instead, OS/2 Warp Convenience Package comes with Installation CD, which has the boot capability. First obtain necessary updates from OS/2 Device Driver Pak On-line web site, install OS/2 Warp Convenience Package, and then install updates obtained from OS/2 Device Driver Pak On-line. The information and updates are available from the following URL: http://service.software.ibm.com/os2ddpak/ http://service5.boulder.ibm.com/2bcprod.nsf Several models of IBM ThinkPad do not support IBM OS/2 Warp Version 4.51 When the home page appears, do the following: (The procedure is subject to change without prior notice) If you already read and agreed to the Program License Agreement, click on I have read the Program License Agreement and AGREE to its terms, and skip to step 6 below. Otherwise, Click on I want to read the Program License Agreement. Read the Program License Agreement. Click on ACCEPT if you agree to its terms and go to the next page. Click on Continue... Click on Systems. Click on IBM Corporation (IBM PC Company - Mobile Systems - ThinkPad). Click on a model name of your IBM ThinkPad computer. Follow the instructions. V. Installation instructions for OS/2 Warp version 3 The information is available from the following web site: http://service.software.ibm.com/os2ddpak/ http://service5.boulder.ibm.com/2bcprod.nsf Several models of IBM ThinkPad do not support IBM OS/2 Warp Version 3 When the home page appears, do the following: (The procedure is subject to change without prior notice) If you already read and agreed to the Program License Agreement, click on I have read the Program License Agreement and AGREE to its terms, and skip to step 6 below. Otherwise, Click on I want to read the Program License Agreement. Read the Program License Agreement. Click on ACCEPT if you agree to its terms and go to the next page. Click on Continue... Click on OS/2 Component Updates. Click on Installation Diskette Updates. Click on PIIX Busmaster / >30GB Drive Support. Follow the instructions.
Document id: YAST-3MARH8
Last modified: 2001-09-19
Copyright © 2001 IBM Corporation

About IBM | Privacy | Legal | Contact