
IBM OS/2 Warp Server and Warp Server SMP FixPak IP08532 US-English

This FixPak can be applied to:

     - IBM OS/2 LAN Server 5.0
     - IBM OS/2 Warp Server
     - IBM OS/2 Warp Server for SMP
     - IBM OS/2 Warp Server with WorkSpace On-Demand Version 1.0
     - IBM OS/2 Warp Server with WorkSpace On-Demand Version 2.0


This FixPak contains fixes for each of the products listed
above and for the following components of these products :
OS/2 LAN Requester, UPM, HPFS, RIPL, Fault Tolerance and
WorkSpace On-Demand servers and clients. After applying this
FixPak, these products will be Year 2000 ready.


WARNING : This FixPak is installed using Corrective Service
          Facility (CSF) 2-B Version 1.41. Once you use this
          version of the FixTool you will not be able to use
          previous versions of the FixTool.

IP08532.INF, located on the first FixPak diskette, contains
installation, and other useful information about this FixPak.
Please review before installation of service.


Diskettes can be created using the LOADDSKF utility.

There are 7 files/images included in this package:
==============================================================
      CSFUS142 DSK   FixPak Tool Diskette 3.50"
      IP08532  1DK   LS DISKETTE #1 3.50 1.44MB
      IP08532  2DK   LS DISKETTE #2 3.50 1.44MB
      IP08532  3DK   LS DISKETTE #3 3.50 1.44MB
      IP08532  4DK   LS DISKETTE #4 3.50 1.44MB
      IP08532  5DK   LS DISKETTE #5 3.50 1.44MB
      IP08532  6DK   LS DISKETTE #6 3.50 1.44MB
