SOFTPAQ NUMBER:  SP5086
PART NUMBER:  N/A
FILE NAME:  N/A
TITLE:  Deskpro 4000 S3 Display Support for OS/2
VERSION:  1.03 Rev A
LANGUAGE:  English

CATEGORY:  Desktops/Driver

PRODUCTS AFFECTED:  Deskpro 4000 Series models with the Compaq S3 ViRGE/GX
		    Graphics Controller, including models: 
                    5166MMX, 5200MMX, 5233MMX

NOTE:  To determine whether your unit has the video controller
       supported by this driver, go to the OS/2 System, click on 
       System Setup and then Selective Install.  Verify adapter 
       is correct next to the Primary Display check box. 
		    
OPERATING SYSTEM:  IBM OS/2

SYSTEM CONFIGURATION:  Compaq S3 ViRGE/GX Graphics Controller

EFFECTIVE DATE:  10 March 1998 

ELECTRONIC DISTRIBUTION ALLOWED:  Yes

SOFTPAQ UTILITY VERSION:  3.1

SUPERSEDES:  SP3838

DESCRIPTION:  This SoftPaq unpacks the files required to install 
the video driver for IBM OS/2 for the Compaq S3 ViRGE/GX 
Graphics Controller used in the above-mentioned Deskpro 4000 models.
Optionally allows a driver diskette to be created.

Enhancements/Fixes:  
 - Corrects system lockup when connecting to either a 5250 or 3270 using 
   Comm Manager.

HOW TO USE:

1. Download the SoftPaq to a temporary, empty directory on your 
hard drive.  The file downloaded is a self-extracting executable 
with a filename based on the SoftPaq Number above.

2. From the download directory, execute the SoftPaq.  When executed 
with no parameters, files are extracted into the current directory. 
To extract the files into a different directory, specify the complete 
path of the directory as a parameter:

     SPxxxx <path> 

Enter "Y" to confirm and files are unpacked into the download 
directory or the directory specified.  

3. After the files have been created, you may delete the  
self-extracting file downloaded in step 1.

4. The driver may be installed directly from the files on the download 
directory or driver diskette can be created. To create a driver diskette,
run MAKEDISK.BAT.

To install the driver, run SETUP.CMD.  From an OS/2 full-screen or OS/2 window 
session, enter:

     <path>\disk01\setup
	where <path> is the drive and directory chosen in step 2

      or 

     A:\setup
	if installing from diskette

Follow on-screen instructions and select VGA mode.

5. When the installation is complete, shut down and restart the computer for 
the changes to take effect.

6. After the driver has been installed, you may delete the files 
from the download directory if you wish.

Copyright 1998, Compaq Computer Corporation.  All rights reserved.

Product names mentioned herein may be trademarks and/or registered
trademarks of their respective companies
