
                   comp.os.os2.marketplace          (Usenet)

                 Saturday, 16-Oct-1999 to Friday, 22-Oct-1999

+----------------------------------------------------------------------------+

From: tulloch@modempool.com                             17-Oct-99 15:32:13
  To: All                                               17-Oct-99 19:56:06
Subj: FA: 3 PS/2 Server 95's

From: Daniel Tulloch <tulloch@modempool.com>

--------------01EB3DF80AD4A27C09CA5321
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

All 3 systems have the following in common:

IBM PS/2 Server 95 Model 9595-1NG
486DX2-66 Intel Processor
95A Planar which has 2 Serial/2 Parallel onboard
IBM SVGA Adapter /A
400W Power Supply
2.88MB FDD
Adaptec AHA-1640 SCSI Adapter

System specifics:

Server 95 #1

IBM 32-bit F/W SCSI-2 Adapter
32MB ECC RAM
IBM 16/4 Token Ring Network Adapter /A
Novell NE2 MCA NIC
IBM 400MB SCSI HDD

Server 95 #2

IBM SCSI Adapter /A
16MB Parity RAM
Quantum Pro-Drive LPS 240MB SCSI-2 HDD

Server 95 #3

IBM 32-bit F/W SCSI-2 Adapter
BusLogic BT-640A 32-bit SCSI-2 Adapter
48MB ECC RAM
IBM 16/4 Token Ring Network Adapter /A
3Com Etherlink/MC TP NIC
IBM DSAS-3540 540MB SCSI-2 HDD
IBM WDS3200 212MB SCSI-2 HDD
Fujitsu M2624FA 520MB SCSI-2 HDD

Box only, No monitor, keyboard, or mouse.
Everything works excellent.
Low-level format and data integrity tests were performed on all DASD.
PC-DOS 7.0 installed.
PS/2 Server95 compatible with DOS, OS/2, Linux, Windows(3.X, 9X, NT)

Info@IBM:  Server95
Questions can be sent to:  tulloch@modempool.com

--------------01EB3DF80AD4A27C09CA5321
Content-Type: text/html; charset=us-ascii
Content-Transfer-Encoding: 7bit

<HTML>
All 3 systems have the following in common:

<P>IBM PS/2 Server 95 Model 9595-1NG
<BR>486DX2-66 Intel Processor
<BR>95A Planar which has 2 Serial/2 Parallel onboard
<BR>IBM SVGA Adapter /A
<BR>400W Power Supply
<BR>2.88MB FDD
<BR>Adaptec AHA-1640 SCSI Adapter
<BR>&nbsp;
<BR>System specifics:

<P><A
HREF="http://cgi.ebay.com/aw-cgi/eBayISAPI.dll?ViewItem&item=183176920">Server
95 #1</A>
<BR>&nbsp;
<BR>IBM 32-bit F/W SCSI-2 Adapter
<BR>32MB ECC RAM
<BR>IBM 16/4 Token Ring Network Adapter /A
<BR>Novell NE2 MCA NIC
<BR>IBM 400MB SCSI HDD
<BR>&nbsp;
<BR><A
HREF="http://cgi.ebay.com/aw-cgi/eBayISAPI.dll?ViewItem&item=183179020">Server
95 #2</A>
<BR>&nbsp;
<BR>IBM SCSI Adapter /A
<BR>16MB Parity RAM
<BR>Quantum Pro-Drive LPS 240MB SCSI-2 HDD
<BR>&nbsp;
<BR><A
HREF="http://cgi.ebay.com/aw-cgi/eBayISAPI.dll?ViewItem&item=183263493">Server
95 #3</A>
<BR>&nbsp;
<BR>IBM 32-bit F/W SCSI-2 Adapter
<BR>BusLogic BT-640A 32-bit SCSI-2 Adapter
<BR>48MB ECC RAM
<BR>IBM 16/4 Token Ring Network Adapter /A
<BR>3Com Etherlink/MC TP NIC
<BR>IBM DSAS-3540 540MB SCSI-2 HDD
<BR>IBM WDS3200 212MB SCSI-2 HDD
<BR>Fujitsu M2624FA 520MB SCSI-2 HDD
<BR>&nbsp;
<BR>Box only, No monitor, keyboard, or mouse.
<BR>Everything works excellent.
<BR>Low-level format and data integrity tests were performed on all DASD.
PC-DOS 7.0 installed.
<BR>PS/2 Server95 compatible with DOS, OS/2, Linux, Windows(3.X, 9X, NT)

<P>Info@IBM:&nbsp; <A
HREF="http://www.can.ibm.com/helpware/9595.html">Server95</A>
<BR>Questions can be sent to:&nbsp; <A
HREF="mailto:tulloch@modempool.com">tulloch@modempool.com</A></HTML>

--------------01EB3DF80AD4A27C09CA5321--

--- WtrGate+ v0.93.p7 sn 165
 * Origin: Usenet: A poorly-installed InterNetNews site (1:109/42)

+----------------------------------------------------------------------------+

From: tulloch@modempool.com                             18-Oct-99 07:46:23
  To: All                                               18-Oct-99 10:22:24
Subj: FA: 3 PS/2 Server 95's

From: Daniel Tulloch <tulloch@modempool.com>

--------------D1CA0317D2B7DB0C773D06C1
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

All 3 systems have the following in common:
********************************************
IBM PS/2 Server 95 Model 9595-1NG
486DX2-66 Intel Processor
95A Planar which has 2 Serial/2 Parallel onboard
IBM SVGA Adapter /A
400W Power Supply
2.88MB FDD
Adaptec AHA-1640 SCSI Adapter
*******************************************

Specific to system:

Server 95 #1

IBM 32-bit F/W SCSI-2 Adapter
32MB ECC RAM
IBM 16/4 Token Ring Network Adapter /A
Novell NE2 MCA NIC
IBM 400MB SCSI HDD

Server 95 #2

IBM SCSI Adapter /A
16MB Parity RAM
Quantum Pro-Drive LPS 240MB SCSI-2 HDD

Server 95 #3

IBM 32-bit F/W SCSI-2 Adapter
BusLogic BT-640A 32-bit SCSI-2 Adapter
48MB ECC RAM
IBM 16/4 Token Ring Network Adapter /A
3Com Etherlink/MC TP NIC
IBM DSAS-3540 540MB SCSI-2 HDD
IBM WDS3200 212MB SCSI-2 HDD
Fujitsu M2624FA 520MB SCSI-2 HDD

Box only, No monitor, keyboard, or mouse.
Everything works excellent.
Low-level format and data integrity tests were performed on all DASD.
PC-DOS 7.0 installed.
PS/2 Server95 compatible with DOS, OS/2, Linux, Windows(3.X, 9X, NT)

Info@IBM:  Server95
Questions can be sent to:  tulloch@modempool.com

--------------D1CA0317D2B7DB0C773D06C1
Content-Type: text/html; charset=us-ascii
Content-Transfer-Encoding: 7bit

<HTML>
All 3 systems have the following in common:
<BR>********************************************
<BR>IBM PS/2 Server 95 Model 9595-1NG
<BR>486DX2-66 Intel Processor
<BR>95A Planar which has 2 Serial/2 Parallel onboard
<BR>IBM SVGA Adapter /A
<BR>400W Power Supply
<BR>2.88MB FDD
<BR>Adaptec AHA-1640 SCSI Adapter
<BR>*******************************************

<P>Specific to system:<A
HREF="http://cgi.ebay.com/aw-cgi/eBayISAPI.dll?ViewItem&item=183176920"></A>

<P><A
HREF="http://cgi.ebay.com/aw-cgi/eBayISAPI.dll?ViewItem&item=183176920">Server
95 #1</A>
<BR>&nbsp;
<BR>IBM 32-bit F/W SCSI-2 Adapter
<BR>32MB ECC RAM
<BR>IBM 16/4 Token Ring Network Adapter /A
<BR>Novell NE2 MCA NIC
<BR>IBM 400MB SCSI HDD
<BR>&nbsp;
<BR><A
HREF="http://cgi.ebay.com/aw-cgi/eBayISAPI.dll?ViewItem&item=183179020">Server
95 #2</A>
<BR>&nbsp;
<BR>IBM SCSI Adapter /A
<BR>16MB Parity RAM
<BR>Quantum Pro-Drive LPS 240MB SCSI-2 HDD
<BR>&nbsp;
<BR><A
HREF="http://cgi.ebay.com/aw-cgi/eBayISAPI.dll?ViewItem&item=183263493">Server
95 #3</A>
<BR>&nbsp;
<BR>IBM 32-bit F/W SCSI-2 Adapter
<BR>BusLogic BT-640A 32-bit SCSI-2 Adapter
<BR>48MB ECC RAM
<BR>IBM 16/4 Token Ring Network Adapter /A
<BR>3Com Etherlink/MC TP NIC
<BR>IBM DSAS-3540 540MB SCSI-2 HDD
<BR>IBM WDS3200 212MB SCSI-2 HDD
<BR>Fujitsu M2624FA 520MB SCSI-2 HDD
<BR>&nbsp;
<BR>Box only, No monitor, keyboard, or mouse.
<BR>Everything works excellent.
<BR>Low-level format and data integrity tests were performed on all DASD.
PC-DOS 7.0 installed.
<BR>PS/2 Server95 compatible with DOS, OS/2, Linux, Windows(3.X, 9X, NT)

<P>Info@IBM:&nbsp; <A
HREF="http://www.can.ibm.com/helpware/9595.html">Server95</A>
<BR>Questions can be sent to:&nbsp; <A
HREF="mailto:tulloch@modempool.com">tulloch@modempool.com</A></HTML>

--------------D1CA0317D2B7DB0C773D06C1--

--- WtrGate+ v0.93.p7 sn 165
 * Origin: Usenet: A poorly-installed InterNetNews site (1:109/42)

+----------------------------------------------------------------------------+

From: letoured@nospam.net                               18-Oct-99 10:16:24
  To: All                                               18-Oct-99 14:36:03
Subj: Re: FA: 3 PS/2 Server 95's

From: letoured@nospam.net

In <380B08A5.F9B747D7@modempool.com>, on 10/18/99 
   at 07:46 AM, Daniel Tulloch <tulloch@modempool.com> said:


Stop spamming us





>All 3 systems have the following in common:
>********************************************
>IBM PS/2 Server 95 Model 9595-1NG
>486DX2-66 Intel Processor
>95A Planar which has 2 Serial/2 Parallel onboard
>IBM SVGA Adapter /A
>400W Power Supply
>2.88MB FDD
>Adaptec AHA-1640 SCSI Adapter
>*******************************************

>Specific to system:

>Server 95 #1

>IBM 32-bit F/W SCSI-2 Adapter
>32MB ECC RAM
>IBM 16/4 Token Ring Network Adapter /A
>Novell NE2 MCA NIC
>IBM 400MB SCSI HDD

>Server 95 #2

>IBM SCSI Adapter /A
>16MB Parity RAM
>Quantum Pro-Drive LPS 240MB SCSI-2 HDD

>Server 95 #3

>IBM 32-bit F/W SCSI-2 Adapter
>BusLogic BT-640A 32-bit SCSI-2 Adapter
>48MB ECC RAM
>IBM 16/4 Token Ring Network Adapter /A
>3Com Etherlink/MC TP NIC
>IBM DSAS-3540 540MB SCSI-2 HDD
>IBM WDS3200 212MB SCSI-2 HDD
>Fujitsu M2624FA 520MB SCSI-2 HDD

>Box only, No monitor, keyboard, or mouse.
>Everything works excellent.
>Low-level format and data integrity tests were performed on all DASD.
>PC-DOS 7.0 installed.
>PS/2 Server95 compatible with DOS, OS/2, Linux, Windows(3.X, 9X, NT)

>Info@IBM:  Server95
>Questions can be sent to:  tulloch@modempool.com

>-<Attachment #1, unnamed (1760 bytes), text/html 7bit>-
_____________
Ed Letourneau <letoured@sover.net>

--- WtrGate+ v0.93.p7 sn 165
 * Origin: Usenet: bCandid - Powering the world's discussions - http
(1:109/42)

+----------------------------------------------------------------------------+

From: tulloch@modempool.com                             20-Oct-99 15:04:17
  To: All                                               20-Oct-99 19:50:28
Subj: FS: Server 95

From: Daniel Tulloch <tulloch@modempool.com>

--------------CB4D53FE03906D60850D1759
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

 Server95@E-bay
IBM PS/2 Server 95 Model 9595-1NG
486DX2-66 Intel Processor
95A Planar which has 2 Serial/2 Parallel onboard
IBM SVGA Adapter /A
400W Power Supply
2.88MB FDD
Adaptec AHA-1640 SCSI Adapter
IBM 32-bit F/W SCSI-2 Adapter
BusLogic BT-640A 32-bit SCSI-2 Adapter
48MB ECC RAM
IBM 16/4 Token Ring Network Adapter /A
3Com Etherlink/MC TP NIC
IBM DSAS-3540 540MB SCSI-2 HDD
IBM WDS3200 212MB SCSI-2 HDD
Fujitsu M2624FA 520MB SCSI-2 HDD

Box only, No monitor, keyboard, or mouse.
Everything works excellent.
Low-level format and data integrity tests were performed on all DASD.
PC-DOS 7.0 installed.
PS/2 Server95 compatible with DOS, OS/2, Linux, Windows(3.X, 9X, NT)

Info@IBM:  Server95
Questions can be sent to:  tulloch@modempool.com

Other  Server95's@Ebay

--------------CB4D53FE03906D60850D1759
Content-Type: text/html; charset=us-ascii
Content-Transfer-Encoding: 7bit

<HTML>


<P>&nbsp;<A
HREF="http://cgi.ebay.com/aw-cgi/eBayISAPI.dll?ViewItem&item=183263493">Server9
5@E-bay</A>
<BR>IBM PS/2 Server 95 Model 9595-1NG
<BR>486DX2-66 Intel Processor
<BR>95A Planar which has 2 Serial/2 Parallel onboard
<BR>IBM SVGA Adapter /A
<BR>400W Power Supply
<BR>2.88MB FDD
<BR>Adaptec AHA-1640 SCSI Adapter
<BR>IBM 32-bit F/W SCSI-2 Adapter
<BR>BusLogic BT-640A 32-bit SCSI-2 Adapter
<BR>48MB ECC RAM
<BR>IBM 16/4 Token Ring Network Adapter /A
<BR>3Com Etherlink/MC TP NIC
<BR>IBM DSAS-3540 540MB SCSI-2 HDD
<BR>IBM WDS3200 212MB SCSI-2 HDD
<BR>Fujitsu M2624FA 520MB SCSI-2 HDD
<BR>&nbsp;
<BR>Box only, No monitor, keyboard, or mouse.
<BR>Everything works excellent.
<BR>Low-level format and data integrity tests were performed on all DASD.
PC-DOS 7.0 installed.
<BR>PS/2 Server95 compatible with DOS, OS/2, Linux, Windows(3.X, 9X, NT)

<P>Info@IBM:&nbsp; <A
HREF="http://www.can.ibm.com/helpware/9595.html">Server95</A>
<BR>Questions can be sent to:&nbsp; <A
HREF="mailto:tulloch@modempool.com">tulloch@modempool.com</A>

<P>Other&nbsp; <A
HREF="http://cgi3.ebay.com/aw-cgi/eBayISAPI.dll?ViewListedItems&userid=tulloch"
>Server95's@Ebay</A></HTML>

--------------CB4D53FE03906D60850D1759--

--- WtrGate+ v0.93.p7 sn 165
 * Origin: Usenet: A poorly-installed InterNetNews site (1:109/42)

+----------------------------------------------------------------------------+

From: vezero@uscom.com                                  20-Oct-99 18:10:27
  To: All                                               20-Oct-99 19:50:28
Subj: How Much?

From: john b <vezero@uscom.com>

--------------DB1F224F3A75D8B4F7727D01
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

Why not tell us how much you want?
john b

Daniel Tulloch wrote:

>
>
>  Server95@E-bay
> IBM PS/2 Server 95 Model 9595-1NG
> 486DX2-66 Intel Processor
> 95A Planar which has 2 Serial/2 Parallel onboard
> IBM SVGA Adapter /A
> 400W Power Supply
> 2.88MB FDD
> Adaptec AHA-1640 SCSI Adapter
> IBM 32-bit F/W SCSI-2 Adapter
> BusLogic BT-640A 32-bit SCSI-2 Adapter
> 48MB ECC RAM
> IBM 16/4 Token Ring Network Adapter /A
> 3Com Etherlink/MC TP NIC
> IBM DSAS-3540 540MB SCSI-2 HDD
> IBM WDS3200 212MB SCSI-2 HDD
> Fujitsu M2624FA 520MB SCSI-2 HDD
>
> Box only, No monitor, keyboard, or mouse.
> Everything works excellent.
> Low-level format and data integrity tests were performed on all DASD.
> PC-DOS 7.0 installed.
> PS/2 Server95 compatible with DOS, OS/2, Linux, Windows(3.X, 9X, NT)
>
> Info@IBM:  Server95
> Questions can be sent to:  tulloch@modempool.com
>
> Other  Server95's@Ebay

--------------DB1F224F3A75D8B4F7727D01
Content-Type: text/html; charset=us-ascii
Content-Transfer-Encoding: 7bit

<!doctype html public "-//w3c//dtd html 4.0 transitional//en">
<html>
Why not tell us how much you want?
<br>john b
<p>Daniel Tulloch wrote:
<blockquote TYPE=CITE>&nbsp;
<p>&nbsp;<a
href="http://cgi.ebay.com/aw-cgi/eBayISAPI.dll?ViewItem&item=183263493">Server9
5@E-bay</a>
<br>IBM PS/2 Server 95 Model 9595-1NG
<br>486DX2-66 Intel Processor
<br>95A Planar which has 2 Serial/2 Parallel onboard
<br>IBM SVGA Adapter /A
<br>400W Power Supply
<br>2.88MB FDD
<br>Adaptec AHA-1640 SCSI Adapter
<br>IBM 32-bit F/W SCSI-2 Adapter
<br>BusLogic BT-640A 32-bit SCSI-2 Adapter
<br>48MB ECC RAM
<br>IBM 16/4 Token Ring Network Adapter /A
<br>3Com Etherlink/MC TP NIC
<br>IBM DSAS-3540 540MB SCSI-2 HDD
<br>IBM WDS3200 212MB SCSI-2 HDD
<br>Fujitsu M2624FA 520MB SCSI-2 HDD
<p>Box only, No monitor, keyboard, or mouse.
<br>Everything works excellent.
<br>Low-level format and data integrity tests were performed on all DASD.
PC-DOS 7.0 installed.
<br>PS/2 Server95 compatible with DOS, OS/2, Linux, Windows(3.X, 9X, NT)
<p>Info@IBM:&nbsp; <a
href="http://www.can.ibm.com/helpware/9595.html">Server95</a>
<br>Questions can be sent to:&nbsp; <a
href="mailto:tulloch@modempool.com">tulloch@modempool.com</a>
<p>Other&nbsp; <a
href="http://cgi3.ebay.com/aw-cgi/eBayISAPI.dll?ViewListedItems&userid=tulloch"
>Server95's@Ebay</a></blockquote>
</html>

--------------DB1F224F3A75D8B4F7727D01--

--- WtrGate+ v0.93.p7 sn 165
 * Origin: Usenet: Verio (1:109/42)

+----------------------------------------------------------------------------+

From: vlabella@comp.uark.edu                            21-Oct-99 11:02:27
  To: All                                               21-Oct-99 16:48:12
Subj: FS: OS/2 Programming books with disks

From: "Vincent P. LaBella" <vlabella@comp.uark.edu>

Look,
	Seven OS/2 programming books are for sale on ebay, all if not most
are out of print!
	Petzold, Schildt etc.

Goto

http://cgi.ebay.com/aw-cgi/eBayISAPI.dll?ViewItem&item=185667527

for more info

=|Vincent P. LaBella vlabella@comp.uark.edu University of Arkansas 
Dept. of Physics   Fayetteville, AR 72701  501-575-4313 FAX:4781|=

--- WtrGate+ v0.93.p7 sn 165
 * Origin: Usenet: The University of Arkansas (1:109/42)

+----------------------------------------------------------------------------+

From: tulloch@modempool.com                             22-Oct-99 19:24:21
  To: All                                               22-Oct-99 21:23:08
Subj: FS: Fully equipped Server95

From: Daniel Tulloch <tulloch@modempool.com>

--------------D2D1119434901E88E624984B
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

 Server95@E-bay
IBM PS/2 Server 95 Model 9595-1NG
486DX2-66 Intel Processor
95A Planar which has 2 Serial/2 Parallel onboard
IBM SVGA Adapter /A
400W Power Supply
2.88MB FDD
Adaptec AHA-1640 SCSI Adapter
IBM 32-bit F/W SCSI-2 Adapter
BusLogic BT-640A 32-bit SCSI-2 Adapter
48MB ECC RAM
IBM 16/4 Token Ring Network Adapter /A
3Com Etherlink/MC TP NIC
IBM DSAS-3540 540MB SCSI-2 HDD
IBM WDS3200 212MB SCSI-2 HDD
Fujitsu M2624FA 520MB SCSI-2 HDD

Box only, No monitor, keyboard, or mouse.
Everything works excellent.
Low-level format and data integrity tests were performed on all DASD.
PC-DOS 7.0 installed.
PS/2 Server95 compatible with DOS, OS/2, Linux, Windows(3.X, 9X, NT)

Other  Server95's@Ebay

Info@IBM:  Server95
Questions can be sent to:  tulloch@modempool.com



--------------D2D1119434901E88E624984B
Content-Type: text/html; charset=us-ascii
Content-Transfer-Encoding: 7bit

<HTML>
&nbsp;<A
HREF="http://cgi.ebay.com/aw-cgi/eBayISAPI.dll?ViewItem&item=183263493">Server9
5@E-bay</A>
<BR>IBM PS/2 Server 95 Model 9595-1NG
<BR>486DX2-66 Intel Processor
<BR>95A Planar which has 2 Serial/2 Parallel onboard
<BR>IBM SVGA Adapter /A
<BR>400W Power Supply
<BR>2.88MB FDD
<BR>Adaptec AHA-1640 SCSI Adapter
<BR>IBM 32-bit F/W SCSI-2 Adapter
<BR>BusLogic BT-640A 32-bit SCSI-2 Adapter
<BR>48MB ECC RAM
<BR>IBM 16/4 Token Ring Network Adapter /A
<BR>3Com Etherlink/MC TP NIC
<BR>IBM DSAS-3540 540MB SCSI-2 HDD
<BR>IBM WDS3200 212MB SCSI-2 HDD
<BR>Fujitsu M2624FA 520MB SCSI-2 HDD
<BR>&nbsp;
<BR>Box only, No monitor, keyboard, or mouse.
<BR>Everything works excellent.
<BR>Low-level format and data integrity tests were performed on all DASD.
PC-DOS 7.0 installed.
<BR>PS/2 Server95 compatible with DOS, OS/2, Linux, Windows(3.X, 9X, NT)

<P>Other&nbsp; <A
HREF="http://cgi3.ebay.com/aw-cgi/eBayISAPI.dll?ViewListedItems&userid=tulloch"
>Server95's@Ebay</A>

<P>Info@IBM:&nbsp; <A
HREF="http://www.can.ibm.com/helpware/9595.html">Server95</A>
<BR>Questions can be sent to:&nbsp; <A
HREF="mailto:tulloch@modempool.com">tulloch@modempool.com</A>
<BR>&nbsp;
<BR>&nbsp;</HTML>

--------------D2D1119434901E88E624984B--

--- WtrGate+ v0.93.p7 sn 165
 * Origin: Usenet: A poorly-installed InterNetNews site (1:109/42)

+----------------------------------------------------------------------------+

+============================================================================+
