   From: "Christian Hennecke" <christian.hennecke@ruhr-uni-bochum.de>
Subject: Possible solution for problems with Crystal sound drivers

Hi all!

I just found a possible solution for the problem with Crystal
Semiconductor sound drivers and sound distortion under Odin.

Increasing the interrupt rate seems to help. To do so do the following:

Mode 2 drivers (1.7x):

Add an /R:x option to the DEVICE=<drive>:\MMOS2\CWAUDIO.SYS line. Valid
values are 1 to 60. I guess the result depends on your machine. Anyway,
60 works for me.

Mode 3 drivers:

Add an /IRQrate:x option. Valid values are 1 to 64.


Christian Hennecke