; OS/2 LAN Requester initialization file |
[networks] net1 = NETBEUI$,0,LM10,34,100,14 net2 = TCPBEUI$,1,LM10,34,100,14 ; This information is read by the redirector at device initialization time. | Hier zijn twee (logische) netwerken net1 (NETBEU) en net2 (TCPBEUI) verbonden met de ethernetkaart.
[requester] ; The following parameters generally do not need to be changed by the user. charcount = 16 chartime = 250 charwait = 3600 keepconn = 600 keepsearch = 600 maxcmds = 16 maxerrorlog = 100 maxthreads = 10 maxwrkcache = 64 numalerts = 12 numcharbuf = 10 numservices = 7 numworkbuf = 40 numdgrambuf = 14 othdomains = printbuftime = 90 sesstimeout = 45 sizcharbuf = 512 sizerror = 1024 sizworkbuf = 4096 ; The wrkheuristics parameter sets a variety of requester fine-tuning options. Brief descriptions are provided here for each digit. More complete descriptions, along with explanations of relationships between digits can be found in the LAN Server Network Administrator Reference Volume 2: Performance Tuning. ; When not otherwise specified, a value of 0 means off (inactive) and 1 means on (active). ; ; 0 opportunistic locking of files (default is 1) ; 1 performance optimization for batch (.CMD) files (default is 1) ; 2 asynchronous unlock and asynchronous write-unlock ; 0 = never 2 = only on a LAN Server virtual circuit ; 1 = always (default) ; 3 asynchronous close and asynchronous write-close ; 0 = never 2 = only on a LAN Server virtual circuit ; 1 = always (default) ; 4 buffer all named pipes and serial devices (default is 1) ; 5 combined read-lock and write-unlock ; 0 = never 2 = only on a LAN Server virtual circuit ; 1 = always (default) ; 6 open and read optimization (default is 1) ; 7 reserved ; 8 use of the chain-send NETBIOS NCB ; 0 = never ; 1 = when a server's buffer is larger than the workstations buffer ; 2 = always (default) ; 9 buffer small read and write requests until the buffer is full ; 0 = never 2 = only on a LAN Server virtual circuit ; 1 = always (default) ; 10 buffer mode ; 0 = always read buffer size amount of data if the request is smaller ; than the buffer size (sizworkbuf) and data is being read ; sequentially ; 1 = use full buffer if file is open for reading and writing ; 2 = use full buffer if reading and writing sequentially ; 3 = buffer all requests smaller than the buffer size (if hits occur) (default) ; 11 RAW read and RAW write SMB protocols (default is 1) ; 12 RAW read-ahead buffer (default is 1) ; 13 RAW write-behind buffer (default is 1) ; 14 read multiplexing SMB protocols (default is 1) ; 15 write multiplexing SMB protocols (default is 1) ; 16 use of big buffers for large core (non-RAW) reads (default is 1) ; 17 same-size read-ahead or read-to-sector boundary (default is 1) ; 18 same-size small record write-behind or write-to-sector boundary (default is 0) ; 19 reserved and must be 0 ; 20 flush pipes and devices on a DosBufReset or DosClose operation ; 0 = Flush only files and devices opened by the caller. Spin until flushed. Wait for confirmation before processing with other tasks. (default) ; 1 = Flush only files and devices opened by the caller. Flush only once. Do not wait for confirmation. ; 2 = Flush all files and all input and output of short-term pipes and devices. Spin until flushed. ; 3 = Flush all files and all input and output of short-term pipes and devices. Flush only once. ; 4 = Flush all files and all input and output of all pipes and devices. Spin until flushed. ; 5 = Flush all files and all input and output of all pipes and devices. Flush only once. ; 21 LAN Server encryption of passwords (default is 1) ; 22 control log entries for multiple occurrences of an error ; 0 = log all occurrences (default) ; 1-9 = limit occurrences that are logged (1-9 define size of table that is used to track errors) ; 23 buffer all files opened with deny-write sharing mode (default is 1) ; 24 buffer all files opened with the read-only attribute set (default is 1) ; 25 read ahead when opening for execution (default is 1) ; 26 handle the interrupt (ctrl+c) key ; 0 = allow no interrupts ; 1 = allow interrupts only on long-term operations ; 2 = always allow interrupts (default) ; 27 force correct open mode when creating files on a core server (reserved for DBCS users) (default is 1) ; 28 NETBIOS NoAck mode ; 0 = NoAck is disabled. ; 1 = NoAck is set on send only. (default) ; 2 = NoAck is set on receive only. ; 3 = NoAck is set on send and receive. ; 29 send data along with SMB write-block RAW requests (default is 1) ; 30 send a message to the screen when the requester logs an error ; 0 = never ; 1 = on write-fault errors only (no time out) (default) ; 2 = on write-fault and internal errors only (no time out) ; 3 = on all errors (no time out) ; 4 = reserved ; 5 = on write-fault errors only (time out) ; 6 = on write-fault and internal errors only (time out) ; 7 = on all errors (time out) ; 8 = on all errors (time out) and pop up an error if a session ; to a server is abnormally disconnected ; 9 = on all errors (time out) and generate an INT24 (critical error) to applications running under DOS emulation if a network hard error is encountered ; 31 reserved ; 32 behavior of DosBufReset on a redirected file (not pipes or devices). When the call to the API returns, the data in the buffer has been handled as follows: ; 0 = Changed data in the buffer was sent from the requester to the server. The server has written the data to disk. ; 1 = Changed data in the buffer was sent from the requester to the server. The server has not yet written the data to disk. ; 2 = DosBufReset was ignored. (default) ; 33 time interval for performing logon validation from the domain controller ; 0 = 5 seconds 4 = 60 seconds 8 = 8 minutes ; 1 = 15 seconds (default) 5 = 90 seconds 9 = 15 minutes ; 2 = 30 seconds 6 = 2 minutes ; 3 = 45 seconds 7 = 4 minutes ; 34 date validation ; 0 = PCLP date format (default) ; 1 = MSNET date format ; 2 = assume date is correct ; 35 free disk space reported to DOS and Windows applications ; 0 = return true value (default) ; 1 = return a value less than two gigabytes ; 36 time and date synchronization with the domain controller at logon ; (default is 1) ; 37 type of verification for the LAN Server logon ; 0 = no verification ; 1 = verify against local NET.ACC ; 2 = verify against domain NET.ACC (default) ; 38 display warning messages for the LAN Server logon ; 0 = do not display warning messages ; 1 = display all warning messages (default) ; 2 = do not display LAN Server specific warning messages ; 3 = display all warning messages, including password expiration date ; 39 buffer all files opened in compatibility mode ; 0 = buffer only files opened for read access in compatibility mode ; 1 = buffer all files opened in compatibility mode (default) ; 40 allow a user to logon multiple times in the same domain (default is 1) ; ; The next lines help you to locate bits in the wrkheuristics entry. ; 1 2 3 4 ; 0123456789012345678901234567890123456789012 wrkheuristics = 1111111121311111110001011120111221001111100 wrkservices = PEER,MESSENGER wrknets = net1,net2 Computername = VISSER Domain = THUIS | numworkbuf = 40 othdomains = thuis2, thuis3 ; andere domeinen (dan hier "thuis" opgeven)
[messenger] logfile = messages.log sizmessbuf = 4096 |
[peer] auditing = resource ; The following parameters generally do not need to be changed by the user. NOTE : srvnets= is represented in the server info struct as a 16-bit lan mask. Srvnet names are converted to indexes within [networks] for the named nets. guestacct = guest autodisconnect = -1 maxauditlog = 100 maxchdevjob = 2 maxchdevs = 1 maxconnections = 26 maxlocks = 64 maxopens = 160 maxsearches = 150 maxsessopens = 80 maxsessreqs = 25 maxsessvcs = 1 maxshares = 16 maxusers = 5 numbigbuf = 4 numfiletasks = 1 numreqbuf = 48 sizreqbuf = 4096 srvhidden = yes ; The srvheuristics parameter sets a variety of server fine-tuning options. Brief descriptions are provided here for each digit. More complete descriptions, along with explanations of relationships between digits can be found in the LAN Server Network Administrator Reference Volume 2: Performance Tuning. ; ; When not otherwise specified, a value of 0 means off (inactive) and 1 means on (active). ; ; 0 opportunistic locking of files (default is 1) ; 1 read-ahead when the requester is performing sequential access ; 0 = do not use read-ahead ; 1 = use single read-ahead thread (default) ; 2 = use asynchronous read-ahead thread ; 2 write-behind (default is 1) ; 3 use of the chain-send NETBIOS NCB (default is 1) ; 4 check all incoming SMBs for correct format (default is 0) ; 5 support FCB opens (default is 1) ; 6 set priority of server (default is 4) ; 0-9 = 0 is highest priority, 9 is lowest priority ; 7 automatically allocate additional memory for directory searches ; (default is 1) ; 8 write records to the audit log only when the scavenger wakes up ; (default is 1) ; 9 do full buffering when a file is opened with deny-write sharing mode ; (default is 1) ; 10 set the interval for the scavenger to wake up ; 0 = 5 seconds 4 = 25 seconds 8 = 45 seconds ; 1 = 10 seconds (default) 5 = 30 seconds 9 = 50 seconds ; 2 = 15 seconds 6 = 35 seconds ; 3 = 20 seconds 7 = 40 seconds ; 11 allow compatibility-mode opens of certain types of files by translating them to sharing mode opens with deny-none ; 0 = Always use compatibility-mode opens. ; 1 = Use deny-none sharing mode if read-only access to .EXE or .COM files. ; 2 = Use deny-none sharing mode if read-only access to .EXE or .COM files. Use deny-write sharing mode if read-only access to .BAT files is requested. ; 3 = Use deny-none sharing mode on all compatibility-mode opens. ; (default) ; 12 allow DOS LAN Services workstations to use a second NETBIOS session when sending printer requests (default is 1) ; 13 number of 64KB buffers used for read-ahead ; 0-9 = number of buffers (default is 1) ; 14 convert incoming path specifications into most basic format (default is 0) ; 15 Oplock Timeout and NETBIOS Acknowledgment Timeout (default is 0) ; 0 = 35 second Oplock Timeout; 34 second NETBIOS Acknowledgment Timeout ; 1 = 70 second Oplock Timeout; 69 second NETBIOS Acknowledgment Timeout ; 2 = 140 second Oplock Timeout; 127 second NETBIOS Acknowledgment Timeout ; 3 = 210 second Oplock Timeout; 127 second NETBIOS Acknowledgment Timeout ; 4 = 280 second Oplock Timeout; 127 second NETBIOS Acknowledgment Timeout ; 5 = 350 second Oplock Timeout; 127 second NETBIOS Acknowledgment Timeout ; 6 = 420 second Oplock Timeout; 127 second NETBIOS Acknowledgment Timeout ; 7 = 490 second Oplock Timeout; 127 second NETBIOS Acknowledgment Timeout ; 8 = 560 second Oplock Timeout; 127 second NETBIOS Acknowledgment Timeout ; 9 = 640 second Oplock Timeout; no NETBIOS Acknowledgment Timeout ; 16 validate IOCTLs (default is 1) ; 17 how long the server maintains unused, dynamic big buffers before freeing the memory. ; 0 = 0 seconds 4 = 5 minutes 8 = 1 hour ; 1 = 1 second 5 = 10 minutes 9 = indefinitely ; 2 = 10 seconds 6 = 20 minutes ; 3 = 1 minute (default) 7 = 40 minutes ; 18 how long the server waits after failing to allocate a big buffer before trying again. ; 0 = 0 seconds 3 = 1 minute (default) ; 1 = 1 second 4 = 5 minutes ; 2 = 10 seconds 5 = 10 minutes ; 19 RAW read and RAW write SMB protocols (default is 1) ; 20 server responds to announcement requests (default is 1) ; ; The next lines help you to locate bits in the srvheuristics entry. ; 1 2 ; 012345678901234567890 srvheuristics = 111101411113110013311 SRVSERVICES = srvnets = NET1,NET2 SRVCOMMENT = eComStation |
[replicator] replicate = IMPORT importpath = H:\ibmlan\repl\import tryuser = yes password = |
[services] ; Correlates name of service to pathname of service program. The pathname must be either 1) an absolute path (including the drive specification) OR 2) a path relative to the IBMLAN root messenger = services\msrvinit.exe peer = services\peerinit.exe replicator = services\replicat.exe requester = services\wksta.exe |