#
#     IBM Touch Device - Calibration Message File.
#
#       Section 1: General Messages used while calibrating.
#
2.00
#
IBM Touch Device Calibration Program
Version
Please wait...
Do NOT touch the screen.
Calculating...
Press the center of the target firmly and accurately.
Bad press - try pressing the center of the target again.
Touch was too hard.
Touch was not held long enough.
Do NOT touch the screen.
Calibration Complete.
Press the spacebar to continue.
****
#
#       Section 2: Yes, No and Quit - message text.
#
Are you satisfied with the accuracy of this calibration?
Type Y to save this calibration data.
Type N to repeat the calibration procedure.
Type Q to quit, without saving or repeating.
To quit, without calibrating, type Q.
****
#
#       Section 3: No, Yes and Quit - keyboard keys to accept.
#
n
y
q
****
#
#       Section 4: Error Messages.
#
Calibration cancelled.
Touch Device Driver is not loaded.
Touch Device command failed.
Internal error - unable to set interrupt vector.
Data file has been corrupted.
Unable to write data file.
Internal error - divide by zero.
Gains out of range.
Calibration Data File not found.
Internal error - insufficient free memory.
Couldn't Save/Restore Device Driver State.
Illegal/missing extension on file.
Illegal Calibration Data file name.
Internal Error - Floating Point.
Bad Device Driver level.
User Abort by Control Break.
Screen not steady after 30 secs, see user guide.
Unable to create thread.
Unable to read Calibration Point file
Calibration Points out of range.
Unable to determine Country dependant information.
Requires US-VGA environment.
****
#
#       Section 5: Prologue Screen Text.
#

  This program allows you to calibrate the IBM Touch Device.

  On the next panel 9 blue targets will appear, one at a time.
  By accurately pressing each target you tell the device the
  exact position of your touch.  Firmly press each target until
  you hear a double tone.  Do not press too hard.  Do not jab the
  screen.

  Make sure you press straight onto the target, not at an angle.
  Remove your hand from the screen between touching targets.
  Do not rest your hand on the screen or the casing.

  When the calibration is completed another set of targets will
  allow you to check the accuracy of your touch.  If you are not
  satisfied you can then repeat the calibration.

  When ready, press the spacebar to start.



  (To quit the program, without calibrating, type Q.)
****
#
#       Section 6: Accuracy Check Screen Text.
#
 You have now calibrated the Touch Device.

 Use these targets to check the accuracy of
 your calibration.  A cross will show where
 your touches are identified.
****
#
#       Section 7: Background Error Screen Text.
#

The Calibration data file could not be found.

It will be necessary to calibrate the Touch Device.

At a command prompt enter the following :

        CD C:\OS2
        <Enter>
        CALIBRAT -u
        <Enter>

****

