8/4/96
Follow the instructions in the README to the letter. It is easy to get a completely
corrupted display setup if you don't. This Build Level seems to fix all display palette
corruption and slow Dos/WinOS2 loading with CL5430 and CL5434 chipsets tested so far,
and probably several others. As always, the oddball CL5429 may not benefit.

Tips: Answer Yes to confirm replacing all newer files with the older ones. If you save
a copy of DSPRES.DLL from Merlin, you can swap it back in later and regain access
to the Warp Sans screen fonts.

I'd be happy to hear any feedback or additional problems on this issue:
Buddy Donnelly
buddyd@ibm.net
