
                  OS/2 Video Device Driver for S3 
             ViRGE,ViRGE/VX,ViRGE/DX,ViRGE/GX,ViRGE/GX2
                      Driver Version 1.03.13
                      Release date: 23 Dec 1997 3:13pm


  QUICK NOTES
  _________________

  o  "S3 DRV1" must be the label on the installation diskette in this
     package.  This label can be applied using the DOS or OS/2 LABEL
     command.  The installation will fail without this step.

  o  You must go back to VGA graphics before installing.  During bootup
     press ALT-F1 once you see the small OS/2 box on the top left hand
     corner.

  o  If you have selected a resolution/refresh rate that is not compatible
     with your monitor, then reboot and press ALT-F1 when the small OS/2
     box appears on the top left hand corner and goto a command prompt.
     Once there, go into your OS/2 directory and delete the VIDEO.CFG file.

  o  If you have the vital data needed regarding your monitor, then you
     can edit the MONITOR.DIF file and edit it to your liking.

  o  Double-Byte Character Support (Japanese, et al.) is available.  Go to
     FTP: ftp.pc.ibm.com  Directory: /pub/pccbbs/pc_servers/
     File: 24l7988.exe
