- All
- Enhanced
- Extended
- Regular
- 12 bits
- 14 bits
- 16 bits
- by RAM size
- by ROM size
- by EEPROM size

- Features
- Configuration Bits
- RAM map
- SFR map

PIC12F529T48A
| Bank 0 |  | Bank 1 |  | Bank 2 |  | Bank 3 |  | Bank 4 |  | Bank 5 |  | Bank 6 |  | Bank 7 |
| SFR 0x000 - 0x006 7 bytes Shared 0x007 - 0x00F 9 bytes GPR 0x010 - 0x01F 16 bytes |  | SFR 0x020 - 0x026 7 bytes Shared 0x027 - 0x02F 9 bytes GPR 0x030 - 0x03F 16 bytes |  | SFR 0x040 Unimplemented 0x041 SFR 0x042 - 0x044 3 bytes GPR 0x045 - 0x046 2 bytes Shared 0x047 - 0x04F 9 bytes GPR 0x050 - 0x05F 16 bytes |  | SFR 0x060 Unimplemented 0x061 SFR 0x062 - 0x064 3 bytes GPR 0x065 - 0x066 2 bytes Shared 0x067 - 0x06F 9 bytes GPR 0x070 - 0x07F 16 bytes |  | SFR 0x080 Unimplemented 0x081 SFR 0x082 - 0x084 3 bytes GPR 0x085 - 0x09F 27 bytes |  | SFR 0x0A0 Unimplemented 0x0A1 SFR 0x0A2 - 0x0A4 3 bytes GPR 0x0A5 - 0x0BF 27 bytes |  | SFR 0x0C0 Unimplemented 0x0C1 SFR 0x0C2 - 0x0C4 3 bytes GPR 0x0C5 - 0x0DF 27 bytes |  | SFR 0x0E0 Unimplemented 0x0E1 SFR 0x0E2 - 0x0E4 3 bytes GPR 0x0E5 - 0x0FF 27 bytes |
It is possible that this colums is inaccurate due to the mirror-SFRs.

| SFR 7 bytes GPR 16 bytes Shared 9 bytes Unimplemented 0 bytes |  | SFR 7 bytes GPR 16 bytes Shared 9 bytes Unimplemented 0 bytes |  | SFR 4 bytes GPR 18 bytes Shared 9 bytes Unimplemented 1 bytes |  | SFR 4 bytes GPR 18 bytes Shared 9 bytes Unimplemented 1 bytes |  | SFR 4 bytes GPR 27 bytes Shared 0 bytes Unimplemented 1 bytes |  | SFR 4 bytes GPR 27 bytes Shared 0 bytes Unimplemented 1 bytes |  | SFR 4 bytes GPR 27 bytes Shared 0 bytes Unimplemented 1 bytes |  | SFR 4 bytes GPR 27 bytes Shared 0 bytes Unimplemented 1 bytes |
It is possible that this colums is inaccurate due to the mirror-SFRs.

Special Function Register.

General-purpose RAM.

Shared RAM.

In this place no RAM.

This page generated automatically by the device-help.pl program (2012-12-22 23:50:57 UTC) from the 8bit_device.info file (rev: 1.10) of mpasmx and from the gputils source package (rev: svn 918). The mpasmx is included in the MPLAB X.