Connected: An Internet Encyclopedia
RFC 1157 - 4.1.6.3. The linkDown Trap

Top: Connected: An Internet Encyclopedia
Up: Requests For Comments
Up: RFC 1157
Up: 4. Protocol Specification
Up: 4.1. Elements of Procedure
Up: 4.1.6. The Trap-PDU
Prev: 4.1.6.2. The warmStart Trap
Next: 4.1.6.4. The linkUp Trap

### 4.1.6.3. The linkDown Trap

A linkDown(2) trap signifies that the sending protocol entity recognizes a failure in one of the communication links represented in the agent's configuration.

The Trap-PDU of type linkDown contains as the first element of its variable-bindings, the name and value of the ifIndex instance for the affected interface.

Next: 4.1.6.4. The linkUp Trap

Connected: An Internet Encyclopedia
RFC 1157 - 4.1.6.3. The linkDown Trap