Connected: An Internet Encyclopedia
RFC 791 - IP Header Option: No Operation

Top: Connected: An Internet Encyclopedia
Up: Requests For Comments
Up: RFC 791
Up: 3. SPECIFICATION
Up: RFC 791 - 3.1. Internet Header Format
Prev: RFC 791 - IP Header Option: End of Option List
Next: RFC 791 - IP Header Option: Security

### RFC 791 - IP Header Option: No Operation

            +--------+
            |00000001|
            +--------+
              Type=1

This option may be used between options, for example, to align the beginning of a subsequent option on a 32 bit boundary.

May be copied, introduced, or deleted on fragmentation, or for any other reason.

Next: RFC 791 - IP Header Option: Security

Connected: An Internet Encyclopedia
RFC 791 - IP Header Option: No Operation