Connected: An Internet Encyclopedia
RFC 1902 - 5. Mapping of the MODULE-IDENTITY macro

Top: Connected: An Internet Encyclopedia
Up: Requests For Comments
Up: RFC 1902
Prev: 4. Naming Hierarchy
Next: 5.1. Mapping of the LAST-UPDATED clause

### 5. Mapping of the MODULE-IDENTITY macro

The MODULE-IDENTITY macro is used to provide contact and revision history for each information module. It must appear exactly once in every information module. It should be noted that the expansion of the MODULE-IDENTITY macro is something which conceptually happens during implementation and not during run-time. Note that reference in an IMPORTS clause or in clauses of SNMPv2 macros to an information module is NOT through the use of the 'descriptor' of a MODULE-IDENTITY macro; rather, an information module is referenced through specifying its module name.

5.1. Mapping of the LAST-UPDATED clause
5.2. Mapping of the ORGANIZATION clause
5.3. Mapping of the CONTACT-INFO clause
5.4. Mapping of the DESCRIPTION clause
5.5. Mapping of the REVISION clause

5.5.1. Mapping of the DESCRIPTION sub-clause

5.6. Mapping of the MODULE-IDENTITY value
5.7. Usage Example

Next: 5.1. Mapping of the LAST-UPDATED clause

Connected: An Internet Encyclopedia
RFC 1902 - 5. Mapping of the MODULE-IDENTITY macro