Connected: An Internet Encyclopedia
RFC 1812 - 10.4.2 Configuration Control

Top: Connected: An Internet Encyclopedia
Up: Requests For Comments
Up: RFC 1812
Up: 10. OPERATIONS AND MAINTENANCE
Up: 10.4 Security Considerations
Prev: 10.4.1 Auditing and Audit Trails
Next: 11. REFERENCES

### 10.4.2 Configuration Control

A vendor has a responsibility to use good configuration control practices in the creation of the software/firmware loads for their routers. In particular, if a vendor makes updates and loads available for retrieval over the Internet, the vendor should also provide a way for the customer to confirm the load is a valid one, perhaps by the verification of a checksum over the load.

DISCUSSION

  Many vendors currently provide short notice updates of their software products through the Internet. This a good trend and should be encouraged, but provides a point of vulnerability in the configuration control process.

If a vendor provides the ability for the customer to change the configuration parameters of a router remotely, for example through a Telnet session, the ability to do so SHOULD be configurable and SHOULD default to off. The router SHOULD require valid authentication before permitting remote reconfiguration. This authentication procedure SHOULD NOT transmit the authentication secret over the network. For example, if telnet is implemented, the vendor SHOULD IMPLEMENT Kerberos, S-Key, or a similar authentication procedure.

DISCUSSION

  Allowing your properly identified network operator to twiddle with your routers is necessary; allowing anyone else to do so is foolhardy.

A router MUST NOT have undocumented back door access and master passwords. A vendor MUST ensure any such access added for purposes of debugging or product development are deleted before the product is distributed to its customers.

DISCUSSION

  A vendor has a responsibility to its customers to ensure they are aware of the vulnerabilities present in its code by intention - e.g., in-band access. Trap doors, back doors and master passwords intentional or unintentional can turn a relatively secure router into a major problem on an operational network. The supposed operational benefits are not matched by the potential problems.

Next: 11. REFERENCES

Connected: An Internet Encyclopedia
RFC 1812 - 10.4.2 Configuration Control