Connected: An Internet Encyclopedia
RFC 1058 - 1.1. Limitations of the protocol

Top: Connected: An Internet Encyclopedia
Up: Requests For Comments
Up: RFC 1058
Up: 1. Introduction
Prev: 1. Introduction
Next: 1.2. Organization of this document

### 1.1. Limitations of the protocol

This protocol does not solve every possible routing problem. As mentioned above, it is primary intended for use as an IGP, in reasonably homogeneous networks of moderate size. In addition, the following specific limitations should be mentioned:

- The protocol is limited to networks whose longest path involves 15 hops. The designers believe that the basic protocol design is inappropriate for larger networks. Note that this statement of the limit assumes that a cost of 1 is used for each network. This is the way RIP is normally configured. If the system administrator chooses to use larger costs, the upper bound of 15 can easily become a problem.
- The protocol depends upon "counting to infinity" to resolve certain unusual situations. (This will be explained in the next section.) If the system of networks has several hundred networks, and a routing loop was formed involving all of them, the resolution of the loop would require either much time (if the frequency of routing updates were limited) or bandwidth (if updates were sent whenever changes were detected). Such a loop would consume a large amount of network bandwidth before the loop was corrected. We believe that in realistic cases, this will not be a problem except on slow lines. Even then, the problem will be fairly unusual, since various precautions are taken that should prevent these problems in most cases.
- This protocol uses fixed "metrics" to compare alternative routes. It is not appropriate for situations where routes need to be chosen based on real-time parameters such a measured delay, reliability, or load. The obvious extensions to allow metrics of this type are likely to introduce instabilities of a sort that the protocol is not designed to handle.

Next: 1.2. Organization of this document

Connected: An Internet Encyclopedia
RFC 1058 - 1.1. Limitations of the protocol