Connected: An Internet Encyclopedia
RFC 1157 - 3.2.6.3. Identification of Object Instances

Top: Connected: An Internet Encyclopedia
Up: Requests For Comments
Up: RFC 1157
Up: 3. The SNMP Architecture
Up: 3.2. Elements of the Architecture
Up: 3.2.6. Form and Meaning of References to Managed Objects
Prev: 3.2.6.2. Resolution of References across MIB Versions
Next: 3.2.6.3.1. ifTable Object Type Names

### 3.2.6.3. Identification of Object Instances

The names for all object types in the MIB are defined explicitly either in the Internet-standard MIB or in other documents which conform to the naming conventions of the SMI. The SMI requires that conformant management protocols define mechanisms for identifying individual instances of those object types for a particular network element.

Each instance of any object type defined in the MIB is identified in SNMP operations by a unique name called its "variable name." In general, the name of an SNMP variable is an OBJECT IDENTIFIER of the form x.y, where x is the name of a non-aggregate object type defined in the MIB and y is an OBJECT IDENTIFIER fragment that, in a way specific to the named object type, identifies the desired instance.

This naming strategy admits the fullest exploitation of the semantics of the GetNextRequest-PDU (see Section 4), because it assigns names for related variables so as to be contiguous in the lexicographical ordering of all variable names known in the MIB.

The type-specific naming of object instances is defined below for a number of classes of object types. Instances of an object type to which none of the following naming conventions are applicable are named by OBJECT IDENTIFIERs of the form x.0, where x is the name of said object type in the MIB definition.

For example, suppose one wanted to identify an instance of the variable sysDescr The object class for sysDescr is:

                 iso org dod internet mgmt mib system sysDescr
                  1   3   6     1      2    1    1       1

Hence, the object type, x, would be 1.3.6.1.2.1.1.1 to which is appended an instance sub-identifier of 0. That is, 1.3.6.1.2.1.1.1.0 identifies the one and only instance of sysDescr.

3.2.6.3.1. ifTable Object Type Names
3.2.6.3.2. atTable Object Type Names
3.2.6.3.3. ipAddrTable Object Type Names
3.2.6.3.4. ipRoutingTable Object Type Names
3.2.6.3.5. tcpConnTable Object Type Names
3.2.6.3.6. egpNeighTable Object Type Names

Next: 3.2.6.3.1. ifTable Object Type Names

Connected: An Internet Encyclopedia
RFC 1157 - 3.2.6.3. Identification of Object Instances