Connected: An Internet Encyclopedia
RFC 1902 - 7.1.2. OCTET STRING

Top: Connected: An Internet Encyclopedia
Up: Requests For Comments
Up: RFC 1902
Up: 7. Mapping of the OBJECT-TYPE macro
Up: 7.1. Mapping of the SYNTAX clause
Prev: 7.1.1. Integer32 and INTEGER
Next: 7.1.3. OBJECT IDENTIFIER

### 7.1.2. OCTET STRING

The OCTET STRING type represents arbitrary binary or textual data. Although there is no SMI-specified size limitation for this type, MIB designers should realize that there may be implementation and interoperability limitations for sizes in excess of 255 octets.

Next: 7.1.3. OBJECT IDENTIFIER

Connected: An Internet Encyclopedia
RFC 1902 - 7.1.2. OCTET STRING