Connected: An Internet Encyclopedia
RFC 1447 - 2.7.2. Units of Conformance

Top: Connected: An Internet Encyclopedia
Up: Requests For Comments
Up: RFC 1447
Up: 2. Definitions
Up: 2.7. Conformance Information
Prev: 2.7.1. Compliance Statements
Next: 3. Acknowledgments

### 2.7.2. Units of Conformance

     -- units of conformance

     partyMIBGroup OBJECT-GROUP
         OBJECTS { partyIndex, partyTDomain, partyTAddress,
                   partyMaxMessageSize, partyLocal,
                   partyAuthProtocol, partyAuthClock,
                   partyAuthPrivate, partyAuthPublic,
                   partyAuthLifetime, partyPrivProtocol,
                   partyPrivPrivate, partyPrivPublic,
                   partyStorageType, partyStatus,
                   partyCloneFrom,
                   contextIndex, contextLocal,
                   contextViewIndex, contextLocalEntity,
                   contextLocalTime, contextStorageType,
                   contextStatus, aclTarget, aclSubject,
                   aclPrivileges, aclStorageType, aclStatus,
                   viewMask, viewType, viewStorageType, viewStatus }
         STATUS  current
         DESCRIPTION
                 "The collection of objects allowing the
                 description and configuration of SNMPv2 parties.

                 Note that objects which support proxy
                 relationships are not included in this conformance
                 group."
         ::= { partyMIBGroups 1 }

     END

Next: 3. Acknowledgments

Connected: An Internet Encyclopedia
RFC 1447 - 2.7.2. Units of Conformance