Connected: An Internet Encyclopedia
RFC 1738 - 4. REGISTRATION OF NEW SCHEMES

Top: Connected: An Internet Encyclopedia
Up: Requests For Comments
Up: RFC 1738
Prev: 3.11 PROSPERO
Next: 5. BNF for specific URL schemes

### 4. REGISTRATION OF NEW SCHEMES

A new scheme may be introduced by defining a mapping onto a conforming URL syntax, using a new prefix. URLs for experimental schemes may be used by mutual agreement between parties. Scheme names starting with the characters "x-" are reserved for experimental purposes.

The Internet Assigned Numbers Authority (IANA) will maintain a registry of URL schemes. Any submission of a new URL scheme must include a definition of an algorithm for accessing of resources within that scheme and the syntax for representing such a scheme.

URL schemes must have demonstrable utility and operability. One way to provide such a demonstration is via a gateway which provides objects in the new scheme for clients using an existing protocol. If the new scheme does not locate resources that are data objects, the properties of names in the new space must be clearly defined.

New schemes should try to follow the same syntactic conventions of existing schemes, where appropriate. It is likewise recommended that, where a protocol allows for retrieval by URL, that the client software have provision for being configured to use specific gateway locators for indirect access through new naming schemes.

The following scheme have been proposed at various times, but this document does not define their syntax or use at this time. It is suggested that IANA reserve their scheme names for future definition:

       afs              Andrew File System global file names.
       mid              Message identifiers for electronic mail.
       cid              Content identifiers for MIME body parts.
       nfs              Network File System (NFS) file names.
       tn3270           Interactive 3270 emulation sessions.
       mailserver       Access to data available from mail servers.
       z39.50           Access to ANSI Z39.50 services.

Next: 5. BNF for specific URL schemes

Connected: An Internet Encyclopedia
RFC 1738 - 4. REGISTRATION OF NEW SCHEMES